# Add changes at the top of the list. Keep it in ASCII, and 80-char wide.
# Do not insert empty lines here, update check depends on it.
 - feature: 70_ENIGMA2: add remotecontrolChannel attribute to customize
                        channelUp/channelDown remote control commands
 - feature: 50_MOBILEALERTSGW: attribut allowfrom added
 - new:     71_YAMAHA_MC: initial release
 - bugfix:  22_HOMEMODE: - fix illegal division by zero in HOMEMODE_Luminance
                         - renamed attribute name HomeYahooWeatherDevice to
                           HomeWeatherDevic
                         - changed characteristic AirPressure UUID to name
 - bugfix:  49_SSCam: no snapinfos when snap was done by SVS itself
                      (Forum: #45671.msg914685.html#msg914685), minor fixes
 - feature: 59_Weather: use demo data up to start then apikey equevalent demo
 - feature: 70_ZoneMinder: added attribute 'apiTimeout'
 - changed: 93_DbLog: minor change of Log entry
 - changed: 70_Pushover: attribute 'storage' was renamed to 'storagePath'
                 and is now visible in FHEMWEB
 - changed: 98_weekprofile: use topic name from reading 'active_topic' 
                 if topic name isn't given
 - changed: 98_STOCKQUOTES: moved to contrib since not maintained and broken
                 due to termination of Yahoo Finance API
 - feature: 55_DWD_OpenData:
                 new readings alertExcludeEvents, SunAz, SunEl and SunUp
                 support forecast resolution value 1 hour
 - bugfix:  12_HProtocolGateway: fix checksum
 - bugfix:  73_AutoShuttersControl: fix typo in Event RegEx for Twilight Event
 - bugfix:  73_AutoShuttersControl: fix little winrec bug then state opened
                                    (max winrec sensors)
 - feature: DarkSkyAPI: add demo support for FHEM demo konfiguration
 - bugfix:  88_HMCCU: set/get config bug fixed
 - feature: 49_SSCam: support of genericStrmHtmlTag attr in streaming devices
 - bugfix:  DarkSky/OpenWeatherMap API fix bug with umlauts
 - bugfix:  73_AutoShuttersControl: fix Bug open Window befor IsDay and closed
                                    IsDay
 - changed: 74_Unifi: removed deprecated UnifiSwitch-functions!
 - bugfix:  74_UnififSwitch: fixed poe restart
 - feature: 57_Calendar.pm: new features and attributes
                            german commandref added
 - bugfix:  00_SIGNALduino: Load protocolHash from web if file  is 
                           missing on fs
 - bugfix:  49_SSCam: some warnings, Forum:#97706
 - bugfix:  88_HMCCU: Fixed minor bugs.
 - feature: 00_SIGNALduino:
                 new webmenu "Display protocollist".
                 Serval new protocols added.
                 New Oregon V3 sensors suppored.
                 Firmware for avr boards can be downloaded and flashed. 
                 on demand from gitghub releases.
                 supports dupTimeout on same iodev
    change:  00_SIGNALduino: Attribute hardware does not longer support nano
                            select nano328 instead
  - feature: 14_SD_RSL: Updated implementation for "all" button on devices
  - feature: 14_SD_WS: support sensors E0001PA,S522,TX-EZ6,other
                      reading sendmode humidityTrend, temperatureTrend,       
                      windspeed, batteryState added
                      attr max-deviation-temp and -hum added
  - changed: 14_SD_WS07: attr correction-xxx to offset-xxx renamed!
  - feature: 14_SD_WS07: new negation-batt attribute
                         Temp only sensors supported 
                         support for max deviation attribute
  - changed: 14_SD_WS09: reading batteryState added, commandref extended
  - changed: 14_Hideki: reading batteryState added
  - bugfix:  73_AutoShuttersControl: fix typo in shuttersMode
  - changed: 14_SD_WS_Maverick: rename Readings for Temperatures
                                added state reading
  - bugfix:  41_OREGON: typo battery percent fixed. de_commandref added
  - bugfix   73_AutoShuttersControl: fix bug then create timer, timer set to
                                     1970
  - new:     98_serviced: new modul for linux services (systemd and initd)
  - bugfix:  12_HProtocolGateway: start poll timer
  - bugfix:  73_AutoShuttersControl: fix many bugs, support for max window
             contact sensors, fix set partyMode then Reading and set command
             equivalent
  - bugfix:  70_BOTVAC: solved recursion while looking up hostname of server
  - feature: limit reading/attr name length in featurelevel 6.0+ (Forum #97493)
  - feature: 49_SSCam: send recordings by telegram is integrated as well as 
                       sending snapshots
  - bugfix:  74_XiaomiBTLESens: fix Undefined subroutine
                                &XiaomiBTLESens::makeDeviceName Bug
  - change:  12_HProtocolGateway: moved strapping table csv file to attribute
  - bugfix:  98_WeekdayTimer: restore old Revision; remove Twilight dependency
  - bugfix:  88_HMCCU: Module HttpUtils included
  - changed. 98_WOL: remove dependency on Twilight + German COmmandref
  - bugfix:  98_WeekdayTimer: Label not found for "next E"
  - bugfix:  70_ONKYO_AVR: model Reading not written correctly
  - feature: 93_DbRep: executeBeforeProc / executeAfterProc is now available 
                       for sqlCmd,sumValue, maxValue, minValue, diffValue, 
                       averageValue
  - changed: 98_WeekdayTimer: remove Twilight dependency
  - feature: 74_AMADautomagicflowset: add support for Android 9 Pie
  - feature: 88_HMCCU: New commands and bug fixes
  - changed: 93_DbLog: CommandRef revised
  - feature: 98_HTTPMOD: starting with featurelevel >5.9 enableCookies,
                         enableControlSet, handleRedirects and
                         enforceGoodReadingNames will default to 1
  - feature: 49_SSCam: new streaming device type "lastsnap", minor fixes
  - change:  93_Log2Syslog: version numbering
  - bugfix:  12_HProtocolGateway: PMS-IB checksum calculation corrected
  - change:  12_HProtocolGateway: move sensorSystem attribute to HProtocolTank
  - feature: 98_Verkehrsinfo.pm: add attribut timeout
  - feature: 12_HProtocolGateway: added 843 protocol for PMS-IB P20
  - feature: 12_HProtocolTank: added Product to calculate 15 degrees volume
  - new:     70_ZoneMinder: fetching Event-Details via API after event received
  - new:     71_ZM_Monitor: fetching Event-Details via API after event received
  - bugfix:  49_SSCam: V8.8.1, fix need attr snapGalleryBoost when sending a
                       snapshot by telegram
  - new:     39_gassistant: Google Assistant support
  - bugfix:  70_BOTVAC: vendor name is no longer case sensitive
  - feature: 49_SSCam: V8.8.0, send snapshots integrated by telegram
  - change:  93_DbRep: running though tableCurrentFillup if database is closed
  - new:     70_BOTVAC: initial release
  - feature: 73_AutoShuttersControl: change blocking handle, add privacy drive
  - bugfix:  49_SSCam: refresh snapgallery device if snap was done by itself
  - feature: 49_SSCam: V8.7.0, send recordings by email is possible now
  - bugfix:  10_MYSENSORS_DEVICE: fix enqueing method, Forum:#96518
  - new:     98_inotify: initial release
  - new:     30_tradfri: initial release
  - new:     42_npmjs: Module to update Node.js modules via NPM package manager
  - feature: 98_Hyperion: add set active/inactive
  - bugfix:  22_HOMEMODE: fix zero devider in HOMEMODE_ContactOpenCheck
                          fix trigger alarm only if alarm triggers have changed
  - bugfix:  49_SSCam: fix version numbering
  - bugfix:  93_DbRep: fix version numbering
  - feature: 98_livetracking: added events for OwnTrack zones
  - feature: 93_DbRep: command exportToFile or attribute "expimpfile" accept
                       option "MAXLINES="
  - bugfix:  09_CUL_FHTTK: removed low batt information from state, moved to
                          reading batteryState
  - feature: 59_Weather: add limit forecast, selection between daily and hourly
                         forecast
  - feature: 49_SSCam: V8.6.1, new attribute snapReadingRotate, time format in
                       readings and galleries depends from global language
                       attribute, minor bug fixes
  - feature: 98_freezemon: New freeze statistics
  - bugfix:  14_CUL_TCM97001: Fix uninitialized value warning
  - bugfix:  14_CUL_REDIRECT: Fix uninitialized value warning
  - feature: 93_DbRep: sqlCmd can handle SQL session variables, Forum:#96082
  - bugfix:  98_DOIFtools: remove Log in DOIFtoolsNextTimer
  - bugfix:  93_DbRep: V8.9.10, fix warnings Malformed UTF-8 character during
                       importFromFile, Forum:#96056
  - change:  59_Weather: add Internal MODEL for statistic
  - feature: 70_BRAVIA: new set command openUrl
  - bugfix:  59_Weather: fix change attribut model
  - bugfix:  98_livetracking: fixed initial Life360 data availability
  - feature: 73_PRESENCE: new set command active/inactive to temporarily
                          disable presence checks
  - bugfix:  DarkSkyAPI: fix reading values, add API Version
  - bugfix:  82_LGTV_WebOS: add SkyOnline at set commands
  - feature: 49_SSCam: 8.5.0, SVS device has "snapCams" command to take
                       snapshots of all cameras and optionally send them
                       alltogether by Email
  - change:  59_Weather: Codestyle, add attribut model to API
  - bugfix:  73_AutoShuttersControl: fix drive up then roommate asleep
  - bugfix:  DarkSkyAPI: fix uninitialized value in localtime at line 430
  - bugfix:  89_FULLY: fixed command set url
  - bugfix:  98_livetracking: fixed HTTP return
  - bugfix:  49_SSCam: fix event generation after snapshots created
  - bugfix:  59_Weather: fix reading double value
  - feature: OpenWeatherMapAPI: add snow and rain in forecast
  - new:     98_todoist: initial release
  - change:  49_SSCam: generate event of every LastSnapFilename,LastSnapId,
                       LastSnapTime if snap was called with arguments,
                       Forum:#45671 #msg887484
  - bugfix:  DarkSkyAPI: OpenWeatherMapAPI, Weather - fix bugs, change
             day_of_week formated, delete deprecated readings
  - bugfixe: DarkSkyAPI: fix hourly wind at factor 3.6
  - new:     44_ROLLO: Universal module to precisely control shutters/blinds
             which support only open/close/stop
  - bugfix:  59_Weather: DarkSky and OpenWeatherMapAPI change formated output,
             add hourly support for DarkSky - thanks to Lippie,
             multiple factor to wind speed and many bugfix
  - bugfix:  73_AutoShuttersControl: Fix shutters drive then window open and
                                     shutter in brightness rage.
  - feature: 82_LGTV_WebOS: Support for SkyOnline App
  - bugfix:  59_Weather: fix table bug in commandref
  - bugfix:  59_Weather: fix mor typo in Commandref
  - feature: OpenWeatherMapAPI: DarkSkyAPI: expand error handling
  - bugfix:  59_Weather: fix typo in commandref
  - feature: 39_alexa.pm: added support autostart of alexa-fhem
                          added support for pubic FHEM Connector skill
  - change:  59_Weather completely reworked
  - bugfix:  98_Verkehrsinfo.pm: internalTimer
  - change:  32_withings: improve Aura handling
  - bugfix:  49_SSCam: fix blocking sscam operation if snap was executed with
                       arguments and aatribute snapEmailTxt is not set,
                       (Forum:#45671 #msg885475)
  - feature: 89_FULLY: Non blocking commands, expert mode
  - bugfix:  73_AutoShuttersControl: little fixes in commandref
  - feature: 49_SSCam: trigger several number of snapshots with alternative
                       text and send it alltogether by email
                       (execute "get <device> versionNotes" for informations)
  - bugfix:  98_DOIFtools: fixed line break in DOIFtoolsLog
  - feature: 72_FB_CALLMONITOR: support for contact images and download of
                                all available contact images from FritzBox
                                phonebooks via TR-064 API.
                                (new attributes: contactImageDirectory,
                                contactDefaultImage and contactImageViaTR064)
  - feature: 72_FB_CALLLIST: support for contact images (new attributes
                             contactImageDirectory and contactImageDirectory)
  - change:  70_ONKYO_AVR: clearing screenItemCxxx readings on page update
  - bugfix:  93_DbRep: sort problem in diffValue Forum:#msg882082
  - bugfix:  98_weekprofile: fix f18 style
  - feature: 98_weekprofile: Force to send complete week profile
                             Attr forceCompleteProfile
  - feature: 98_weekprofile: delay between sending profile data to the
                             same type of device. Attr sendDelay
  - bugfix:  88_HMCCU: Bug fixes
  - change:  10_MYSENSORS_DEVICE: make OTA feature available,
                                  change battery name convention,
                                  support MySensors API 2.0 features like
                                  heartbeat and smartSleep
  - bugfix:  49_SSCam: fix problem with some older SMTP SSL module
  - bugfix:  73_AutoShuttersControl: fix typo in commandref
  - change:  49_SSCam: V8.3.1, change usage of older SMTP versions when Email
                       shipping is used
  - feature: 73_AutoShuttersControl: add support blockingAfterManual at
             Brightness, Bugfixes
  - feature: 49_SSCam: integrated Email shipping of snapshots, save recordings
                       locally with get saveRecoring command
  - new:     98_vitoconnect: initial release
  - feature: 14_CUL_TCM97001: Add Ventus W155, bugfixing
  - feature: 89_FULLY: Support for HTTPS added
  - change:  DOIFtools: add DOIF's weekday 9 to next timer
  - feature: 34_ESPEasy: improved deepsleep support
  - feature: 73_AutoShuttersControl: add maxBrightness for morning open
  - feature: 73_AutoShuttersControl: support for shading, fix bugs
  - feature: 37_harmony: use websockets if xmpp is not available
                         fixes issues with firmware 4.15.206
  - bugfix:  97_TrashCal: changed to new format
  - bugfix:  42_AptToDate: fix state reading after getDistribution
  - feature: 49_SSCam: tooltip hints in camera devices, commandref revised
  - feature: 36_WMBUS: new attribute ignoreUnknownDataBlocks
  - feature: 49_SSCam: V8.0.0, new type "hls" of streaming devices, hls
                       playback now available for all common browsers,
                       tooltip hints in streaming devices, minor fixes
  - feature: 30_HUEBridge, 31_HUEDevice: added get startup command
  - change:  55_DWD_OpenData: maintenance release (forum #83097 msg #869647)
  - change:  mqtt2.template: change name convention + cleanup
  - feature: 72_FB_CALLLIST: new readings/events "count-..." implemented to
                             count different call types
  - change:  72_FB_CALLMONITOR: removed klicktel.de for reverse search, as
                                the service is not available anymore
  - bugfix:  49_SSCam: fix in autocreateCams and take snapshot
  - feature: 98_MediaList.pm: new readings: sortby and status for better
                integration in FTUI
  - change:  49_SSCamSTRM: V2.1.0, change get popupStream to set popupStream
  - feature: 49_SSCam: V7.7.0, autocreateCams command added to SVS device,
                       SSCamSTRM devices have get popupStream command, pls.
                       execute "get <SSCam> versionNotes" for further info
  - bugfix:  51_MOBILEALERTS.pm: Offlimit for decodeHumidityDecimal added
  - change:  98_MSwitch.pm, update V2.07
  - change:  20_FRM_IN: only update on change (Forum #81815)
  - bugfix:  73_AutoShuttersControl: fix absent Event and ModeDown absent bug
  - bugfix:  73_AutoShuttersControl: fix gone then absent bug
  - feature: 49_SSCam: V7.6.0, The PTZ panel is completed by "Preset" and
                       "Patrol" dropdown lists (for PTZ cams only)
  - feature: 49_SSCamSTRM: click on content in stream device or snap gallery
                           opens a popup window
  - new:     70_LaMetric2: add official module for LaMetric Smart Clock
  - feature: 73_AutoShuttersControl: change ReadingsVal to ReadingsNum for
                read position Reading, add setDriveReading for wiggle
  - bugfix:  73_AutoShuttersControl: Code clean, fix unwanted rollo rides
  - feature: msgSchema: add support for LaMetric screen messages
  - bugfix:  70_BRAVIA: removed unnecessary internals name, generation, model
  - bugfix:  74_XiaomiBTLESens: fix humidity bug
  - bugfix:  88_HMCCU: Some minor bugs fixed
  - bugfix:  42_XiaomiBTLESens: bugfix humidity reading
  - feature: 42_AptToDate: add new get command getDistribution to fetch
                           distribution info
  - change:  93_DbRep: attribute timeout set for minTimestamp
  - feature: 73_AutoShuttersControl: change hardLockOut mode code
  - bugfix:  73_AutoShuttersControl: bug line 623
  - feature: 73_AutoShuttersControl: add lockOut support at Z-Wave
  - feature: 73_AutoShuttersControl: ASC Attribut support for value zero
                - no creation of the attributes during the first scan or no
                  attention to a drive command
  - bugfix:  73_AutoShuttersControl: fix many bugs, change window event logic
  - change:  93_DbRep: fix warnings and minor changes
  - change:  93_DbLog: V3.13.0, addLog considers DbLogInclude (Forum:#92854),
             new attributes traceFlag, traceLevel (only for support !)
  - feature: attrTemplate set command added
  - bugfix:  73_AutoShuttersControl: fix logical bugs,
             change Antifreeze values
  - change:  DOIFtools: forced change to li-tags in direct help (Forum #93243)
  - feature: 74_AMADautomagicFlowset: new readings for Caller
  - bugfix:  73_AutoShuttersControl: fix multiple NOTIFYDEV entry's then set
                                     scanForShutters
  - feature: 93_DbRep: new command delDoublets, minor fixes
  - change:  49_SSCam: COMPATIBILITY set to 8.2.2, minor fix
  - bugfix:  73_AutoShuttersControl: fix ASC_twilightDevice
  - bugfix:  73_AutoShuttersControl: fix setPosSetCmd Object
  - bugfix:  73_AutoShuttersControl: fix parts of Commandref
  - bugfix:  98_SmarterCoffee: fix Undefined subroutine &SmarterCoffee::fhem
  - feature: 72_TA_CMI_JSON: added Logging Analog/Digital and RAS values.
  - feature: 98_livetracking: added OsmAnd server for Traccar iOS client
  - new:     73_AutoShuttersControl: Module for the automated control of
                                     shutters based on certain properties
  - feature: 93_DbRep: V8.8.0, attribute valueFilter applied to more functions,
                       new attribute 'fastStart'. (see 'get ... versionNotes')
  - feature: 00_10_MQTT2_CLIENT added (Forum #92888)
  - bugfix:  46_Aqicn: fix commandref, change to packages
  - bugfix:  88_HMCCU: fixed set toggle command
  - new:     98_livetracking: added module
  - bugfix:  38_netatmo: changed geocoding to openstreetmap
  - bugfix:  88_HMCCU: support for CCU firmware 3.41.7
  - bugfix:  38_netatmo: fixed ignored values after 'dead' state
  - feature: 72_XiaomiDevice: load_power reading for power plug
  - feature: 34_ESPEasy: added set cmds: active/inactive/reopen, shutdown tcp
               server port if bridge is disabled/inactive, tcp server will be
               started first after FHEM's global event 'INITIALIZED'.
  - new:     72_TA_CMI_JSON: introduced JSON-API integration with CMI devices
  - changed: 49_SSCam: usage of attribute \"livestreamprefix\" changed,
                       minor code changes, SSCamSTRM changed for compatibility
                       and new attributes with direct attribute help
  - feature: 74_Unifi: Added readings for wan_ip and results of speedtest
  - feature: 77_UWZ: new language support, french and hollandisch
  - change:  93_DbRep: V8.6.0, devices and readings can be excluded by
                       EXCLUDE-option in attributes "reading/device",
                       reduceLog use attributes "device/reading" - see
                       commandref for further information
  - change:  73_AMADCommBridge 74_AMADDevice: change commandref, change version
  - feature: 70_ZoneMinder: introduced Attribute usePublicUrlForZmWeb
  - bugfix   98_SmarterCoffee: fix fhem crash bug
  - feature: 88_HMCCU: client device update optimized
  - bugfix:  89_FULLY: fixed version check bug
  - feature: 74_AMADtaskerset: import with share link
  - change:  42_AptToDate: change to package methode
  - bugfix:  74_XiaomiBTLESens: fix humidity code
  - feature: 98_Verkehrsinfo.pm: add attribut disable
  - feature: allowed: multi-allowed changes (Forum #92423)
  - feature: 93_DbRep: V8.4.0, reduceLog from DbLog integrated into DbRep,
                       sqlCmd/dbValue with textField-long as default, both
                       attributes timeOlderThan / timeDiffToNow can be set,
                       get versionNotes changed to support en/de, new attribute
                       "countEntriesDetail", countEntries separate count of
                       every reading if attribute "countEntriesDetail" is set
  - change:  49_SSCam: COMPATIBILITY changed to 8.2.1
  - bugfix:  74_XiaomiBTLESens : fix warning Illegal hexadecimal digit
                                 ignored
  - bugfix:  93_DbLog: timer not deleted if reopen after reopen xxx executed
             (forum.fhem.de/index.php/topic,91869.msg848433.html#msg848433)
  - feature: 70_ZoneMinder: added attribute loginInterval and setter for login
  - bugfix:  38_netatmo: changed connection check mechanism
  - new:     98_SmarterCoffee: new modul for SmarterCoffee devices
  - bugfix:  74_XiaomiBTLESens: fix humidity bug
  - feature: 49_SSCam: direct help for attributes, new get versionNotes command
  - change:  ROOMMATE, GUEST: Support for updated GEOFANCY version
  - feature: 98_GEOFANCY: add new reading LocTravDist; add support for
                Geofency.app webhook attributes radius, currentLatitude,
                currentLongitude, motion, wifiSSID and wifiBSSID.
                New readings: PosBSSID, PosLat, PosDistHome, PosDistLoc,
                PosLong, PosMotion, PosSSID, PosTravDist
  - bugfix:  98_GEOFANCY: fixed last* readings
  - feature: 89_FULLY: New commands for sound playback and photo.
  - bugfix:  74_XiaomiBTLESens: fix disableForTimer Problem after reboot
  - feature: 31_HUEDevice: added water reading for Xiaomi Aqara Water sensor
  - bugfix:  73_GardenaSmartBridge/Device
                fix Undefined subroutine &GardenaSmartDevice
  - change:  93_DbLog: Log output of recuceLogNbl & use of charFilter enhanced
  - feature: 93_Log2Syslog: attribute sslCertPrefix added (Forum:#92030)
  - bugfix:  10_IT fix usage with multible io devices
  - bugfix:  73_GardenaSmartBridge/Device fix typo oK to ok, change to
                package System
  - change:  93_DbRep: V8.2.3, check availability of DbLog-device at
                       definition time of DbRep-device
  - change:  93_Log2Syslog: send BSD-format changed, commandref revised
  - bugfix:  93_DbRep: fix don't get the real min timestamp in special cases
  - bugfix:  51_MOBILEALERTS: Fix temperature for MA10320PRO
  - change:  93_DbLog, 93_DbRep: minor fix time until DB is closed
  - change:  38_netatmo: changed weathermap calls to new endpoints
  - feature: 5.9 released

- 2018-10-07 (5.9)
  - change:  93_DbRep: direct help for attributes
  - bugfix:  72_XiaomiDevice: set incorrect fan speed to 0
  - bugfix:  38_netatmo: increased timeouts to counter server issues, logging
  - bugfix:  88_HMCCU: Detection of non standard addresses
  - feature: 93_Log2Syslog: TCP-Server in Collector-mode / SSL-support and a
                            lot more, pls. see new get versionNotes command
                            for further Information
  - feature: 93_DbRep: 8.1.0, new get versionNotes command
  - bugfix:  88_HMCCU: Temporary CCU programs are ignored now.
  - change:  19_Revolt: allow adjustment of energy value, filtering of
             implausible values
  - bugfix:  72_XiaomiDevice: better handling of definition w/ missing token
  - change:  32_withings: add in_bed for sleep trackers, ignore inactive users
  - change:  57_Calendar: new attribute quirks with ignoreDtStamp value.
  - change:  57_Calendar: cutoffOlderThan also removes recurring events when
             the series has ended.
  - change:  55_DWD_OpenData: KML based forecast, readings have changed,
             attr forecastProperties must be updated (forum #83097)
  - bugfix:  12_HProtocolGateway: Filllevel conversion corrected
  - bugfix:  57_Calendar.pm: make ical file work again
  - change:  34_ESPEasy: get/set cmd handling rewritten, more supported ESP
             Easy cmds, user defined cmds/mappings, nfx plugin handling
             changed (Forum #91353)
  - change:  93_DbRep: an invalid timestamp will put into state if found on
                       startup
  - bugfix:  38_netatmo: fixed changed values and deprecated API calls
  - bugfix:  93_DbLog: 3.12.1, crash if SVG called (forum:#91285)
  - change:  32_withings: API endpoint changed back to Withings servers
  - bugfix:  93_DbLog: 3.12.0, SVG-select corrected
             (forum.fhem.de/index.php/topic,65860.msg815640.html#msg815640)
  - bugfix:  88_HMCCU: Fixed device definition bug.
  - bugfix:  88_HMCCU: Fixed shutdown bug.
  - bugfix:  32_withings: API endpoint change to Nokia servers
  - feature: 93_DbRep: V8.0.0, restoreMySQL for clientSide dumps implemented
  - bugfix:  74_XiaomiBTLESens: fix bug in disabledForInterval (Forum #835350)
  - change:  88_HMCCU: New release
  - feature: 93_DbLog: 3.11.0, function reduceLog[Nbl] syntax extended to limit
                               days to reduce (pls. see commandref for details)
  - change:  01_FHEMWEB.pm: change default style to f18
  - change:  01_FHEMWEB.pm: change iconPath: to fhemSVG:openautomation:default
  - bugfix:  72_XiaomiDevice: update vacuum volume readings after set
  - change:  98_DOIFtools: improved direct help contetn
  - change:  38_netatmo: removed rain sum readings
  - feature: 00_MYSENSORS: FOTA (thanks Beta-User), gateway fix (thanks Sidey)
  - new:     12_HProtocolGateway / 12_HProtocolTank
  - bugfix:  72_XiaomiDevice: remove unused battery readings for new fans
  - feature: 49_SSCam: activate/deactivate cam internal PIR-sensor
  - new:     10_MQTT_GENERIC_BRIDGE an MQTT bridge, which simultaneously
             collects data from several FHEM devices and passes
             their readings via MQTT or set readings from
             the incoming MQTT messages or executes them
             as a 'set' command on the configured FHEM device.
  - feature: 72_XiaomiDevice: vacuum events, resume zoned cleanup
  - feature: 51_MOBILEALERTS: Added MA10120PRO
  - feature: 51_MOBILEALERTS: Added TFA30.3060.01.IT
  - change:  89_FULLY: Set start URL and bug fixes
  - bugfix:  49_SSCam: V7.0.1, enable/disable issue
             (forum.fhem.de/index.php/topic,45671.msg830869.html#msg830869)
  - change:  98_DOIFtools: add help labels in commandref for attr, set and get
                add MODEL to statistics report, check DOIF excludes Perl mode
  - new:     98_MSwitch.pm: Multi Switch Modul
  - feature: 93_DbRep: V7.19.0, attribute "valueFilter" to filter datasets in
                                fetchrows
  - feature: 49_SSCam: V7.0.0, compatibility to SVS 8.2.0
  - feature: 93_Log2Syslog: V4.8.5, new Syslog-Server Mode and some other
                            improvements, version is moved from contrib
  - bugfix:  73_GardenaSmartBridge fix get humidity bug, add rename Fn
  - change:  71_YAMAHA_AVR: renamed attributes:
                "request-timeout" => "requestTimeout"
                "volume-smooth-change" => "volumeSmoothChange"
                "volume-smooth-steps" => "volumeSmoothSteps"
             already configured values will be converted by FHEM automatically
  - feature: 71_YAMAHA_AVR: add new set command tunerFrequencyBand to change
             between FM and DAB band on DAB-based models
  - bugfix:  71_YAMAHA_AVR: fix set commands preset/presetUp/presetDown for
             input tuner on DAB based models
  - bugfix:  71_YAMAHA_AVR: fix set commands remoteControl tunerPresetUp,
             tunerPresetDown and tunerFrequency for DAB based models
  - added:   98_systemd_watchdog: tested and moved from contrib
  - bugfix:  36_Vallox: Initialization bug fixed
  - added:   00_MQTT: ability for client notifications: on connect,
                      on disconnect, on timeout
  - fixed:   00_MQTT: failure on handling with mqtt-devices without
                      or with wrong devio attributes
  - change:  maintainer change for 00_MQTT, 10_MQTT_DEVICE, 10_MQTT_BRIDGE
             (eisler => hexenmeister)
  - feature: 36_Vallox: Added DF Method, Added CO2SetPoint Handling, Optimized
  - feature: 59_WUup: added attribute unit_solarradiation
  - bugfix:  38_netatmo: removed heating home/room autocreate
  - feature: 46_SmartPi: exchange commandref, add NotifyFn
  - new:     00_MQTT2_SERVER / 10_MQTT2_DEVICE
  - bugfix:  93_DbRep: fix in fetchrow function (forum:#89886),fix highlighting
  - bugfix:  82_LGTV_WebOS: fix set cmd for AmazonLovefilm
  - feature: 51_MOBILEALERTS: added feature to adjust values in define
  - changed: 09_CUL_FHTTK: adapted battery reading to new common reading
                Forum #87575
  - bugfix:  82_LGTV_WebOS: fix uninitialized value
  - change:  98_dewpoint: adjust log level for FAN/ALARM on/off to 4
  - bugfix:  82_LGTV_WebOS: fix current program list readings
  - change:  74_Unifi: changed readings -UC_newClients and -AP_utilization
  - bugfix:  36_WMBUS: fix decryption for AES CBC mode
  - feature: 42_AptToDate: add dist-upgrade available with Attribut
  - change:  74_XiaomiBTLESens: more debug messages, delete old batteryreadings
  - change:  83_IOhomecontrol, 84_IOhomecontrolDevice: complete rewrite and
             extended features
  - feature: 42_AptToDate: add Attribut upgradeListReading for Reading in JSON
  - change:  98_DOIFtools: added shortcut remove_DOIFtoolsLog to commandref
  - change:  01_FHEMWEB.pm: default plotEmbed to 0 (Forum #82351)
  - feature: 73_GardenaSmartBridge: 74_GeardenaSmartDevice: add support for
                                                            Irrigation Control
  - change:  98_feels_like.pm: Improved algorithms, fix reDEFINE
  - new:     42_AptToDate: Modul to retrieves apt information about Debian
                           update state
  - bugfix:  74_NUKIDevice: fix Perl Warnings
  - feature: 88_HMCCU: Support for channel number in attribute ccuscaleval
  - change:  98_DOIFtools: more precise hint related to DOELSE (Forum #89260)
  - change:  98_feels_like.pm: Improved algorithms
  - change:  98_dewpoint: new attributes absoluteHumidity, vapourPressure
                          attribute absFeuchte is now deprecated,
                          write warning to log
  - bugfix:  41_Oregon: batterypercent typo, Forum #89120
  - feature: 49_SSCam: HTTPS Support, buttons for refresh SSCamSTRM-devices
  - changed: 14_Hideki: standard battery readings
  - changed: 14_SD_WS: standard battery readings
  - changed: 14_SD_WS07: standard battery readings
  - changed: 14_SD_WS09: standard battery readings
  - changed: 41_Oregon: standard battery readings
  - change:  76_SMAInverter: Internal MODEL added
  - feature: 49_SSCam: V5.3.0, new createStreamDev generic, control elements
                       for runView content within fhemweb, some new CamLive-
                       Readings, minor fixes
  - change:  95_Dashboard: V3.10.1, added FW_hideDisplayName, Forum #88727
  - change:  98_feels_like.pm: Improved algorithms
                               New attribute "sensorType"
                               minor bugfixes
  - change:  82_LGTV_WebOS: change part of code
  - bugfix:  49_SSCam: fix state turns to "off" even though cam is disabled
  - bugfix:  38_netatmo: fixed camera recording and notification settings
  - feature: 36_WMBUS: support for WMBUS type C and Kamstrup Multical 21
                       encoding.
                       ATTENTION: decryption has changed, please install
                       the perl modules Crypt::Mode::CBC and
                       Crypt::Mode::CTR if you want to decrypt messages.
                       (sudo cpan -i Crypt::Mode::CBC Crypt::Mode::CTR)
  - change:  93_DbLog: commandref hint for special character usage in passwords
  - change:  74_AMADtasker: AMAD Taskerproject change to new battery states
  - feature: 49_SSCamSTRM: new attr hideDisplayName regarding to Forum #88667
  - bugfix:  49_SSCam: global vars
  - bugfix:  88_HMCCU: fixed rpcServerAddr attribute and update of sysvar dpt
  - change:  49_SSCam: V5.2.0, support longpoll refresh of SSCamSTRM-Devices
                       Design change of SSCamSTRM-Devs due to longpoll support
  - change:  82_LGTV_WebOS: change launchApp Vvalue for AmatonVideo and add
                            set command for AmazonVid
  - change:  74_XXiaomiBTLSens: Thermo/HydroSense new state format, new Reading
                                batteryState and batteryPercent
  - change:  49_SSCamSTRM: new attribute "forcePageRefresh" for better control
                           of page refresh (for e.g. Floorplan,Dashboard)
  - feature: 89_FULLY: Added screen saver commands.
  - feature: 49_SSCam: V5.0.0, HLS Streaming implemented, new Streamingdevice
                       based on module 49_SSCamSTRM, some improvements & fixes
  - feature: 98_Text2Speech: added Duch language for Google TTS
  - feature: 74_UnifiSwitch: initial version
  - feature: 74_Unifi: new child-Module UnifiSwitch
                       new reading UC_newClients for new clients
                       block clients by mac-address
  - change:  98_dewpoint: new attribute legacyStateHandling
  - feature: 93_DbRep: V7.18.0, possible use of y:(\d) in timeDiffToNow,
                       timeOlderThan, delEntries considers executeBeforeDump,
                       executeAfterDump, minor fixes
  - feature: 49_SSCam: PTZ-Panel integrated into created StreamDevice
  - fixed:   74_Unifi: import encode_json for newest libs
  - change:  10_KNX: new major release. See commandref for details. The
                     following attributes are deprecated now: readonly,
                     listenonly, slider and useSetExtensions.
  - change:  36_WMBUS: standard battery readings
  - change:  32_withings/38_netatmo/72_XiaomiDevice: standard battery readings
  - bugfix:  98_dewpoint: Use NOTIFYDEV with framework functions
  - feature: 57_Calendar: new parameter "limit" (forum #87566)
  - bugfix:  55_DWD_OpenData: updateAlertsCache causing "not a HASH reference"
                              error on some platforms (forum #83097)
  - change:  98_dewpoint: Don't manipulate STATE of target device if has
                          stateFormat defined.
  - new:     55_DWD_OpenData: weather and alerts from DWD
  - bugfix:  74_Unifi: Cookies for UnifiController 5.9.4
  - bugfix:  74_GardenaSmartDevice: fix uninitialized value $abilities
  - feature: 72_FB_CALLMONITOR: support for wildcard phonebook entries (numbers
                                with trailing star sign)
  - bugfix:  74_XiaomiBTLSens: bugfix
  - new:     98_feels_like.pm: New module to compute a "feels like" temperature
                               and the cloud coverage from a WH2600 like
                               sensor array
  - change:  52_I2C_HDC1008: improve and restructure I2C error handling
  - bugfix:  57_Calendar: fix count for series with exceptions
  - bugfix:  72_FB_CALLMONITOR: fix control code entries in phonebook and
                                reverse search text file
  - feature: 49_SSCam: V4.1.0, support Audiostream cams, minor internal changes
  - change:  93_Log2Syslog: ssldebug for debugging SSL messages, minor fixes
  - feature: 49_SSCam: V3.10.0, CreateStreamDev added, new lastrec_fw_MJPEG,
                       lastrec_fw_MPEG4/H.264 playback MPEG4/H.264 recordings
  - feature: 93_DbRep: V7.17.3, writeToDB - readingname can be replaced by the
                       value of attribute "readingNameMap"
  - change:  88_xs1Bridge: documentation | xs1 with password
  - bugfix:  36_Vallox: Fixed Multireadings. Added Legacy Mapping.
                        added set commands
  - bugfix:  00_MQTT: topics and payload patch
  - bugfix:  73_GardenaSmartBridge: fix fetch token after rereadcfg
  - feature: 60_allergy: alternative data source for extended 5 day forecast
  - new:     74_HusqvarnaAutomower.pm: New module to control your
             Husqvarna Automower with original Connect Module (SIM)
  - bugfix:  73_GardenaSmartBridge: fix delete password then rereadcfg
  - bugfix:  93_DbRep: 7.17.2, doesn't writeToDB if device name contain "."
  - feature: 93_DbLog: addLog - not available reading can be added as new one
                       (forum:#86966)
  - feature: 02_RSS: label and goto in layout definition (forum #86844)
  - change:  59_Weather: reverted changes in HTML routine (forum #87187)
  - feature: 59_Weather: italian translations and other (forum #87080)
  - feature: 49_SSCam: V3.9.1, PTZ control panel added, please consider
                       attributes "ptzPanel_.*" and command "createPTZcontrol"
  - bugfix:  93_DbRep: V7.17.1, sqlCmd can't use §timestamp_begin§
  - feature: 73_GardenaSmartBridge: add set command deleteAccountPassword
  - change:  88_HMCCU: minor changes
  - feature: 93_DbRep: new function dbValue, DbReadingsVal (blocking)
  - bugfix:  93_DbLog: 3.10.7, create addLog-event if reading was not found
  - bugfix:  73_GardenaSmartBridge: add error trigger for notify sub
  - feature: 98_SVG.pm: horizontalLine* added (Forum #86800)
  - change:  93_DbLog: verbose level in addlog changed if reading not found
  - feature: 59_WUup: added AqPM2.5, AqPM10; fixed documentation
  - bugfix:  73_ElectricityCalculator: missing notifydev implemented
  - bugfix:  73_GasCalculator: missing notifydev implemented
  - bugfix:  73_WaterCalculator: missing notifydev implemented
  - change:  88_xs1Dev: xs1-function to set from FHEM
  - change:  88_xs1Bridge: fix PEARL WARNING
  - change:  10_MYSENSORS_DEVICE: implemented alive check thanks to Beta-User
  - bugfix:  93_DbRep: 7.15.2, Internal MODEL is set, minor fixes
  - change:  93_DbRep: 7.15.1, sqlCmd accept widget textField-long,
                               Internal MODEL is set
  - feature: 72_FB_CALLMONITOR: new attribute "sendKeepAlive" to send cyclic
                                keep-alives when connected FritzBox for example
                                is located behind another NAT router
  - bugfix:  72_FB_CALLMONITOR: fix log message on every reverse search:
                                "unknown reverse search method ,"
  - bugfix:  93_DbLog: V3.10.4, fix addLog if no valueFn is used
  - bugfix:  93_DbLog: V3.10.3, minor fixes in addLog function
  - new:     00_Neuron.pm, 10_NeuronPin.pm: support for Neuron Devices
  - feature: 59_WUup: add attribute round
  - bugfix:  72_FB_CALLMONITOR: fix not working get command
                                showPhonebookEntries for remote phonebooks
  - bugfix:  73_GardenaSmartBridge: add commandref parts
  - change:  93_DbLog: V3.10.2, event parsing of Weather changed, add option
                       CN=<caller name> to addlog-function
  - change:  49_SSCam: V3.8.4, usage of Internal MODEL changed
  - bugfix:  00_SIGNALduino: fixed ws7000 decoding
  - feature: 72_XiaomiDevice: predefined zones and points, carpet mode
  - bugfix:  88_xs1Bridge: blacklist PEARL Warning + Code mod
  - feature: 74_AMADDevice: add support to set and read Adaptive brightness
  - bugfix:  88_xs1Bridge: blacklist option (forum #790923)
  - bugfix:  49_SSCam: V3.8.3, fix of version 3.8.2
  - change:  49_SSCam: V3.8.2, internal codereview, minor fixes
  - feature: 73_GardenaSmartBridge/74_GardenaSmartDevice: rewrite parts of
             Bridge Modul and add Support for predefined start point
  - feature: 49_SSCam: V3.8.0, new setHome command, minor fixes
  - feature: 72_XiaomiDevice: added zone and goto
  - bugfix:  57_Calendar: fix weekly events, get full all, defaultTimeFormat
  - change:  93_DbLog: V3.10.0, addLog considers DbLogExclude in Devices,
                       keyword "!useExcludes" to switch off considering
                       DbLogExclude in addLog, DbLogExclude & DbLogInclude
                       can handle "/" in Readingname, commandref revised
  - bugfix:  00_SIGNALduino: Perl Warnings and FHEM crash fixed
  - added:   88_xs1Bridge: Documentation added
  - added:   88_xs1Dev: various sensor types added
  - feature: 57_Calendar: get ... vevents and much more (forum #86148)
  - feature: 73_AMADCommBridge/74_AMADDevice: add new mediaPlayer Support, add
                                              takeScreenshot function
  - feature: 14_Hideki: changed decrypting and improved crc check
  - change:  14_SD_WS_Maverick: reworked module, renamed readings
                               added commandref
  - bugfix:  14_SD_WS07: Error retrieving rssi value fixed
  - feature: 14_SD_WS07: added correction-temp and correction-hum
                         added two models temp/temp-hum
  - change:  00_SIGNALduino: Protokoll 12.1 with protocol 12 (Hideki)
                            combined and 12.1 removed
  - feature: 49_SSCam: 3.7.0, new delPreset command, minor fixes
  - bugfix:  10_OWServer: avoid init and autocreate on tentative connection
  - feature: 49_SSCam: 3.6.0, new setPreset command, minor changes
  - feature: 72_FB_CALLMONITOR: show a "not found" popup, when reverse search
                                via get command fails
  - feature: 93_DbRep: V7.15.0, new command sqlSpecial
  - bugfix:  74_XiaomiBTLSens: fix commandref entrys
  - feature: 49_SSCam: V3.5.0, new get command listPresets
  - change:  93_DbRep: V7.14.8, exportToFile,importFromFile can use file as an
                       argument, fix no save to database if value=0 (writeToDB)
  - feature: 10_OWServer: added OWNet module version suggestion to define
  - feature: 49_SSCam: V3.4.0, new commands startTracking, stopTracking for
                       PTZ-Cams with object tracking capability
  - added:   74_HOMBOT: add commandref summary, code design
  - change:  73_GardenaSmartBridge: change logging output for username and
                                    password
  - feature: 93_DbRep: 7.14.6, attr expimpfile can use some kinds of wildcards
  - feature: 59_WUup: V0.9.6, calculate solarradiation from lux to W/m²
  - feature: 73_AMADCommBridge: fix Commandref, add allowfrom support
  - bugfix:  74_XiaomiBTLESens: Backslash found where operator expected
  - bugfix:  98_TRAFFIC: v1.3.7, fixed special characters and updateschedule
  - change:  10_OWServer: autoselecting OWNet module
  - bugfix:  72_FB_CALLLIST: allow newlines in mapping attributes values
  - feature: 74_XiaomiBTLESens: add new set command resetBatteryTimestamp
  - bugfix:  93_DbRep: some perl warnings fixed
  - fhem.pl: restoreDir restructured (Forum #85801)
  - added:   88_xs1Bridge: added blacklist function
  - feature: 93_DbLog: V3.9.0, syntax of attribute excludeDevs enhanced
  - update:  39_Talk2Fhem: Timephrases added, bugfixes and some changes
  - bugfix:  74_AMADCommBridge: fix Commandref
  - bugfix:  82_LGTV_WebOS: fix litte typos fix eval bug
  - update:  21_HEOS: fix Use of uninitialized value {repeat}
                      in substitution (s///)
  - change:  88_xs1Bridge: Typ timerswitch added
  - change:  88_xs1Dev: Typ timerswitch added
  - feature: 72_FB_CALLMONITOR: new reverse search provider 11880.com (german)
                                and herold.at (austrian)
  - change:  93_DbRep: V7.14.4, increased timeout of special function
  - feature: 74_Unifi: added set updateClient, encrypt user and password
  - change:  49_TBot_List: deleteonly lists / internal changes
  - change:  50_TelegramBot: more silent cmds, caption formatting,several fixes
  - change:  lib/OWNet.pm: updated to latest version from
             https://sourceforge.net/p/owfs/code/ci/master/tree/module/
             ownet/perl5/OWNet/lib/OWNet.pm
  - feature: 66_ECMD: new attribute stop
  - change:  93_DbLog: V3.8.9, commandref revised
  - feature: fhem.pl: OldReading* added (Forum #85406)
  - feature: 93_DbRep: V7.14.3, minTimestamp - get lowest timestamp in database
  - bugfix:  72_FB_CALLLIST: fix broken german umlaut in timestamps on
                             perl version >= 5.22
  - bugfix:  72_FB_CALLMONITOR: fixing reverse search via dasoertliche.de
  - feature: 39_Talk2Fhem: V0.5 Object radiusing
  - bugfix:  93_DbLog: V3.8.8, no exit if configuration couldn't be read
  - change:  93_DbLog: V3.8.7, no change limits got fron SVG
  - bugfix:  88_xs1Dev: new type shutter integrated (Forum #85137)
  - bugfix:  88_xs1Bridge: actuator functions incorrect (Forum #85137)
  - bugfix:  93_DbRep: fix perl warning
  - bugfix:  38_netatmo: fixed public stations update, added fixed interval
  - bugfix:  93_DbRep: V7.14.1, bugfix for PostgreSQL
  - added:   88_xs1Dev: added new module for control xs1
  - changed: 88_xs1Bridge: changed for another module
  - bugfix:  88_HMCCU: Fixed bug in attribute peer
  - bugfix:  32_withings, 38_netatmo: maintenance update
  - added:   72_XiaomiDevice: added new module for Xiaomi WiFi devices
  - feature: 93_DbRep: V7.14.0, new command syncStandby
  - bugfix:  21_HEOS: decode_json() in a eval, fix play_previous
  - bugfix:  73_NUKIBridge/74_NUKIDevice: decode_json() in a eval
  - Update:  73_AMADCommBridge/74AMADDevice: 4.2 new Version with Tasker Support
  - bugfix:  14_CUL_TCM97001: Fix temperature reading
  - bugfix:  49_SSCam: V3.3.0, code review, API bug fix of runview lastrec,
                       commandref revised (forum:#84953)
  - bugfix:  73_ElectricityCalculator: Spelling error "di(s)abled" corrected
  - bugfix:  73_GasCalculator:         Spelling error "di(s)abled" corrected
  - bugfix:  73_WaterCalculator:       Spelling error "di(s)abled" corrected
  - bugfix:  93_DbRep: V7.13.2, fix of aggregation month
  - feature: 00_MQTT: topic with space or colon
  - bugfix:  98_GOOGLECAST: fix open connections and state value
  - feature: 10_MQTT_DEVICE: add SetExtensions
  - bugfix:  00_MQTT: small bugfix
  - feature: 98_DOIFtools: support for multiple holiday files in holiday2we for
             next timer calculation
  - change:  53_GHoma: plugs with energy measurement implemented
                      reading energy now in kWh / SetExtensions / DbLog_splitFn
  - change:  93_DbRep: commandref revised
  - change:  93_DbLog: V3.8.5, Parse Event for Zwave changed
  - feature: 00_MQTT: new attribute "client-id"
  - feature: 93_DbRep: V7.13.0, changeValue may use perlcode {} as "new string"
  - feature: 93_DbRep: V7.12.0, compression of dumpfile, restore of compressed
                       files possible
  - change:  77_SMAEM: V3.1.0, extend error handling in define
  - bugfix:  73_ElectricityCalculator: Min dt for calc. reduced from 30 to 1 s
  - feature: 93_DbRep: V7.11.0, "repairSQLite" to repair a corrupted SQLite DB
  - bugfix:  88_xs1Bridge: code changeover + safety connection check
  - bugfix:  73_PRESENCE: new collectord .deb package fixing perl warnings
  - bugfix:  88_HMCCU: fixed CUxD bug and minor bugs
  - feature: 93_DbRep: V7.10.0, new "changeValue" command, minor fixes
  - bugfix:  88_xs1Bridge: fix Filelog check
  - new:     39_Talk2Fhem: new module for language control
  - feature: 70_BRAVIA: TV input select for all active tuners
                        Channel selection by channel uri
                        Optimized fetch of app and input presets
  - feature: 98_structure: saveStructState/restoreStructState (Forum #84154)
  - bugfix:  74_XiaomiBTLESens: fix corrupt character for temperature
  - bugfix:  74_XiaomiBTLESens: fix humidity bug than temperature is lower 10
  - feature: 88_xs1Bridge: automatic Logfile after define | feature extension
  - changed: 98_weekprofile: send values for on/off instead of "on"/"off"
  - feature: 93_DbRep: V7.9.0, new attribute "avgTimeWeightMean" (averageValue)
                               some code review and corrections
  - bugfix:  88_xs1Bridge: fix Code
  - bugfix:  74_XiaomiBTLESens: fix many bugs with ssh connection, fix negativ
                                temperature bug
  - feature: 93_DbRep:V7.8.1, new command "eraseReadings", some fixes
  - bugfix:  93_DbLog:V3.8.4, cover userCommands, avoid crash (forum:#83973)
  - feature: 51_MOBILEALERTS: Added directionInt for MA10660
  - changed: 50_MOBILEALERTSGW/51_MOBILEALERTS: Migrate to readingsDelete
  - new:     98_freezemon: initial check-in
  - feature: 74_Unifi: added voucher-functions
  - change: 30_MilightBridge: Use new RemoveInternalTimer function
  - new:     52_I2C_EMC1001.pm: initial check in
  - feature: 30_HUEBridge, 31_HUEDevice: added createGroupReadings attribute
  - feature: f18: implement dragging / dashboard
  - change:  93_DbLog: V3.8.3, configCheck improved, execute cache only every
                       syncInterval/2 if cacheLimit reached, error-handling
                       improved
  - bugfix:  93_DbRep: V7.7.1, minor fix if disabled
  - feature: 93_DbRep: V7.7.0, attribute "averageCalcForm" - select variant of
                       averageValue reporting, calc of daily medium temperature
                       according german weather service
  - bugfix:  88_HMCCU: Fixed missing events after get vars command
                       Fixed state after RPC server start
  - change:  74_Unifi: SSIDs-Readings and drop-downs use goodReadingName()
  - feature: 72_FB_CALLLIST: enhanced possibilities to disable a FB_CALLLIST
                             definition (via attribute "disable")
                             new attribute processEventsWhileDisabled
  - feature: 73_PRESENCE: new presenced deb package (ping command, systemd)
  - feature: 93_DbRep: V7.6.1, data with "|" in value are possible to process,
                       attr "sqlCmdHistoryLength" to use sqlCmdHistory list,
                       attr "fetchMarkDuplicates" to highlight multiple data
  - update:  88_HMCCU: Version 4.2
  - new:     88_HMCCURPCPROC: Sub process based RPC server for HMCCU.
  - feature: 73_PRESENCE: new collectord package (RSSI based room selection
                          for BTLE devices (lepresenced), ping command for
                          daemon monitoring, systemd service unit)
  - bugfix:  93_DbLog: use of uninitialized value $txt if addlog has no value
  - feature: 33_readingsGroup: added german commandref (by HomeAuto_User)
  - feature: 10_pilight_ctrl: support bh1750 illuminance sensor
  - feature: 71_YAMAHA_NP: Added player readings support for
                           airplay and spotify inputs.
  - change:  93_DbLog:V3.8.0, log events containing pipe "|" possible
  - bugfix:  98_TRAFFIC: v1.3.5, fixed return readings in DbLog_SplitFn
  - feature: attr: -a and -r Options added (Forum #83414)
  - feature: 20_FRM_IN: added Firmata 2.5 feature PIN_MODE_PULLUP
                        note: requires perl-firmata 0.64
  - change:  74_Unifi: SSIDs-Readings and drop-downs use goodReadingName()
  - feature: new module 37_NotifyAndroidTV.pm to send notifications
             to Notifications for Android TV/Fire TV apps (justme1968)
  - bugfix:  98_TRAFFIC: v1.3.4, fixed DbLog_SplitFn, misc improvements
  - change:  72_FB_CALLMONITOR: reverse search provider klicktel.de is
                                DEPRECATED and will be removed in a future
                                release. please use dasoertliche.de instead.
                                attribute apiKeyKlicktelDe removed
  - bugfix:  93_DbLog: V3.7.1, fix typo in commandref
  - change:  93_DbRep: V7.5.5, minor corrections in delSeqDoublets
  - change:  72_FB_CALLMONITOR: new attribute apiKeyKlicktelDe and
                                apiKeySearchCh to configure own private API keys
                                for reverse search via klicktel.de or search.ch
  - feature: 93_DbRep: V7.5.4, dumpFilesKeep can be set to "0", new attribute
                       "ftpDumpFilesKeep" for version management on FTP,
                       delSeqDoublets optimized for consumption of resources
  - feature: 98_DOIFtools: blockinginfo added to running timer info
  - change:  73_PRESENCE: following attributes were renamed:
                          * ping_count => pingCount
                          * fritzbox_speed => fritzboxCheckSpeed
                          * bluetooth_hci_device => bluetoothHciDevice
                          existing configuration will be converted automatically
  - bugfix:  74_XiaomiBTLESens: fix error messages
  - feature: 46_TeslaPowerwall2AC: Powerwalls overwiev
  - feature: 73_PRESENCE: new set commands overrideInterval and clearOverride
                          to temporary override the check interval.
                          new attributes retryCount and retryInterval
  - feature: 89_FULLY: Added support for attribute disable
  - change:  93_DbLog: V3.7.0, log verbose 5 enhanced, configuration read check
                       added to configCheck
  - feature: 74_Unifi: new Readings for WLAN-states, fixed Warning
  - feature: 93_DbRep: V7.5.1, new set-options display/writeToDB for
                       (max|min|sum|average|diff)Value,
                       create background_processing_time before execute
                       commands in attribute "executeAfterProc" (db-dumps)
  - feature: 10_FRM: new attribute "disable", new states "disabled",
                     "defined" and "connected", new attribute "errorExclude",
                     new reading "stringMessage", new internal "pullup_pins"
  - bugfix:  74_XiaomiBTLESens: fix Illegal hexadecimal digit ' ' ignored
  - change:  74_XiaomiBTLESens: better timer logic
  - feature: 20_FRM_AD: analog resolution now depending on device capability
  - change:  93_DbLog: V3.6.5, avoid shutdown problem if database is too slow,
                       extend configCheck with shutdown preparation check,
                       fix logentries if device disabled and db not available
  - bugfix:  74_Unifi: fixed blockClient
  - bugfix:  98_dewpoint.pm: Fix event processing when updating STATE
  - bugfix:  73_ElectricityCalculator.pm: Spelling error
  - change:  74_XiaomiBTLESens: Code clean
  - feature: 21_HEOSPlayer: add input URL as set command
  - feature: 74_Unifi: add new set command to en-/disable Site Status-LEDs
  - bugfix:  74_XiaomiBTLESens: fix ssh gatttool which test
  - new:     74_XiaomiBTLESens: modul replace 74_XiaomiFlowerSens, add Support
                                for Xiamomi Themometer/Hygrometer mit Display
  - bugfix:  42_SYSMON: Falsche Angabe von Ram free / used bei Debian Stretch
  - bugfix:  70_BRAVIA: fixed hash for space
                        (application, channel, input names)
  - change:  93_DbLog: change verbose level of addlog from 2 to 4
  - bugfix:  93_DbRep: old dumpfiles not deleted by dumpMySQL clientSide
  - bugfix:  70_BRAVIA: typo fixed, 'set application' works now
  - feature: 93_DbRep: V7.4.0, new commands dumpSQLite/restoreSQLite,
                       execute commands before/after set optimizeTables,
                       vacuum, restoreMySQL, restoreSQLite available,
                       CAUTION !! attributes executeBeforeDump/executeAfterDump
                       are renamed to executeBeforeProc/executeAfterProc
  - feature: 74_Unifi: add new set commands to block/unblock clients,
                       enable/disable WLAN, new client-Reading essid
  - feature: structure: implement dynamic members via devspec (Forum #82604)
  - feature: new module 74_UnifiVideo for UnifiVideo integration (justme1968)
  - change:  93_DbLog: V3.6.2, new attribute "exportCacheAppend", minor fix in
                       Log verbose 5
  - bugfix:  82_LGTV_WebOS: fix wrong paired reading and more
  - change:  98_dewpoint: Use NOTIFYDEV
  - bugfix:  93_DbRep: syntax error if perl version < 5.20
  - feature: 74_AMADDevice: add new set command "takePicture",change Commandref
  - feature: 98_GOOGLECAST: support speak command for TTS
                            set castdevice speak "Hallo"
  - feature: 51_MOBILEALERTS: Added Sensor WL2000
  - change:  93_DbRep: V7.3.0, charfilter avoid control characters in datasets
                       to export, function exportToFile importFromFile improved
  - feature: FHEMWEB: new style f18
  - feature: 98_weekprofile.pm: new set command 'reread_master'
  - change:  10_SOMFY: minor changes remvoe debug and add parsestate reading
  - bugfix:  74_XiaomiFlowerSens: fix error then use ssh and no connect
  - change:  72_FB_CALLIST: mapping tables (icon-mapping, external-mapping,...)
             will be evaluated after initialization is finished (Forum: #81892)
  - feature: 01_FHEMWEB.pm: -> as room separator (Forum #82151)
  - bugfix:  10_FRM: accept Firmata firmware without AnalogInputFirmata
  - bugfix:  10_MYSENSORS_DEVICE: corrected S_LIGHT_LEVEL
  - bugfix:  93_DbRep: fix "month out of range" that causes fhem crash
  - feature: 20_FRM_PWM: new attribute "restoreOnStartup"
  - feature: 20_FRM_OUT: new attributes "activeLow" and "valueMode"
  - feature: 10_FRM: SerialFirmata support
  - update:  10_FRM: OWX IODev assignment
  - update:  10_FRM: Firmata 2.7+ support
  - bugfix:  98_weekprofile: fix "error restore topic"
  - change:  14_CUL_TCM97001: Fix Logoutput, Fix device output with
             multiple sensors
  - change:  74_AMADDevice: change DEF and add Attribut IODev, add Reading
                            incommingSmsText
  - change:  74_XiaomiFlowerSens: fix Problems with sshHost Methode
  - change:  73_GardenaSmartBridge/74_GardenaSmartDevice: add NotifyFn Support
             change AttrFn Routine
  - feature: 93_DbRep: V7.2.0, new attributes "seqDoubletsVariance",
                       "timeYearPeriod", minor fixes
  - feature: 98_TRAFFIC: v1.3.3, added alternatives, various improvements
  - feature: 70_BRAVIA: new command "application" to start an application on TV
  - feature: FHEMWEB: add structure to roomnames (Forum #63530)
  - feature: 98_dewpoint: Generated readings are now subject to standard
                       processing.
                       ! Be sure to add readings to event-on- .... attributes
                       ! if you want events to be generated !
  - feature: 93_DbLog: V3.6.0, check global blockingCallMax in configCheck,
                       configCheck available also for SQLITE now
  - feature: 10_SOMFY: internal rework / prep for Alex / position command
  - feature: 70_BRAVIA: new command "text" to add text to an input field
  - changed: allowed.pm/fhem.pl: SecurityCheck cleanup, Forum #81509
  - new:     88_xs1Bridge: New modul to read xs1 EZcontrol
  - change:  93_DbRep: V7.0.0, changelog:
                       - faster exec if no time attribut/aggregation is set
                       - bugfix in fetchrows if data contain chars like "'
                       - new command get blockinginfo
                       - identify if reopen is running on assigned dblog-device
                       - bugfix in delSeqDoublets
                       - internal code changes/reviews
  - feature: 50_TelegramBot: new set cmd silentmsg to disable_notification
  - bugfix:  73_GardenaSmart: v0.4.0 bugfixes
  - feature: 31_PLAYBULB: v1.4.0 support for Sphere Model BTL301w
  - change:  77_UWZ: v2.0.0, replace Iconv-Converter with perl encode()
  - change:  93_DbLog: V3.4.0, importCacheFile, addCacheLine use char filter
                       (switch it on with attribute useCharfilter)
  - feature: 98_GOOGLECAST: support displaying websites on Chromecast
                            pychromecast > 1.0.0 needed
                            support skip/rewind
  - feature: 10_EQ3BT: support maxRetries and timeout attribute
  - bugfix:  98_DLNARenderer: fix renew subscription warnings
  - feature: 98_BOSEST: support Audio Notification API for TTS
                        no more minidlna installation needed
                        only supported for up to 100 characters
  - new:     97_PiXtendV2: New module to control a PiXtend V2 -S- board
  - change:  93_DbLog: V3.4.0, avoid output RUNNING_PID + args by "list device"
  - new:     50_MOBILEALERTSGW/51_MOBILEALERTS: New moduls for MobileAlerts
  - change:  93_DbRep: V6.4.2, changelist:
                       - prepare for usage of datetime picker widget
                       - new attr "sqlResultFieldSep" (field separator)
                       - change "delSeqDoublets" to respect attribute "limit"
                       - bug fix in "delSeqDoublets delete" function
  - change:  93_DbLog: V3.3.0 ,changelist to last version 2.2.15:
                       - enhanced log output of reduceLog,reduceLogNbl
                       - new command addCacheLine,add data to cache immediately
                       - new attr "useCharfilter"
                       - new attr "commitMode", see commandref
                       - avoid print out the content of cache by "list device"
                       - minor fixes
  - feature: 99_weekprofile: add support for CCU2 (experimental)
  - change:  93_DbRep: V6.3.2 ,changelist to last version:
                       - new command delSeqDoublets
                       - add last command option to internal LASTCMD
                       - add format d:xx h:xx m:xx s:xx for attributes
                         timeDiffToNow, timeOlderThan
                       - new attribute fetchRoute to switch asc,desc datafetch
  - change:  HttpUtils: compression activated
             disable it with attr global httpcompress 0
  - bugfix:  46_SmartPi: fix syntax error bug in Attribut Sub
  - change:  98_dewpoint: Refactoring using API calls, verbose attribute added
  - change:  FileLog removes newlines from the data (Forum #79684)
  - bugfix:  98_Siro.pm: Support favorit for model ERB15LE
  - feature: notify/FileLog: add ignoreRegexp attribute (Forum #79684)
  - feature: 46_SmartPi: add decimal Attr, fix Notify bug
  - bugfix:  74_XiaomiFlowerSens: fix many Notify bugs
  - change:  backup is always started in the background (Forum #80237)
  - bugfix:  72_FB_CALLMONITOR: fix not working reverse-search-phonebook
             file import
  - change:  93_DbLog: V2.22.15, some Log verbose level adapted/added
  - bugfix:  44_S7_ARead: event-on-change-reading
  - bugfix:  44_S7_AWrite: event-on-change-reading
  - bugfix:  44_S7_DRead: event-on-change-reading
  - bugfix:  44_S7_DWrite: event-on-change-reading
  - bugfix:  44_S7_S5Client.pm: loading serial modul
  - change:  89_FULLY: on-timer implemented
  - change:  77_SMAEM: V3.0.1, use abort cause of BlockingCall
  - change:  93_Log2Syslog: V3.2.0, add NOTIFYDEV (if possible)
  - change:  70_BRAVIA: set remoteControl supports command codes
  - change:  98_dewpoint: Consolidated and corrected formulas for dewpoint
                          (Forum #78359)
  - fix:     00_SIGNALduino: Fix Bresser Sensor and perl sensor
                             max length was to short (Forum #79929)
  - bugfix:  74_GardenaSmartBridge: change state to connected
  - bugfix:  74_XiaomiFlowerSens: fix change InternalTimer now
  - bugfix:  49_SSCam: V3.2.4, don't retrieve presets during restart if cam is
                       disabled
  - feature: 98_Hyperion: - new "set binary restart/stop"
                          - non-blocking for "get configFiles",
                            "set configFile" and "set binary"
                          - ATTENTION: change from command killall to kill,
                            please adjust your sudoers file (if applicable)
  - new:     14_SD_RSL - basic support for conrad RSL
  - update:  14_Hideki: windsensor support added
             00_SIGNALduino: Updated to v3.3.2
             14_SD_WS: new tfa sensor supported
             14_SD_WS07: extraction of rssi value support
             14_SD_WS09: wind/rain total support
  - change:  93_DbLog: V2.22.14, create state-events if state has been changed
                       (Forum:#78867)
  - feature: 10_EQ3BT: support remote Bluetooth interface via SSH (thx@Cooltux!)
  - feature: 93_DbRep: V6.0.0, FTP transfer dumpfile after dump (MySQL), delete
                       old dumpfiles within Blockingcall, minor fixes
  - feature: 57_Calendar: new field categories (nils_, Forum #79237)
  - change:  72_FB_CALLMONITOR: delete stored FRITZ!Box password in
             FHEM/uniqueID file upon deletion of a FB_CALLMONITOR definition
  - feature: TR064Utils.pm added
  - changed: 88_HMCCU: Improved attributes ccureadingfilter, stripnumber
  - feature: 89_FULLY: New commands for motion detection and brightness
  - update:  98_Siro.pm: add Disable attribute
  - bugfix:  50_TelegramBot: fix minusdesc warning / cleanup
  - fix:     71_YAMAHA_AVR: fix navigateListMenu on RX-Vx65/RX-Vx67 series
  - feature: 89_FULLY: Turn motion detection on or off
  - new:     89_FULLY: Control Fully Browser
  - bugfix:  72_FB_CALLMONITOR: replace all unicode placeholders correctly
             in reverse search results
  - feature: 72_FB_CALLMONITOR: block calls, that matches configured
             blocking rules (deflections) from the FritzBox
             (new attribute check-deflections), see commandref for details
  - changed: 98_Dooya: updated module
  - new:     98_Siro: New module for Siro blinds
  - bugfix:  73_UpsPico: Swap to Net::OpenSSH module and error message handling
  - changed: 37_harmony: added set inactive/active commands
  - bugfix: 31_Nello: syntax error
  - feature: fhemweb_iconRadio.js: add a user defined class to svg icons by
             prefix class<classname>@, improved matching for a numeric sequence
             of compare values, color numbers are now case insensitive
  - feature: fhemweb_iconButtons.js, fhemweb_iconLabel.js,
             fhemweb_iconSwitch.js: add a user defined class to svg icons by
             prefix class<classname>@, color numbers are now case insensitive
  - bugfix: 31_Nello: updated MQTT IP
  - feature: save writes a copy into restoreDirs (Forum #78769)
  - feature: WMBus: preliminary support for SML payload
  - feature: 98_DOIFtools: unattended save removed, Forum(78769)
               DOIFtools will perform save if allowed by
               attribute DOIFtoolsExecuteSave when creating automatically a
               readingsGroup for DOIF, an userReadings for DOIF, a DOIFtoolsLog
               or an icon for DOIF by user request
  - feature: 74_XiaomiFlowerMonitor: add attribut for Blocking.pm logoutput
  - bugfix:  14_CUL_TCM97001: Bug: "other state" bei W174,
             Plausibility check for W174, Append documentation
  - bugfix:  71_YAMAHA_AVR: fix max volume when using float values in
             set command "volume"
  - bugfix:  93_DbRep: V5.8.6, don't limit length of attr reading/device if
                       attr contains a list
  - feature: 70_KODI: added reading jsonResponse which contains the last
                        received message from Kodi
  - feature: 46_Aqicn: FHEMWEB text color formated, thanks to maddhin
  - update:  74_XiaomiFlowerMonitor: new version, change internal routine
  - feature: fhemweb_iconRadio.js: optionally colorize selected icons instead
                                    of its background by prefix use4icon@
  - feature: fhemweb_iconButtons.js: optionally colorize selected icons instead
                                     of its background by prefix use4icon@
  - feature: 93_DbRep: V5.8.5, attr device can be a devspec, attr reading can
                       be a list (pls. see commandref), minor fixes
  - update:  46_TeslaPowerwall2AC.pm: new formula to calculate batteryPower
  - new:     46_Aqicn.pm: new modul, fetch information about air quality by
                          city name
  - bugfix:  82_LGTV_WebOS: 1.2.0 bugfix - hack for properly fhem freez after
                            tvswitch off and more
  - change:  93_DbLog: V2.22.13, output of reopen command improved
  - bugfix:  93_DbLog: V2.22.12, avoid illegible messages in "state"
  - feature: 59_WUup: add set-command "update"
  - bugfix:  46_TeslaPowerwall2AC: fix get data internal timer bug
  - bugfix:  93_Log2Syslog: typo in commandref
  - feature: global dnsHostsFile attribute added (Forum #78025)
  - feature: 98_DOIFtools: add getter hsvColorGradient, returns a table of
             value, colornumber, RGB values and color bar using Color::hsv2rgb
  - new:     46_TeslaPowerwall2AC: retrieves data from a Tesla Powerwall 2AC
  - bugfix:  21_HEOSMaster: fix typo in define Fn
  - feature: 93_DbRep: V5.8.0, can set table as flexible argument for command
                               countEntries and fetchrows
  - new:     76_msgDialog: introducing new module to define dialogs for instant
                           messaging via TelegramBot, Jabber and yowsub
  - feature: 93_DbLog: V2.22.11, Attribute DbLogType expanded by SampleFill
  - feature: 93_DbRep: V5.7.1, commands tableCurrentPurge, tableCurrentFillup
  - feature: 98_DOIFtools: add getter modelColorGradient, returns a table of
             value, colornumber, RGB values and color bar using Color::pahColor
  - new:     98_Siro.pm: New module for Siro shutters
  - feature: 98_DOIFtools: add RGB color values to color table
  - bugfix:  88_HMCCURPC: fixed bug in event timeout handling
  - change:  59_LuftdatenInfo: DEF change (should happen automatically)
  - feature: 98_DOIFtools: add getter linearColorGradient, returns a table of
             value, colornumber, color bar
  - feature: 74_AMADDevice: add set command userFlowRun
  - change:  57_CALVIEW.pm: -new readings weekdayname and weekday
                            -new attr weekdayformat
  - feature: 88_HMCCU: Added parameter waitforccu to define command
  - bugfix:  42_SYSMON: PERL WARNING: Use of uninitialized value
  - bugfix:  59_WUup.pm: fix state and missing attributes (#695364, #696275)
  - change:  93_DbLog: V2.22.10, adapted to use extended abortArg
  - change:  76_SMAInverter: V2.9.2, adapted to use extended abortArg
  - feature: 77_UWZ: add new sortby creation and add Italia Maps
  - feature: 49_SSCam: V3.2.3, new optimizeParams command to set cam properties
  - bugfix:  72_FB_CALLMONITOR: fix wrong reverse-search of emergency call
             (110/112/...), fix missing deletion of phonebook on reread.
  - change:  93_DbRep: V5.6.4, use new Blocking.pm abortArg
  - bugfix:  22_HOMEMODE: v1.1.10 - fix notifydev for HomeEventsHolidayDevices
  - bugfix:  10_MQTT_DEVICE: fix set arguments
  - feature: 49_SSCam: V3.2.2, new command get listLog (SVS-Devs), minor fixes
  - change:  77_SMAEM: V3.0.0, make SMAEM ready for multimeter usage
  - new      /www/pgm2/fhemweb_icon*.js: new widgets for FHEMWEB iconButtons,
             iconLabel, iconRadio, iconSwitch (Forum:#75696)
  - bugfix:  93_DbRep: V5.6.3, crash due to wrong timestamp calc (Forum:#77328)
  - change:  01_FHEMWEB.js: on demand loading of fhemweb_*.js (Forum #76868)
  - bugfix:  73_GardenaSmartBridge: fix part of code
  - feature: 49_SSCam: V3.1.0, move extevent from CAM- to SVS-model, Reading
                       PollState enhanced, minor fixes
  - change:  93_DBLog: V2.22.8, avoid multiple entries of
                       Device:Reading-combinations in Dopdown-list when
                       creating SVG
  - bugfix:  10_MQTT_BRIDGE: fix comandref $device
  - feature: 74_AMADDevice: add media support for YouTubeKids
  - bugfix:  74_AMADautomagicFlowset_4.0.9.xml: fix restore volume bug
  - feature: 73_GardenaSmartBridge: add syntax check for disabledForIntervals
                                    check set Interval Valur greater than 0
  - feature: 74_XiaomiFlowerMonitor: add syntax check for disabledForIntervals
  - feature: LightScene: added set all command
  - feature: 49_SSCam: V3.0.0, new concept - differ between CAM-/SVS-device,
                       version is downwardly compatible, but homeMode-commands
                       are moved from CAM to SVS-device - ! SEE COMMANDREF !
  - bugfix:  71_YAMAHA_AVR: generate readings for tuner in DAB mode
  - bugfix:  93_DbLog: V2.22.7, bugfix in configCheck for PostgreSQL
  - feature: 10_MYSENSORS_DEVICE: updated to latest MYSENSORS version
  - feature: 50_TelegramBot: hide cmd in favorites/changed favorites confirm
  - feature: 49_SSCam: V2.9.0, function get homeModeState, minor fixes,
                       commandref revised
  - bugfix:  00_MQTT: fix event-on-change Reading
  - changed: 30_HUEBridge: added set inactive/active commands
                           create event for lastError reading
  - change:  93_DbLog: V2.22.6 commandref revised
  - new:     73_UpsPico: New module for UpsPico UPS from pimodules
  - feature: LightScene: added traversalOrder attribute
  - bugfix:  31_PLAYBULB: fix battery character value
  - bugfix:  00_MYSENSORS: fix delete gateway
  - bugfix:  82_LGTV_WebOS: fix Argument "none" isn't numeric in addition
  - bugfix:  73_AMADCommBridge: fix utf8 character in set mode
  - feature: 82_LGTV_WebOS: version 1.0.0 add WakeOnLAN function
  - bugfix:  00_MQTT: fix Undef
  - feature: 83_IOhomecontrol: new attribute setCmds
  - bugfix:  00_MQTT: added delete
  - new:     83_IOhomecontrol: control IOhomecontrol devices via REST API
  - feature: 31_PLAYBULB: add support for Candle S Firmware 1.4
  - feature: 73_GardenaSmartBridge: add attribut disabledForInterval
  - new:     73_WaterCalculator.pm: New module for water consumption and cost
  - bugfix:  73_AMADCommBridge: fix commandref and Flowset
  - feature: 74_AMADautomagicFlowset: add support for wired headset plugged
  - feature: 74_AMADDevice: add change temporary ttsMsg language, code clean
  - feature: 50_TelegramBot: new set cmd msgDelete
  - feature: 95_holiday: move holiday files from contrib to FHEM
  - feature: 31_Nello: updated to new api specifications
  - feature: 49_SSCam: V2.8.0, switch Surveillance Station HomeMode available
  - bugfix:  73_GardenaSmartBridge: code clean, update german tranlation
  - feature: 74_AMADDevice: add ttsMsgVol, sets automatically a preset volume
  - feature: proxy global attribute for HttpUtils (Forum #60471)
  - bugfix:  93_DbLog: V2.22.5, several fixes Forum:#75894
  - feature: 74_GardenaSmartDevice: check character for create devicenames
  - bugfix:  FHEM2FHEM: addStateEvent attribute (Forum #76229)
  - bugfix:  HttpUtils: use urlDecode for password in URL (Forum #76230)
  - bugfix:  74_GardenaSmartDevice.pm: fix little Commandref bug's
  - new:     73_GardenaSmartBridge/74_GardenaSmartDevice control your Gardena
                Smart Products
  - feature: 98_MediaList.pm: added sorting setting function,
                default sort by filename
  - feature: 10_pilight_ctrl: support protocol heitech
  - feature: 91_sequence: add delay and omit name options (Forum #75925)
  - bugfix:  74_AMADDevice: fix a lot of Bugs
  - feature: 93_Log2Syslog: V3.1.0, get certinfo added
  - bugfix:  73_AMADCommBridge: fix doubble set Command at Bridge
  - bugfix:  31_PLAYBULB: fix right curl Missing
  - changed: 72_FB_CALLMONITOR: reverse search only numbers for the specific
             country (e.g. german numbers only via klicktel.de,dasoertliche.de,
             austrian numbers via dasschnelle.at, swiss via search.ch)
  - feature: 37_Spotify: new readings
  - new:     93_Log2Syslog: V3.0.0, first release
  - bugfix:  93_DbRep: V5.6.2, commandref revised
  - feature: 00_MQTT: OnMessageFn, last-will, onConnect/onDisconnect
  - feature: 10_MQTT_DEVICE: improved publishSet, retain, subscribeReadings
  - feature: 10_MQTT_BRIDGE: improved retain, subscribeSet
  - new:     31_Aurora.pm: first release
  - bugfix:  21_HEOS: fix missing curl
  - bugfix:  31_PLAYBULB: code cleaning
  - bugfix:  21_HEOS: little Bugfixes, code cleanup
  - changed: 88_HMCCU Version 4.1.001
  - feature: HttpUtils/IPv6 with the useInet6 global attribute (Forum #75557)
  - bugfix:  74_AMADautomagicFlowset_4.0.5.xml: add openTask Check with
                                                timer trigger
  - bugfix:  49_SSCam: V2.7.0, set maximum password lenth to 20
  - bugfix:  73_AMADCommBridge: fix AnalyzeCommandChain sub call, fix
                                AMADautomagicFlowset
  - bugfix:  72_FB_CALLLIST: fix shifted table header
  - new:     59_WUup: first release (Forum #65587)
  - feature: 49_SSCam: V2.6.3, snapGallery can be triggered by e.g. notify
  - bugfix:  93_DbLog: V2.22.3, Forum:#74690, unitialized message in row ...
  - feature: 34_ESPEasy: reject non local IPs wo/ basic auth
  - bugfix:  50_TelegramBot: delayed retry & rename (#msg668108)
  - changed: 70_BRAVIA: renamed reading/internal modelName to model
  - new:     98_GOOGLECAST: first release, read commandref for requirements
  - changed: 74_AMADautomagicFlowset_4.0.3.xml: workaround for better auto
                                                flowsetupdate
  - feature: 74_AMADDevice: 4.0.5 - Support für NFC and scanning NFC TagId
  - bugfix:  74_AMADautomagicFlowset_4.0.2.xml: fix openApp Trigger
  - bugfix:  31_Nello: fixed device ID detection
  - feature: 93_DbLog: V2.22.1, new attribute "suppressAddLogV3"
  - feature: 49_SSCam: V2.6.1, new commands snapGallery, createSnapGallery and
                       corresponding attributes
  - feature: 34_ESPEasy.pm: plugin neopixelfx/nfx added (Forum #73949)
  - new:     31_Nello: first release
  - feature: 01_FHEMWEB.pm: add webCmdLabel (Forum #72581)
  - changed: fhem.pl: search cmds via lowercase/abbrev in modules (Forum #75007)
  - changed: 14_CUL_TCM97001: Add rain/wind Sensor
  - changed: 10_IT: Add FreeTec update documentation
  - changed: configDB: store files base64 encoded, Forum:#74302
  - bugfix:  93_DbLog, back to V2.22.0, Forum:#75039
  - bugfix:  93_DbLog, V2.22.1, Forum:#74690, warning unitialized value
  - feature: 70_WINCONNECT: [WinWebGUI] - Fenster verstecken
  - feature: 57_Calendar: added attribute cutoffOlderThan (forum #74481)
  - feature: fhem.pl: add -d option for debugging (Forum #74774)
  - bugfix:  74_AMADDevice: fix decode_utf8 call in eval
  - feature: 57_Calendar: reduce memory footprint (forum #74481)
  - bugfix:  74_AMADDevice: fix openurl bug
  - bugfix:  49_SSCam: "uninitialized value in pattern ..." on fhem start
  - feature: 49_SSCam: V2.4.0, new commands "snapinfo" and
                       "runView lastsnap_fw", minor fixes
  - feature: 93_DbLog: V2.22.0, new attribute "addStateEvent"
  - bugfix:  74_AMADDevice: Version 4.0.1 Charset utf8
  - changed: 93_DBLog: V.2.21.3, commandref revised
  - new:     74_AMADDevice: New Version of AMAD (AMADNG) Verion 4.0
  - new:     73_AMADCommBridge: New Version of AMAD (AMADNG) Verion 4.0
  - change:  74_AMAD: delete from SVN
  - new:     70_NEUTRINO: new modul for neutrino sat receiver
  - bugfix:  74_AMAD: Change Commandref
  - change:  93_DbLog: V2.21.2, some improvements like get reading 'state' of
                       state-events, timeout increased, change configCheck for
                       DbRep Report_Idx
  - new:     46_SmartPi: Support read data from  Smart Pi expansion module
  - change:  93_DbRep: V5.6.1, commandref revised, minor fixes
  - feature: 93_DbRep: V2.6.0, new get-command "procinfo" (MySQL), default
                       timeout changed to 86400
  - bugfix:  93_DbRep: minor bugfixes (thanks to Omega)
  - feature: 49_TBot_List: configure also add with attr confirmUnsolicited
  - feature: 49_TBot_List: configure confirm delete  as attribute confirmDelete
  - changed: 98_fheminfo.pm: remove release, featurelevel, uptime infos
  - added:   98_uptime.pm: new command module to show FHEM uptime
  - change:  93_DbLog: V2.19.0, replace internal DBMODEL by MODEL completely
  - update:  88_HMCCU: Version 4.1
  - feature: 93_DbRep: V5.5.0, new command restoreMySQL, use new Internal
             MODEL in DbLog since version 2.18.2
  - feature: 98_fheminfo: do not show complete uniqueid in frontend
  - feature: 77_UWZ: 1.6.0 add new attribut intervalAtWarnLevel for flexible
                     warn timer
  - feature: 10_FS20: add useSetExtensions attribute, default is 1
  - feature: 82_LGTV_WebOS: Version 0.8.0, fix screenMsg Charset problem
  - bugfix:  93_DbLog: V2.18.3, cannot load V2.18.2, new internal 'model'
  - bugfix:  list: do not change the upper casing of hashes (Forum #73828)
  - bugfix:  71_YAMAHA_NP: Prevent directPlay from starting netradio stream
             several times in slow internet connections
  - feature: 93_DbLog: V2.18.2, new command configCheck for MySQL, PostgreSQL
  - new:     98_archetype: introducing new  module to inheritance attributes
                and defines devices
  - bugfix:  50_TelegramBot: rewrite readfile function $_ warning - #msg651947
  - bugfix:  49_SSCAM: V2.2.3, fix if SVSversion small is "0"
  - new:     00_SmartMeterP1: V1.7 New module for reading elec.+gas smartmeters.
  - feature: 93_DbRep: V5.3.1, new commands optimizeTables (MySQL) and vacuum
                               (SQLite, PostgreSQL) to optimize database
  - bugfix:  36_Vallox: Added Bus Version Handling. Misc Bugfixes.
  - bugfix:  32_withings: temporary fix of login function before rewrite
  - bugfix:  93_DbRep: V5.2.1, bugfix in sqlCmd to support PRAGMA, UTF8
  - feature: 93_DbLog: V2.17.1, optional UTF-8 support for MySQL database
             (additional parameter in db.conf neccesary for activation)
  - feature: YAMAHA_AVR: new set commands / readings to control HDMI outputs
             (only for models with two HDMI outputs)
  - featere: exclude_from_update can check the source too (Forum #73275)
  - change:  93_DbRep: V5.2.0, preparation for UTF-8 support by DbLog
  - bugfix:  36_Vallox: Changed read. Added attributes. Changed DeviceID.
  - bugfix:  MQTT: undef patch
  - bugfix:  ESPEasy: added missing event command (Forum #73291)
  - bugfix:  YAMAHA_AVR: use DSP-based commands for RX-V2065
  - bugfix:  MQTT_DEVICE: publishSet patch (Forum #msg648963)
  - feature: MQTT_DEVICE: publishSet patch (Forum #msg648596)
  - feature: 01_FHEMWEB.pm: selectnumbers widget modifier (Forum #73188)
  - feature: 98_structure.pm: add evaluateSetResult attribute (Forum #73113)
  - feature: ESPEasy: improved defineFn if bridge port is missing, docu update
  - feature: 37_Spotify: resume on target
  - feature: 93_DbRep: V5.1.0, create dumps of MySQL on client- or serverside,
                       column UNIT is added to the result of fetchrows-command
  - feature: ESPEasy: command reference revised
  - bugfix:  49_SSCam: crash after FHEM-restart if answer from DS is empty
  - update:  98_DOIFtools: chaining DOIF's detailFn if present
  - feature: ESPEasy: added: dmx, motorshield, neopixel, candle, serialsend...
  - feature: 57_Calendar: asynchronous parsing, disable update
  - change:  34_ESPEasy: add IPv6 ULA to local IPs, add regexps to ACLs
  - bugfix:  93_DbLog: V2.16.11, lock SQLite from logging if deleteOldDaysNbl
                       or reduceLogNbL is running in async mode
  - feature: ESPEasy: improved dual ip stack support
  - change:  FHEMWEB/telnet needs password if directly(!) connected to the
             internet, see https://forum.fhem.de/index.php?topic=72717
  - change:  34_ESPEasy: adjustments due to changes in TcpServerUtils.pm
  - feature: 44_S7_ARead: supports for Logo7 and Logo8 short notations
  - feature: 44_S7_AWrite: supports for Logo7 and Logo8 short notations
  - feature: 37_Spotify: specify default device by its name
  - feature: 98_alarmclock: New feature stop Alarm
  - bugfix:   98_DOIFtools: fixed empty N_timer
  - bugfix:  37_Spotify: fixed offset playContextByURI
  - bugfix:  38_CO20: fixed reconnects, improved stability
  - feature:  37_Spotify: album cover, new attr, return error to reading
  - feature:  37_Spotify: trigger events on reading changes
  - bugfix:  37_Spotify: fixed prototype warning
  - feature: 37_Spotify: first release
  - bugfix:  38_netatmo: fixed blocking connection check on dns error
  - change:  02_RSS: height/width for rect layout directive
  - change:  34_ESPEasy: performance tuning, some fixes
  - feature:  74_Unifi.pm: added get poeMode and set poeState commands
                           added _utilization and _poePower readings
  - feature: 93_DbRep: v4.16.1, json as option of sqlResultFormat
  - feature: 31_PLAYBULB: add support for ssh remote control
  - change:  42_Nextion: fault tolerance in reader / fixes
  - feature: 50_TelegramBot: favorites rework - inline / allow : in inline
  - change:  49_TBot_List: changed query data to prefix TBL_ / quiet peerid
  - feature: 98_alarmclock: New features AlarmTime9_Vacation, skip next Alarm
  - new      21_HEOS*: new modules to provide HEOS Multiroomsystem
  - bugfix   93_DbRep: commandref corrected
  - change:  SubProcess.pm: buffer reads, messages amended
  - feature: 98_alarmclock: New feature PresenceDevice
  - change:  49_SSCam: version 2.2.1, last record playback possible as iFrame,
                       deviceoverview available,
                       CAUTION - syntax of runView options has been changed !!
  - change:  22_HOMEMODE: v1.1.0 please change %ALARM% to %ALARMHR%
  - change:  93_DbRep: version 4.15.0, limitation of fetchrows result to 1000
                       adjustable by attr limit, performance increased in many
                       cases, some bugfixes of PostgreSQL sumValue/averageValue
  - change:  93_DbLog: new version 2.16.10, syntax of addlog command changed,
                       reading userCommandResult contains "no result" if the
                       db interface delivers undef
  - feature: 93_DbRep: new version 4.14.0, new command sqlCmd to execute
                       arbitrary sql commands (thanks viegener for input),
                       DbRep provides an userExit interface to execute
                       customer code independent from events
  - bugfix:  74_NUKIDevice: fix success Reading num
  - bugfix:  42_SYSMON: wlan speed, memory usage detection
  - update:  57_Calender: optimization for speed
  - bugfix:  36_Vallox: Changed way multireadings are updated.
  - feature: 49_TBot_List: sorting entries plus corrections
  - bugfix:  73_PRESENCE: fix restart of threshold counter after FHEM restart
  - feature: 44_S7: new attribute receiveTimeoutMs
  - feature: 38_CO20: introduced state reading
  - change:  73_NUKIBridge,74_NUKIDevice: fix Perlwarnings
  - bugfix:  38_CO20: fixed definition with serial number
  - bugfix:  32_withings: safer json decoding
  - feature: 38_netatmo: home notification settings
  - feature: 98_alarmclock: New feature RepRoutine
  - feature: 31_PLAYBULB: support for new Garden Model, move battery Reading to
                          powerLevel and add powerCharge Reading for Garden
  - feature: 00_DFPlayerMini: improved requestAck handling
  - change:  49_SSCam: new version 2.1.3, change of internal processes, new
             get scanVirgin command
  - bugfix:  73_ElectricityCalculator: SiPrefix multiplier instead divider
  - bugfix:  73_GasCalculator: SiPrefix multiplier instead divider
  - bugfix   73_km200: Errorlist unsorted timestamp part 4
  - change:  36_Vallox: Changed way readings are updated.
                Added efficiency calculation and readings for HRC.
  - change:  71_YAMAHA_AVR: changing values of reading values conform
             to FHEM AV guidelines ("stopped", "playing" or "paused")
  - bugfix   73_km200.pm: Errorlist unsorted timestamp part 3
  - bugfix:  76_SMAInverter: version 2.9.1, issues for some inverter types
                             e.g. SunnyBoy systems
  - bugfix:  36_Vallox: Correction of binary reading interpretations. Optimized.
                Added Set for binary values.
  - feature: 34_ESPEasy: add use of encode_utf8 for json_decode
  - new:     36_Vallox: support Vallox DigitSE ventilation system
  - feature: 71_YAMAHA_AVR: new set command & readings for displayBrightness,
             extraBass, surroundDecoder and ypaoVolume
  - change:  70_ENIGMA2: HDD capacity is now re-calculated to GB if unit can be
                         determined
  - bugfix:  88_HMCCU: Fixed bug during FHEM start
  - feature: 88_HMCCU: New reading based calculation modes
  - feature: 34_ESPEasy.pm: Added ESPeasy Mega internals build.*
  - bugfix   73_km200.pm: Errorlist unsorted timestamp
  - bugfix:  72_FB_CALLMONITOR: fix reverse-search of dasschnelle.at
  - feature: 70_BRAVIA: command remoteControl supports 'PictureMode'
  - bugfix:  22_HOMEMODE: Use of uninitialized value $d in hash element
             minor commandref fix
  - new:     22_HOMEMODE: initial SVN check-in v1.0.0
  - bugfix:  74_AMAD: fix Use of uninitialized value,no Flowset update nececcary
  - feature: 34_ESPEasy: added ESPEasy commands: tone and rtttl
  - bugfix:  88_HMCCU: fixed config commands
  - feature: 30_pilight_contact: add battery reading if information is available
  - update:  88_HMCCU: Homematic firmware download, advanced scripting
  - feature: 98_TRAFFIC: v1.3.2, stroke styles, warnings reduced, bugfix
  - update:  98_DOIFtools: more precise regexp for INITIALIZED event because
                there is more than one initialisation event now
  - feature: 82_LGTV_WebOS: Version 0.6.0, pingPresence, Bugfixes
  - bugfix:  02_FTUISRV: fix replacesetMagic to use hash - fhem.pl warning
  - bugfix:  10_pilight_ctrl: fix GS-iwds07
  - feature: 98_TRAFFIC: v1.3.1, attribute change, map setting save buttons
  - feature: 98_TRAFFIC: v1.3, map customizable, enhancements, fix JSON error
  - change:  76_SMAInverter: changed SMA_logon, enhanced inverter Types
  - feature: 98_DLNARenderer: support $readingFnAttributes
  - feature: 34_ESPEasy: urlEncode text for display commands
  - feature:  71_PHILIPS_AUDIO: Added NP3500 support. "lvl" Reading bugfix.
  - change:  93_DbLog: version 2.16.5 primary key evaluation changed
  - bugfix:  32_withings: updated for new account key characters
  - bugfix:  71_PHILIPS_AUDIO: fhem.pl crash while server shutdown
  - feature: 33_readingsGroup: allow "set magic" reding pre- and suffixes
  - bugfix:  71_PHILIPS_AUDIO: Corrected gavorites behaviour if more than 16
  - chnage:  17_EGPM2LAN.pm: Password handling changed; removed from config
  - change:  93_DbRep: version 4.12.2, PK evaluation changed
  - bugfix:  71_PHILIPS_AUDIO: Player readings fix.
  - feature: 71_PHILIPS_AUDIO: Module rewritten for better usability.
                               New commands. See documentation.
  - update:  38_CO20: identify devices by id / serial number
  - update:  38_netatmo: dynamic update intervals for devices
  - update:  98_weekprofile: update reading profile_count after save profiles
  - feature: 98_weekprofile: new attribute widgetTranslations for translations
  - bugfix:  98_weekprofile: handle csrfToken
  - bugfix:  02_HTTPSRV: strip parameters from filename
  - bugfix:  88_HMCCURPC: fixed binary RPC init procedure
  - feature: 93_DBLog: new version 2.16.3, new command addlog,
                       new attr valueFn, split events of ZWAVE
  - bugfix:  38_netatmo: fixed camera settings dependencies
  - update:  88_HMCCU: Version 4.0 with CUxD support
  - feature: RESIDENTStk wakeuptimer: wakeupEnforced may be 3 to only enforce
               wake-up when wake-up time is set earlier than
               default wake-up time
  - new:     10_pilight_ctrl: support temperature protocols bmp085 and bmp180
  - new:     10_pilight_ctrl: support contact sensor GW-iwds07
  - new:     59_LuftdatenInfo: introducing new module to fetch PM, temperature
                and humidity data from Luftdaten.info
  - change:  93_DbRep: new version 4.12.1, get tableinfo changed for MySQL
  - bugfix:  98_DOIFtools: fixed browser issues for Chrome and IE
  - feature: 98_monitoring: whitelist attribute added
  - feature: 93_DbRep: support of primary key (set in table history/current)
  - update:  88_HMCCU: Optimized reading update performance
  - feature: 00_SONOS: New lists for groupinformations
  - bugfix:  88_HMCCU: Fixed toggle function for HMCCUCHN devices
  - change:  93_DbLog: new version 2.14.4, new set-commands exportCache,
                       importCachefile, some fixes (e.g. many SVGs from SQLite
                       in one room)
  - bugfix:  93_DbRep: bugfix timestamp in minValue, maxValue if DB-VALUE
                       contains more than one numeric value (e.g. in sysmon)
  - bugfix:  38_netatmo: sanity check for dynamic interval
  - bugfix:  88_HMCCU: fixed bug in update of virtual devices
  - feature: 70_BRAVIA: command remoteControl supports 'Netflix'
  - feature: 50_TelegramBot:  favorite handling / hidden favorites /
                utf8Special for unicode issues /
  - new:     00_DFPlayerMini: module to control an embedded MP3 player
  - feature: 75_MSG: add support for PostMe module
  - feature: 74_XiaomiFlowerSens: 1.0.1 new Attributs minLux and maxLux
  - feature: 98_monitoring: blacklist attribute is now a space seperated list
                of devspecs instead a comma seperated list of devices
  - bugfix:  32_withings: web token fix
  - bugfix:  93_DbRep: switch wintertime to summertime, minor fixes
  - update:  32_withings: account data encryption
  - update:  38_netatmo: dynamic interval, various fixes, logging changes
  - feature: 75_MSG: add support for parseParams
  - feature: 10_RESIDENTS: add new durTimer* readings, similar to
                           ROOMMATE/GUEST
  - update:  49_SSCAM new version 1.42, minor fixes
  - update:  88_HMCCU: Optimized code
  - update:  88_HMCCURPC: Optimized error handling
  - feature: 74_XiaomiFlowerSens: 1.0.0, add Attribut ssh Support for remote
                                  call, Atrribut min and max Value for Reading-
                                  Warnings
  - update:  98_DOIFtools: real next timer handles DOIF's attribute weekdays
  - update:  88_HMCCU: Introducing new client module HMCCURPC.
  - new:     74_Nmap: introducing new module to perform a network scan with
                Nmap and display information about the available network
                devices
  - update:  98_DOIFtools: better shortcut positioning
  - feature: 70_Pushover: new command 'msgCancel' to prematurely cancel
                          confirmation requests for priority 2 messages
  - feature: 00_SONOS: New feature 'get Queue' added
  - update:  98_DOIFtools: few more derived operands
                           in DOIFtools event monitor assistant
  - new:     98_monitoring: introducing new  module to monitor devices towards
                events and stores them in two lists
  - update:  88_HMCCU: Prepared code for version 4.
  - update:  98_DOIFtools: minor fixes, added create DOIF Definition with
                event derived operands when using event monitor in DOIFtools
  - update:  49_TBot_List: handleUnsolicited & multiline entries
  - bugfix:  93_DbRep: get svrinfo has only used /opt/fhem/fhem.db (SQLite)
  - new:     98_expandJSON: initial check in
  - update:  98_DOIFtools: added hints to the derived operands
  - update:  98_Text2Speech: some small improvements
                special Audiodevice "none" is now "default due
                collision with new Server mode
  - update:  98_DOIFtools: Improved DOIF-Operand derivation from an event line
                if the event monitor is opend in DOIFs detail view.
                Improved dialog to insert the  selected operand in a definition
  - new:     31_PLAYBULB: Integrates different smart lights from MIPOW and
                          displays several settings
  - bugfix:  00_SONOS: Errorhandling for RadioName etc.
  - feature: 98_template: new FHEM command template
  - feature: 70_MEDIAPORTAL: Plugins can be retreived and changed to
  - update:  00_SONOS: New version, see Wiki- or File-Changelog
  - update:  88_HMCCU: Code optimized. Fixed Windows process ID bug.
  - bugfix:  71_YAMAHA_NP: Fixed tuner readings in standby.
  - bugfix:  42_Nextion:  mult. fixes - page10 / disconnect / init
  - bugfix:  71_YAMAHA_NP: Fixed volume slider
  - bugfix:  95_Dashboard: fixed issue with csrf token that prevents
                           ajax request to succeed
  - feature: 71_YAMAHA_NP: Code rewritten for improved usabiliy. See docs.
  - new:     98_MediaList: adds support to navigate through local attached
             media library, pls see https://wiki.fhem.de/wiki/MediaList
  - feature: 98_Text2Speech: new server mode to serve audiofile for requestors
  - feature: at+notify: extend the FHEMWEB Wizard with a simple command modifier
  - feature: 42_SYSMON: support ssh login with public key
  - bugfix:  10_EQ3BT: fix lastChangeBy reading
  - bugfix:  74_AMAD: 2.6.12 fix empty androidVersion Reading when use Nougat
  - feature: 42_SYSMON: added ssh support (thx to PitpatV), minor fixes
  - bugfix:  88_HMCCU: Fixed toggle bug
  - bugfix:  60_allergy.pm: fixed error handling for server replies
  - update:  38_netatmo.pm: 3 stations minimum for PUBLIC statistics
  - update:  74_AMAD: new Version 2.6.11, add startDaydream and more media
                      commands
  - update:  93_DbRep: V4.11.1, new options for timestamp_begin,timestamp_end
                       see commandref for details
  - update:  88_HMCCU: added tracing for RPC set config
  - bugfix:  32_withings: removed experimental code
  - new:     82_LGTV_WebOS: to control LG TV's with WebOS
  - bugfix:  42_Nextion:  restore version
  - feature: YAMAHA_AVR: new attribute volumeMax to limit the maximum volume
  - update:  70_WS3600.pm extension for UV and illuminance
  - bugfix:  38_CO20.pm: fixed Device::USB init errors
  - update:  93_DBLog: new Version 2.13.5, supports primary key now,
                      set commands clearReadings and eraseReadings,
                      non-blocking variants of count, reducelog and
                      deleteOldDays
  - update:  88_HMCCU: Code optimized
  - new:     49_TBot_List.pm: initial check in
  - feature: 42_Nextion:  attributes disable/timeout, fix for page 10
  - update:  02_FTUISRV: doc change on ftui-if
  - feature: 50_TelegramBot:  Secured: api key handled in setkey/getkey
                  msgChatId with peer / communication with TBot_List
  - update:  98_DOIFtools: add a possibility to set the attribute icon for DOIF
                by multiselect to helper_doif, DOIF's new icon D[:]IF
  - update:  38_netatmo.pm: API changes
  - new:     34_ESPEasy.pm: initial check in
  - bugfix:  38_netatmo.pm: fixed error crash
  - update:  32_withings.pm: added unknown values for body scale
  - update:  98_DOIFtools: add CSRF-Token, add DOIFtoolsLogDir
  - bugfix:  38_netatmo.pm: fixed login crash, updated webhooks
  - update:  32_withings.pm: replaced with new module
  - feature: 5.8 released

- 2017-02-19 (5.8)
  - feature: 88_HMCCU: advanced reading filters
  - feature: 74_AMAD: add closeCall command
  - bugfix:  98_DOIFtools: some more webname issues
  - bugfix:  98_DOIFtools: webname ignored
  - bugfix:  74_XiaomiFlowerSens: 0.6.8 new set command
  - feature: 23_LUXTRONIK2: new heatSourceDefrost-Readings
  - bugfix:  74_XiaomiFlowerSens: 0.6.6 change RegEx for Error Handling
  - feature: 93_DBLog: attributes colEvent, colReading, colValue now also
                       valid for SQLite DB
  - update:  98_DOIFtools: two more checks in checkDOIF
                output language depends now on global attribute language
                recommedation in checkDOIF is now in german language available
  - feature: 02_FTUISRV: attribute templatefile and more tolerance on spaces
  - bugfix:  74_XiaomiFlowerSens: 0.6.5 bugfix in gatttool Routine
  - bugfix:  73_ElectricityCalculator: Power peaks due fhem Blocksge
  - bugfix:  98_Text2Speech: writing stats for checking outdated files fixed
                             Attr TTS_noStatisticsLog now working properly
  - bugfix:  74_XiaomiFlowerSens: 0.6.4 rewrite Errorhandling
  - bugfix:  70_BRAVIA: utf-8 character handling
                        use WOL only if device is absent (exception 2013 model)
                        respect channel uri for tv input selection
  - changed: 93_DbRep: V4.10.3, rename reading "diff-overrun_limit-"
             to "diff_overrun_limit_"
  - changed: 57_Calendar: avoid some warnings
  - bufix:   00_MQTT: fixed delete MQTT_DEVICE
  - update:  98_DOIFtools: suppress lookup windows in DOIF or DOIFtools
                by attribute DOIFtoolsNoLookUp and DOIFtoolsNoLookUpInDOIF
  - bugfix:  88_HMCCU: Bug fixes
  - update:  98_DOIFtools: improved lookup window handling for for huge content
                add attributes section and Ok button
  - update:  98_DOIFtools: add lookup window for probably assiciated devices
                (internals and readings) in DOIF and DOIFtools detail view
  - bugfix:  FB_CALLIST: cleanup readings on set command clear
  - update:  88_HMCCU.pm: version 3.9.001 with minor changes
  - update:  98_DOIFtools: add attribute to move event monitor directly above
                readings section in detail view of DOIF
  - update:  93_DbLog: update to version 2.11.1, solves some issues since
                version 2.10.4, command set ... reopen extended
  - update:  98_DOIFtools.pm: add some hints, improved logfile handling
  - bugfix:  74_XiaomiFlowerSens: 0.6.3 fix blockingDone Routine
  - feature: 75_MSG: support for ReplaceSetMagic; msg command may now be used
                     with texts containing [device:reading] to replace with
                     found readings
  - feature: 98_weekprofile: attributes for temperature 'on' and 'off'
  - feature: 98_BOSEST: NEW REQUIREMENT sox, libsox-fmt-mp3 for TTS
  - feature: 98_BOSEST: support more than 100 chars for TTS
  - bugfix:  98_BOSEST: several TTS and Spotify bugfixes
  - feature: 98_BOSEST: support playPause toggle
  - feature: 10_EQ3BT: use all available BT interfaces
  - feature: 10_EQ3BT: new reading lastChangeBy FHEM/Thermostat
  - feature: 10_EQ3BT: support $readingFnAttribute
  - bugfix:  10_EQ3BT: do not run parallel gatttool commands for same dev
  - feature: FB_CALLMONITOR: new set command "reopen"
  - feature: 66_ECMD: new attribute autoReopen
  - update:  74_AMAD: Version 2.6.8 new feature sendSMS
  - feature: 66_ECMD: new attribute autoReopen
  - bugfix:  98_DOIFtools.pm: fixed bug from last change
  - update:  98_DOIFtools.pm: some code rework
  - update:  98_DOIFtools.pm: dynamic column width in report
  - update:  98_DOIFtools.pm: add delete readings in other devices than DOIF
  - update:  88_HMCCU.pm: version 3.9
  - update:  98_DOIFtools.pm: marking an eventline in DOIFs event monitor
               shows different representations of the event as operand
               for DOIF definitions
  - update:  73_NUKIBridge/74_NUKIDevice 0.6.0 Support for API v1.5
  - update:  98_DOIFtools.pm: new attribute DOIFtoolsEventOnDeleted generates
               events for stat_ Readings before deletion
               remove add... button in DOIFtools event monitor
  - changed: 00_SIGNALduino.pm: version 3.3.1
                 needs less cpu time for parsing messages
                 new command to query protocolids
                 improve send queue: Send not before response of previous
                 warnings and some errors fixed
                 compatibel with last changes from IT module
  -changed:  14_SD_WS.pm: new sensor bresser temeo supported
  - new:     98_QRCode.pm: Creating QRCodes for various purposes.
                           QRCodes ar generated by a web service.
  - bugfix:  98_DOIFtools.pm: fixed Error: >name< has no TYPE, but following
                keys: >< which occurs during a statistics report generation if
                devices are deleted during event recording before
  - bugfix:  HMCCUConf.pm: changed default value of ccudef-readingfilter
  - update:  10_IT: send EV1527 command for switch, change some log level
  - change:  98_powerMap: default value for reading pM_power was renamed to
                          pM_consumption to circumvent overlapping of commonly
                          used reading 'power' where it is normally used as
                          boolean.
  - update:  93_DbLog: its now version 2.10.4, some improvements and new
                       attributes
  - update:  74_XiaomiFlowerSens: 0.6.0 rewrite subroutinen for better handling
  - bugfix:  88_HMCCU.pm: fixed default attributes
  - update:  98_DOIFtools.pm: filter mentioned in event report
             Event monitor toggles instead on/off
             some shortcuts for get and set commands, hideable by attribute
  - new:     98_mark: new command mark added
                      to mark devices TEMPORARY or VOLATILE
  - bufix:   00_MQTT: fixed delete MQTT device
                      added setKeyValue/getKeyValue for username and password
  - changed: 49_SSCAM: compatibility to SVS 8.0.0
  - bugfix:  74_XiaomiFlowerSens 0.4.1, bugfix new error handling
  - update:  88_HMCCU: version 3.8
  - feature: 74_XiaomiFlowerSens 0.4.0, better error handling
  - change:  73_PRESENCE: store threshold counter in state file for restarts
  - feature: 98_DOIFtools.pm: new report filter for event rate
  - new:     96_Snapcast.pm: New module to control a snapcast server
  - update:  98_DOIFtools.pm: improved Attribute handling, help corrections
             new attribute DOIFtoolsHideStatReadings hides _stat Readings
             new device filter regex for report generation
             checkDOIF checks if timer referring DOIF's name have defaultvalues
  - feature: 98_powerMap: introduce pre-defined powerMap templates
                          for several FHEM modules
  - bugfix:  93_DbRep: uninitialized value renmode if role is Agent
  - update:  DOIFtools:documentation
  - new:     98_DOIFtools: tools for DOIF
  - bugfix:  93_DbLog: its now version 2.9.2 (thanks to DS_Starter)
               new bugfix for SQLite issue SVGs, DbLog_Log changed to
                 $dev_hash->{CHANGETIME}, DbLog_Push
               changed (db handle new separated)
               changed DbLog_ParseEvent to CallInstanceFn,
               renamed flushCache to purgeCache,
               renamed syncCache to commitCache,
               attr cacheEvents changed to 0,1,2
               changed DbLog_ParseEvent to CallFn
  - change:  73_PRESENCE: new collectord package to support RSSI selection
  - feature: 73_NUKIBridge,74_NUKIDevice: add NUKIDevice Readings rssi paired
  - feature: 73_PRESENCE:
             - new mode "event" to determine presence state based on events of
                other FHEM definitions.
             - new attributes "absenceTimeout" and "presenceTimeout" for
               absence/presence verification in mode "event".
  - feature: 11_OWDevice: new attribute cstrings, fix for trimvalues
  - new:     98_powerMap: introducing new module to calculate power and
                          energy for every FHEM device w/o power meter
  - updated: 38_netatmo.pm: added support for Presence, Homecoach & Webhook
  - new:     98_GoogleAuth.pm for use of 2-factor-authentication in FHEM
  - updated: codemirror & addons version to 5.22.0 (minified)
  - bugfix:  93_DbLog.pm: Version is now 2.9.1, "MySQL Server has gone",
                          new commands purgeCache, commitCache
  - bugfix:  74_XiaomiFlowerSens: fix disableForInterval Bug
  - bugfix:  88_HMCCU.pm: fixed attribute substexcl
  - update:  88_HMCCU.pm: new version 3.7
  - bugfix:  contrib/Widgets/DateTimePicker/fhemweb_datetime.js:
             - added set parameter to ID to differentiate datetime widgets
  - new   :  74_XiaomiFlowerSens, to retrieves data from a Xiaomi Flower Monito
  - update:  73_NUKIBridge, 74_NUKIDevice
             set Commands are filtered by Attributs,better check alive function
             Callback/Webhook support for software bridge
  - bugfix:  93_DbLog.pm: is now version 2.8.8, no dropdown list in SVG in
                          asynchronous mode, minor fixes
  - feature: 20_ROOMMATE,20_GUEST: introduce new attribute r*_presenceDevices
                                   to allow easy status synchronisation with
                                   other FHEM devices (e.g. PRESENCE module)
  - bugfix:  93_DbLog.pm: is now version 2.8.6, some small bugfixes
             (thanks a lot to DS_Starter)
  - update:  55_InfoPanel.pm: attribute mobileApp added
                              to support fullscreen experience
  - update:  98_cloneDummy.pm
             changed: do not use NOTIFYDEV
             fixed:   set $rval in _state instead of $reading
             added:   new attribute deleteBeforeUpdate
  - bugfix:  73_NUKIBridge/74_NUKIDevice fix lockState with App Bridge
  - bugfix:  14_CUL_TCM97001: fix KW9010 sensor
  - feature: 70_Pushover: add new msg set syntax and introduce
                          Apple Watch glance support
  - change:  70_Pushover: old msg set syntax was declared as being deprecated.
  - feature: 93_DbLog: can now working in  async mode (thanks to DS_Starter)
  - new:     19_VBUSIF: new Device to connect an RESOL VBUS Device
  - new:     21_VBUSDEV: new locical Device to connect to different
             Resol and compatible VBUS Devices via VBUSIF.pm
  - bugfix:  73_GasCalculator: Reset for calendar year fixed
  - bugfix:  73_ElectricityCalculator: Reset for calendar year fixed
  - bugfix:  14_CUL_TCM97001: fix HH humidy for GT_WT_02
  - feature: 57_Calender: new attribute SSLVerify
  - feature: 00_MQTT: Added username password (optional).
  - feature: 41_OREGON: support event-min-interval, event-on-change-reading,
                        etc. Changed module to new log function
                        added support for THWR800 and RTHN318 sensors
  - bugfix:  41_OREGON: fixed return type to prevent massive logmessages
                        fixed THN132N message length
  - feature: 71_YAMAHA_AVR: support for dsp/straight command/reading for
             DSP-Z based models (thanks to dev0) and RX-Vx67 series
  - feature: 10_SOMFY: new RTS commands 0x9 und 0xA (set wind_sun_9/wind_only_a
  - bugfix:  93_DbRep: importFromFile format problem if UNIT-field wasn't set
  - feature: 98_fhemdebug, to aid "Error: >< no TYPE" debugging.
  - feature: 70_Jabber Added possibility to change componentname via
             attr JabberDomain
  - feature: 93_DbRep: function readingRename added, delEntries is able to
             use SQL-Wildcards in attr reading/device
  - bugfix:  98_Verkehrsinfo.pm: Fix state update, Hessenschau message
  - feature: 50_TelegramBot:  msgForceReply, disable,
                  keyboards in messages, inline keyboards and dialogs
  - bugfix:  74_NUKIDevice: Fix Problem with battery Reading
  - update:  97_TrashCal.pm: fetches shared dates at an public webpage
                of waste disposal
  - bugfix:  73_GasCalculator: Corrected month of annual reading
  - bugfix:  73_ElectricityCalculator: Corrected month of annual reading
  - update:  98_Text2Speech.pm: (thanks to Ellert)
                 * attribute 'playing' will updated only in local mode
                 * in case of abort of blockingfunction, 'playing' is set to 0
                 * Remote mode: if modul 'presence' is in use and TTS-remote
                   host is defined, this info will be used to prevent an
                   waiting state for unavaliable remote Host
                 * new Attribute: TTS_noStatistcsLog to disable logging of
                   usage of cachefiles, please read Commandref carfully!
  - bugfix:  73_GasCalculator: Monthly reading and yearly reading name alingned
  - feature: 98_TRAFFIC: reverse waypoints, integrated map for visualization
  - update:  77_UWZ: New Version 1.4.7 added headlines for weblinks
  - update:  73_NUKIBridge,74_NUKIDevice: New Version 0.4.0
             More Feature get,set ,Callback/Webhook Funktion
  - change:  98_exportdevice: command was deprecated and moved to contrib in
                              favor of FHEMWEB builtin functions
  - bugfix:  93_DbRep: bugfix group by-clause due to incompatible changes made
                       in MyQL 5.7.5 (Forum #msg541103)
  - feature: 66_ECMD, 67_ECMDDevice:
              - if split is used, the strings at which the messages are split
                are still part of the messages
              - no default attributes for requestSeparator and responseSeparato
              - input of raw data as perl-encoded string (for setting
                attributes)
              - be more verbose and explicit at loglevel 5
              - documentation corrected and amended
  - feature: 57_Calendar: BYDAY: recognizes and honors one or several weekdays
                          with and without prefix (e.g. -1SU, 2MO) with MONTHLY
  - bugfix:  contrib/Widgets/DateTimePicker/fhemweb_datetime.js: parameter
             settings fixed -> e.g. defaultTime:21:00
  - bugfix:  88_HMCCU: Fixed memory leak in RPC server
  - feature: 01_FHEMWEB: Dump "Probably associated with" in Raw definition
  - bugfix:  93_DbRep: added balance diff to diffValue, balance diff to next
                       period if value is 0 between two periods with values
                       are set
  - feature: 33_readingsGroup: added sortColumn attribute and <tfoot> special
  - bugfix:  88_HMCCU: Fixed RPC server autostart
  - feature: 98_TRAFFIC: flexible update schedule, travelMode
  - bugfix:  88_HMCCU: Wrong CCUNum
  - bugfix   73_GasCalculator: Corrected hidden power average power readings
  - bugfix:  73_ElectricityCalculator: German commandref corrected
  - feature: 88_HMCCU: Added aggregation rules in version 3.6
  - bugfix:  73_ElectricityCalculator: PowerDayMin not zero as from midnight
  - feature: 73_ElectricityCalculator New Reading: EnergyCostDay
  - bugfix:  10_EQ3BT: better error handling if no notification was received
                       allow multiple gatttools to be executed in parallel
                       remove error reading
                       add errorCounters based on function (update/...)
                         which will be increased if reading from the thermostat
                         fails 30 times for one command
                       remain consumption values after restart
  - feature: 98_BOSEST: support shuffle/repeat
  - bugfix:  98_BOSEST: NEW LIBRARY URI::Escape library required
                        support special characters
                        module didn't work if you had only 1 preset
                        remove unknow event log entry for ping/pong
  - bugfix:  14_CUL_TCM97001: Fix checksum calculation for GT_WT_02
  - change:  10_IT: Implementation for HE800 de-/encoding
                    Implementation for HE800 dimmer
                    Fix wrong return values
  - new:     98_Verkehrsinfo.pm: New module retrieves trafficinformation
  - new:     76_SMAInverter: support for SMA Inverters
  - feature: 37_dash_dhcp: added devAlias attribute
  - update:  74_AMAD: statusRequest every Time
  - change:  93_DbRep: code reviewed, no functional changes
  - change:  93_DbRep: DbRep version as INTERNAL, check if DBI module is
                       installed
  - bugfix:  76_MSGMail: Clean up net::smtp version number before comparison
  - bugix:   14_Hideki:  fixed wrong return in ParseFn (msg533900)
             14_SD_WS:   fixed wrong return in ParseFn (msg533900)
             90_SIGNALduino_un:   fixed wrong return in ParseFn (msg533900)
  - change:  93_DbRep: change of day aggregation
  - bugfix:  93_DbRep: Syntaxerror due to Forum #msg529312
  - bugfix:  74_AMAD: 74_AMADautomagicFlowset_2.6.7.xml fix Problems with zero
                      Global Variables
  - feature: 18_CUL_HOERMANN has toggle. culfw 1.67 needed
  - feature: 98_Hyperion: effects can now be set with additional effect args
                          new set addEffect
                          new attr hyperionCustomEffects
                          new reading effectArgs
  - bugfix:  98_Hyperion: clear is working now
                          effects with dash in name are accepted now
  - change:  93_DbRep: sub diffValue changed due to Forum #msg520154,
                       attr diffAccept added, add diffValue state Warnings due
                       to several situations and generate readings
                       not_enough_data_in_period / diff-overrun_limit
  - change:  YAMAHA_AVR: create events even when current.* readings will be
             set to an empty string. (Forum: #60902)
  - bugfix:  10_ZWave: possible changes for multichannel devices (Forum #50176)
  - new:     39_siri.pm: configuration of fhem/siri integration
             39_alexa.pm: configuration of fhem/alexa integration
  - feature: 30_pilight_contact: new module to handle pilight contact sensors
  - feature: 59_Weather: attribute disable
  - new:     10_EQ3BT: Support EQ3 Bluetooth thermostat
                       define living.thermostat EQ3BT <MAC>
  - updated: 88_HMCCU: New version 3.5
  - feature: 98_weekprofile: create events see help for further information
  - feature: 36_WMBUS: support for Amber Wireless AMB8465-M as IoDev
  - feature: 67_ECMDDevice: new attribute noState
  - bugfix:  02_RSS: make hash reference explicit
  - updated: 74_AMAD: New Version 2.6.6 remove APSSID in define, add Attribut
                      setAPSSID to prevent WLan sleeps, add Attribut
                      setTtsMsgLang set to tts language
  - new:     Unit.pm: adding general (but optional) unit support
                      for FHEM and FHEM modules
  - feature: readingsChange FHEM helper module added
  - changed: 93_DbRep: daylight saving time check improved
  - changed: Pushsafer: added devicename to availableMessages reading name
  - feature: 98_Hyperion: new set toggleMode
                          new attr hyperionToggleModes
                          new german commandref
  - bugfix:  93_DbRep: calc issue due to daylight saving time end (winter time)
  - new:     30_pilight_raw.pm: New Attribut sendCount
  - bugfix: 10_SOMFY: wrong attribute reference ...-up-time-to-close removed
  - new:     42_Nextion.pm: New module to connect Nextion displays
  - changed: YahooWeatherAPI: react on wrong units
  - changed: Pushsafer: optimized picture file error handling
  - new:     59_Wunderground: new weather module to fetch
                              data from Weather Underground
  - bugfix:  50_HP1000: correct default unit for windSpeed/windGust from m/s to
                        km/h and transfer unit conversions to new UConv.pm
  - feature: Pushsafer: new option "picture", "picture2" and "picture3" for
                        "message" set command to send pictures from local
                        filesystem or a IPCAM device. See commandref for detail
  - change:  FB_CALLMONITOR: open TCP connection non-blocking,
                             shutdown connection when disabled
  - bugfix:  73_km200: Experimental keys on scalar is now forbidden
  - feature: 10_SOMFY: positionInverse für homebridge + fixes
  - feature: 50_TelegramBot:  multibot support / markup on send text / msgEdit
  - feature: 93_DbRep: get svrinfo contains SQLite database file size (MB)
  - feature: 93_DbRep: get data of dbstatus, dbvars, tableinfo, svrinfo
                       (database dependend)
  - added:   70_Pushsafer: new module to send push notifications via
             www.pushsafer.com
  - feature: 93_DbRep: allow SQL-Wildcards (% _) in attr reading & attr device
  - bugfix:  49_SSCam: Experimental keys on scalar is now forbidden
                       (Perl >= 5.23) Forum: #msg501709
  - added:   37_dash_dhcp.pm: new module for amazon dash buttons
  - feature: 98_Hyperion: removed attribute hyperionAttrRestore
                          default attributes just being added on define
  - added:   73_NUKIBridge,74_NUKIDevice: New Modules to control Nuki Smartlock
  - feature: 98_Hyperion: new attribute hyperionAttrRestore
                          readings will always be refreshed now
  - feature: 93_DbRep: deviceRename added, new Internal DATABASE,
                       Internal/Attribute ROLE added for Autorename-function
  - bugfix:  93_DbRep: delEntries not running on SQLite
  - added:   74_THINKINGCLEANER: new module to support remote control of
                               Roomba cleaning robots
  - feature: 02_FTUISRV: if and loop constructs added
  - bugfix:  74_AMAD: fix FHEM crash when use AMAD and apptime togehter
  - new:     98_TRAFFIC: provide traffic details with Google Distance API
  - feature: 98_Hyperion: set configFile only available if at least two files
                          are found while get configFiles
                          minor code improvements
  - feature: 50_TelegramBot: urlescaped filenames / location send-receive
                            timeout for send
  - feature: 73_ElectricityCalculator: header and readingFnAttributes added
  - feature: 73_GasCalculator: header and readingFnAttributes added
  - feature: 73_km200: header and readingFnAttributes added
  - feature: 93_DbRep: function minValue added
  - bugfix:  38_netatmo: fix for invalid forecast data crashing FHEM
  - feature: 98_Hyperion: version check for hyperion server
                          required min version of hyperion is now 1.03.2
                          attr hyperionVersionCheck to disable version check
  - bugfix:  95_Dashboard: fix for device specs not working in dashboard any
               more.
  - bugfix:  95_Dashboard: fix for yesterdays commit.
  - feature: readingsGroup: allow grouping of similar readings from one device
  - feature  14_SD_WS09: WH1080 CRC-Berechung angepaßt--> automatische
                         Modelauswahl
  - feature: 00_SIGNALduino: nonblocking communication, improved init
               and keepalive, fixed manchester related stuff, Supports
               Somfy RTS Protocol. Decoding manchester encoded messages
               longer than buffer is now possible.
               new function sendMSG.
               Firwmware updated to 3.3.0, please flash
               supports send command from IT Module.
               Serval new protocols implemented.
  - bufgix:  14_SD_WS09.pm
                WH1080 CRC corrected --> model is selectet per default
  - feature: 98_Dooya: Deatures shutters and blinds with dooya protocol
  - feature: 14_SD_WS_Maverick: Supports Maverick bbq thermometer
  - feature: 14_SD_WS: Multi purpose Module to support various weather sensors.
  - feature: 01_FHEMWEB/Reading: accept Readings in <html> (Forum #58320)
  - bugfix:  95_Dashboard: fixes an issue causing devices with interal attribut
                           group to not appear in the dashboard.
  - bugfix:  93_DbRep: include day before and next in calculation if Timestamp
                       is exactly 'YYYY-MM-DD 00:00:00'
  - feature: 93_DbRep: Internal "LASTCMD" added,
                       new reading background_processing_time,
                       diffValue calculation moved to backgrd to reduce load
  - feature: 93_DbRep: new function importFromFile to import data from file
                       (CSV format)
  - bugfix:  73_ElectricityCalculator: Crash due wrong hash pointer assignment
  - feature: new optional arguments for device creation in  copy command
  - bugfix:  49_SSCam: bugfix of get presets, get patrols of zoom-cams
                       without pan/tilt
  - updated: 74_AMAD: New Version 2.6.3 new Reading userFlowState,
                      new set Command userFlowState, checkAndroidVersion
                      on doNotDisturb Reading
  - change:  suppressReading attribute added for all devices (Forum #57841)
  - bugfix:  88_HMCCU: Fixed CUxD device datapoint handling
  - change:  10_IT: create events during readings update.
                    change logging
                    Add Sensor EV1527
                    Support for SIGNALduino
                    (Forum #52827)
  - change:  88_HMCCU: fixed bug in attribute stripnumber. Added autocreate
  - change:  49_SSCam: internal timer of start-routines optimized
  - bugfix:  88_HMCCUCHN: fixed bug in toggle command
  - bugfix:  88_HMCCUDEV: fixed bug in toggle command
  - bugfix:  98_DLNARenderer: fixed SyncPlay for CaskeId players
  - change:  10_ZWAVE: TRANSMIT_NO_ACK is reading only (Forum #57781)
  - feature: 93_DbRep: new attr readingPreventFromDel to prevent readings from
                       deletion when a new operation starts
  - change:  49_SSCam: attr simu_SVSversion changed, added 407 errorcode msg,
                       external recording changed for SVS 7.2
  - bugfix:  73_ElectricityCalculator: get/set list per device and not global
  - bugfix:  98_DLNARenderer: fix pauseToggle/next/prev (thx@MattG)
  - bugfix:  73_GasCalculator:         get/set list deleted for CounterDevice
  - bugfix:  73_ElectricityCalculator: get/set list deleted for CounterDevice
  - bugfix:  73_km200: Bugfix for double entries in RespondingServices.
  - feature: 73_km200: New service type found: "serviceinfo".
  - added:   HMCCUConf: Interface between FHEM and Homematic CCU2
  - added:   88_HMCCU: Interface between FHEM and Homematic CCU2
  - added:   88_HMCCUCHN: Interface between FHEM and Homematic CCU2
  - added:   88_HMCCUDEV: Interface between FHEM and Homematic CCU2
  - change:  93_DbRep: changed format of diffValue-reading if no value was
                       selected
  - new:     24_TPLinkHS110: Support for TPLink HS100/110 wifi power outlet
  - bugfix:  73_GasCalculator:         get/set list corrected for CounterDevice
  - bugfix:  73_ElectricityCalculator: get/set list corrected for CounterDevice
  - bugfix:  93__DbRep: error in diffValue  if no value was selected
  - feature  93_DbRep: exportToFile to CSV-format, Reading "errortext" added
  - feature: 73_GasCalculator:         System readings are hidden now
  - feature: 73_ElectricityCalculator: System readings are hidden now
  - change:  17_EGPM2LAN: get-commands fixed
  - change:  93_DbRep: plausibility checks of database column character length
  - bugfix:  98_Hyperion: final fix for crash bug
  - bugfix:  74_AMAD: fix usb-ethernet condition in the "Send Data to
                      AMADCommBridge= Flow
  - new:     73_ElectrcityCalculator: Calculates electric energy costs
  - bugfix:  98_Hyperion: refresh of readings duration and priority
                          regex for set blacklevel,gamma,threshold,whitelevel
  - change:  98_Hyperion: renamed reading previous_mode to mode_before_off
  - feature: 98_Hyperion: reading duration now shows remaining duration if set
                          or infinite if not specified
  - updated: 74_AMAD: New Version 2.6.2 CommandRef Update, new set command for
                      media control
  - change:  98_Hyperion: non-blocking server connection
  - feature: 49_SSCam: function get stmUrlPath added, fit to new commandref
                       style, attribute showStmInfoFull added
  - change:  57_CALVIEW: fixed internal timer error
  - change:  38_netatmo: error state, enabled debug logging for verbose 5
  - change:  10_ZWave.pm: change numbers in events (hex -> dec, Forum #56682)
  - added:   98_exportdevice: new command to export device definitions
  - feature: 90_at: computeAfterInit attribute (Forum #56706)
  - change:  93_DbRep: fit to new commandref style
  - bugfix:  20_ROOMMATE,20_GUEST: Fixed wakeuptimer <> at-device sync
  - feature  93_DbRep: current_year_begin, previous_year_begin,
                       current_year_end, previous_year_end added as possible
                       values for timestmp attribute,
                       new attribute timeOlderThan, commandref continued
  - feature: attr global commandref modular, Forum #39854
  - bugfix:  49_SSCam: empty event LastSnapId corrected
  - change:  49_SSCam: Logging of verbose 4 changed
  - change:  10_ZWave.pm: change numbers in events (hex -> dec, Forum #56682)
  - feature: 49_SSCam: new attribute "noQuotesForSID"
  - changed: 49_SSCam: commandref revised, more v4 logging in special case
  - updated: 74_AMAD: New Version 2.6.1 support for more Mediaplayer Readings
                      new error handling for "send data to AMADCommBridge Flow"
  - change:  38_netatmo: status "no data"
  - bugfix:  98_Hyperion: reporting Hyperion as off while clearall is active
  - updated: 74_AMAD: New Minor Release 2.6 new 2 Media Readings,
                      new trigger for Mediastate MUST INSTALL AUTOMAGIC 1.31.0
                      fix fix Issues 480148
  - bugfix:  38_netatmo: forecast data check
  - bugfix:  73_km200.pm: Bugfix for uninitialized values
  - feature: 73_GasCalculator: New Readings "EnergyXLast" and "EnergyCostXLast"
  - changed: 98_Hyperion: introducing new attribute hyperionNoSudo
  - changed: 38_netatmo: removed event-on-change default, min HOME interval
  - changed: 93_DbRep: usage of "insert" changed, pls. refer to commandref
  - changed: 93_DbRep: function "insert" added, check of numeric value type
             in functions maxvalue, diffvalue
  - added:   98_Hyperion: initial release of completely new module
  - feature: 10_OWServer/11_OWDevice: new device DS2433 4kbit 1-Wire RAM
  - updated: 77_UWZ: New Release 2.4
    bugfix:  77_UWZ: Perl warnings uninitialized value fixed
  - updated: 77_UWZ: New Release 2.4.5
                     new Attribut's sort_readings_by,htmlsequence
                     new Readings Warn_X_Creation(_*), WarnUWZLevel,
                                  WarnUWZLevel_Color,WarnUWZLevel_Str
  - feature: 44_TEK603: added usable level in percent
  - added:   38_netatmo: exchanged for completely new module
  - feature: 98_DLNARenderer: Support players which require DIDL-Lite
  - bugfix:  73_km200: Bugfix for double and triple downloads
  - feature: 73_km200: DbLog_splitFn implemented
  - bugfix:  74_AMAD: fix Issues 475717
  - feature: 77_UWZ: added lang attribute
  - feature: 98_rssFeed: optionally create events for all readings
  - bugfix:  77_UWZ: fix Issues 472183 and 473982
  - updated: 77_UWZ: New Minor Release 1.4 multi languarge support, more Maps,
                     Routine for search AreaID
  - updated: 74_AMAD: transmissionERROR Reading only expertMode is set
  - changed: 57_CALVIEW: value test, thx klausw
  - added:   98_DLNARenderer: Autodiscover, control and receive events from
             DLNA MediaRenderer devices
               define dlnasearch DLNARenderer
  - added:   98_BOSEST: Autodiscover, control and receive events from
             BOSE SoundTouch devices (e.g. BOSE SoundTouch 10, 20, 30)
             See commandref for library dependencies
               define bosesystem BOSEST
  - added:   77_SMASTP: Support for SMA Sunny Tripower Inverter
  - added:   77_SMAEM: Support for SMA Energy Meter
  - added:   00_HMUARTLGW: new module for eQ-3 HomeMatic UART/LanGateway
  - change:  93_DbRep:  function "diffValue" added, readingnames changed to
             ensure valid reading order, write "-" for reading-value if no
             dataset is found in selection timerange
  - updated: 74_AMAD: New Minor Release 2.4 new AMADCommBridge API
  - changed: 10_ZWave: alarm Events text changed, comma replaced, Forum #53389
  - feature: 93_DbRep: new module added - reporting of database content
             written by DbLog, see commandref for details
  - feature: new module added: 52_I2C_SHT3x.pm (macs)
  - bugfix:  70_Jabber: log OTR empty message if debug-mode == 1 only
  - changed: 70_BRAVIA: re-worked state handling
  - feature: PRESENCE: new attribute presenceThreshold to define a number of
             checks that have to result in "present" before the state of
             PRESENCE is changed to present. See commandref for details.
  - feature: colorpicker: new modes HSV and HSVp
  - bugfix:  PRESENCE: fix generating readings when definition is disabled
  - changed: 49_SSCam: Workaround for problems with SVS version 7.2
             concerning start recording and PTZ-actions,
             new attribute "showPassInLog" added, see commandref
  - feature: 30_pilight_smoke: new module - represent a pilight smoke detector
  - bugfix:  73_GasCalculator: Bugfix for "Can't use an undefined value..."
  - bugfix:  10_pilight_ctrl: Experimental splice on scalar is now forbidden.
  - feature: 73_GasCalculator: "set" and "get" - command in GUI implemented.
  - bugfix:  50_TelegramBot: Unicode / Umlaute handling reworked
  - changed: 30_MilightBridge: Specify port in define
  - changed: 31_HUEDevice: allow toggle command for unreachble devices
             new ignoreReachable attribute
  - update:  77_UWZ: New Minor Release 1.2 Support for United Kingdom
  - feature: 74_AMAD: add Conditionsupport for older Androisversions
                      (Kreidezeit)
  - bugfix:  73_GasCalculator: Unknown "?"-reading no longer created.
  - feature: 74_AMAD: battery_temperature formated
  - bugfix:  74_AMAD: deviceState timestamp bugfix for usb-ethernet Devices
  - feature: 74_AMAD: more better method for wlan keep alive, new Readings
                      for battery live state
  - bugfix:  73_km200.pm: Bugfix for set command with switchprograms
  - feature: 73_GasCalculator: set command finaly implemented. :-)
  - changed: 30_LIGHTIFY.pm: added disabledForIntervals
             added bridge goToScene and setSoftOn/setSoftOff commands
             added device rename command
  - changed: 30_HUEBridge: added disabledForIntervals, added lastError,
              use state/stateFormat instead of STATE
  - feature: PRESENCE: added lepresenced to commandref (by PatrickR)
  - feature: PRESENCE: new attribute bluetooth_hci_device to select a
             specific bluetooth sender for presence checking
             (only for mode "local-bluetooth")
  - feature: 74_AMAD: new Feature added support for do not Disturb Mode
  - bugfix : 74_HOMBOT: check path for sshpass
  - feature: fhem_codemirror: Added new codemirrorParams:
                              keyMap, jumpToLine, jumpToLine_extraKey
  - feature: 10_pilight_ctrl: NEW: protocol oregon_21 for temperature
  - deleted: 52_I2C_GY30_BH1750FVI: Arno Augustin hatte fast zeitgleich
             eine  technisch bessere Variante entwickelt. Diese ist
             nicht mehr notwendig
  - updated: 52_I2C_HDC1008: Umbau auf asynchrones I2C lesen,
             alle sleeps entfernt
  - feature: 74_AMAD: new Feature change current volume + or - value
                      set TABLET volume -5
  - updated: 74_AMAD: New Minor Release 2.2 real state for deviceState Reading,
                      Support for Amazon Music Player and Spotify Player, Keep
                      Alive funktion for Android 6
  - bugfix: 77_UWZ: Commandref Warn Type 7 and 6 exchanged, new method for no
                    eperimental warnings
  - feature: plex: play command now handles single media items, music albums
             and playlists. playAlbum command removed. (by Risiko)
  - added:   52_I2C_BH1750: modul for i2c BH1750 light sensor
  - bugfix:  50_TelegramBot: captions for Images / special chars in Contacts
  - feature: YAMAHA_AVR: new set command presetUp and presetDown for preset
             selection in the current input
  - added:   52_I2C_GY30_BH1750FVI: modul i2c light intensity sensor
  - added:   52_I2C_HDC1008: modul for i2c humidity and temperature sensor
  - bugfix:  FB_CALLLIST: fixing double space in certain call state values.
             PLEASE CHECK YOUR CONFIGURATION (notify, DOIF, FTUI, etc.) after
             this update!!!
  - added:   71_ONKYO_AVR_ZONE: separate module for ONKYO_AVR zones;
             any existing ONKYO_AVR devices used for zoning need to to
             redefined manually by a ONKYO_AVR_ZONE device
  - change:  70_ONKYO_AVR: rewrite based on IODev
  - feature: configDB: new command 'configdb dump' added.
             currently only supported for sqlite!
  - bugfix:  FB_CALLLIST: fix not working calllist when renaming the
             configured FB_CALLMONITOR definition.
  - feature: 10_SOMFY : Added readingFnAttributes
  - bugfix:  FB_CALLLIST: no reading update when list becomes empty
  - feature: added new module 37_plex.pm
  - feature: FBAHAHTTP module as replacement for the deprecated FBAHA
  - feature: 50_TelegramBot reply set command / allowedCommands as restriction
  - change:  49_SSCam: get "snapfileinfo" will get back an Infomessage if
                       Reading "LastSnapId" isn't available
  - feature: dummy attribute useSetExtensions
  - change:  speedtest: create readings without units
  - feature: HUEBridge,HUEDevice,LightScene: use new HUE scenes api
  - feature: 74:AMAD: add Attribut for TTS speed and notify file path
  - bugfix : 74:AMAD: modify informationsflow
  - feature: 00_ZWDongle: add backupCreate / backupRestore
  - bugfix:  49_SSCam: module will not load due to Unknown warnings category
                       'experimental' when using an older perl version
  - feature: 71_PHILIPS_AUDIO : Added input support for AW9000
  - bugfix:  50_TelegramBot: contact handling failed (/ in contact names ??)
  - feature: new module 02_FTUISRV.pm for server side templates for tablet UI
  - feature: 30_pilight_switch: new attribute 'sendCount' to send the
             command n times.
  - feature: 98_rssFeed: creating some readings containing ticker data.
             This can be enabled via new attribute rfDisplayTickerReadings.
  - change:  FB_CALLLIST: delete also corresponding readings if a call gets
             deleted
  - feature: 49_SSCam: Attribute "disable" to deactivate the module added
  - bugfix:  14_CUL_TCM97001: Fix battery bits.
             Fix Auriol receive
  - feature: 50_TelegramBot  supergroup support description for favorites
                             text customization for response messages
  - feature: 49_SSCam: motion detection parameters can be entered if
                       motion detection by camera or by SVS is used
  - feature: 74_AMAD: Flowinstaller and FlowsetUpdater - Support for older
                      Androidversions
  - change:  59_Weather: included caching in YahooWeatherAPI
  - change:  49_SSCam: behavior of "set ... on" changed, Attr "recextend" added
             please have a look at commandref and Wiki
  - bugfix:  49_SSCam: setstate-warning if FHEM is restarted and SVS not
             reachable (Forum: #308)
  - bugfix:  userReadings trigger is always $ terminated (Forum #52165)
  - bugfix:  74_AMAD: fix checkActivTask
  - bugfix:  74_AMAD: fix Commandref, APSSID for non WLAN Devices
  - change:  YAMAHA_AVR: removed set command tunerPreset,
             added new set command preset to select a configured preset for
             the currently selected input. Please change your configuration
             to new command if you use tunerPreset in notify/at definitions
  - feature: PRESENCE: new attribute absenceThreshold to define a number of
             checks that have to result in "absent" before the state of
             PRESENCE is changed to absent. See commandref for details.
  - bugfix:  PRESENCE: new collectord script and .deb package fixing not
             working statusRequest when a room in collectord is disconnected
  - updated: 74_AMAD: New Minor Release 2.0 Please read the Wiki or Commandref
                      !!! ATTENTION !!! Modify Definition is necessary
  - feature: 77_UWZ: new Modules to receive Information about Unwetterwarnung
  - bugfix:  49_SSCam: command check for set cmd's don't work completely
  - feature: FHEMWEB Event-Monitor: stops autoscroll when user scrolls
             manually. If user scrolls to the bottom end, autoscroll continues.
  - feature: perlSyntaxCheck global attribute (currently used by notify & at)
  - bugfix:  31_MilightDevice: Fixed incompatibility with Color::rgb2hsv
  - feature: new module 37_fakeRoku.pm to control fhem from a harmony hub
  - feature: new module 52_I2C_MMA845X.pm added
  - change:  49_SSCAM: change to new RemoveInternalTimer for functions
  - feature: new module 52_I2C_K30.pm added
  - bugfix:  98_weekprofile: send reference profile to device
  - feature: 10_pilight_ctrl | 30_pilight_switch: support protocol daycom
  - feature: 59_Weather: rewritten to use JSON API
  - bugfix:  49_SSCAM: "link_open" doesn't work after last update
  - added:   70_BRAVIA: new module for Sony Televisions
  - feature: 98_statistics: attr specialDeltaPeriod (new) enhanced for more
             than one value and different periods
  - bugfix:  00_SIGNALduino: Replaced firmware with an old one.
  - feature: 49_SSCAM: add "lastrec","lastrec_open" to playback last recording
  - change:  49_SSCAM: "ptzlistpresets" - "id" changed to "position" according
             to Synology-ticket,
             run "geteventlist" automatically after recording-stop,
             delay of InternalTimer(s) changed
  - feature: 71_PHILIPS_AUDIO Improved usability. New preset/fav attributes.
  - bugfix:  71_YAMAHA_NP Minor code correction
  - bugfix: SYSMON: attribute disable does not work properly
  - fixed:   10_pilight_ctrl send long raw codes
  - fixed:   98_weekprofile fix mutated vowels
  - feature: 50_TelegramBot  new option to retry for send &
                             confirmation dialog for favorites
  - fixed:   configDB.pm - fix filelist problem on perl >= 5.20
  - fixed:   configDB.pm - add modpath evaluation
  - feature  71_PHILIPS_AUDIO Added model attribute
  - feature  71_YAMAHA_NP Added model attribute
  - feature  71_YAMAHA_NP: Smooth volume change added. General code cleanup
  - change:  49_SSCAM: routine "initonboot" changed
  - bugfix:  49_SSCAM: default recordtime 15 s is used if attribute "rectime"
             is set to "0"
  - bugfix:  YAMAHA_AVR: fix not working navigateListMenu under certain
             circumstances
  - feature  73_GasCalculator: Last Day/Month/Year/Meter - readings implemented
  - feature  49_SSCAM: command "extevent" added
  - bugfix:  10_SOMFY: removed "setlist" (obsolete) and updated loglevels
  - bugfix   49_SSCAM: "uninitialized value $lastrecstarttime",
             "uninitialized value $lastrecstoptime"
  - feature  49_SSCAM: new attribute "videofolderMap", see commandref
  - feature  31_MilightDevice: added white "hsv" transitions, fixed RGB
  - feature  49_SSCAM: Reading "CamLastRec" added which contains Path/name
             of last recording
  - feature: FB_CALLLIST: new attribute "expire-calls-after" to automatically
             delete call entries after a certain time frame. See commandref
             for details and syntax.
  - feature: FB_CALLLIST: new reading "numberOfCalls" which shows the number
             of shown call entries.
  - bugfix:  00_SIGNALduino: updated firmware to 3.2.0-hf1
                             solves MU and MC issue
  - bugfix:  PRESENCE/presenced: fixed crash of presenced when receiving an
             invalid command, new deb packages released (see commandref)
  - bugfix:  44_TEK603: Fixed TankLevel=NO_DATA
  - feature: LGTV_IP12: new reading "power"
  - change:  LGTV_IP12: changed values of mute reading from true/false to on/of
  - bugfix:  30_MilightBridge: suppress protocol change message on startup
  - bugfix:  74_Unifi.pm: Changed unsupported character for AP and UC readings
                          from hash to hyphen.
  - feature  49_SSCAM: enhanced command runView by option "link_open" to
             open a streamlink immediately
  - feature: new module LGTV_IP12 for controlling LG SmartTV's manufactured
             between 2012-2014 via network connection
  - feature: 30_MilightBridge: Support tcp bridge.
  - bugfix:  30_MilightBridge/98_ping: Use Blocking.pm for ping checks so
             it does not block main thread.
  - feature  49_SSCAM: functions for cam-livestream added
  - bugfix:  73_km200.pm: Bugfix InternalTimer; Improvement Log Level
  - bugfix:  pre-coomit-hook test
  - bugfix:  98_weekprofile: detect channel of HM-CC-TC as correct thermostat
  - bugfix:  00_SIGNALduino: Version 3.2.0 Module & Firmware
             serval fixes and enhacements, improved stability, supports many
             new protocols, ITv3 sockets and switches, new sendMsg Function.
             You need to flash your SIGNALduino with the new firmware.
  - bugfix:  14_Hideki: support rain sensors
  - bugfix:  14_SD_WS07: Fixed some wordings
  - feature: 14_SD_WS09  Module for WH1080
             (WS-0101, TFA30.3189) & CTW600 868MHz OOK/AS
  - feature: TimeSeries: median, holdtime for event-aggregator
  - feature: 57_CALVIEW: added internal notify-fn for calendar-devices,
             added attr disable for internal notify-fn, removed ts state and
             started_* reading, removed old mode-attributes /def modes,
             changed commandref
  - bugfix:  49_SSCam: fixed a problem that the state is "disable" instead of
             "disabled" if a camera is disabled and FHEM will be restarted
  - feature: 98_weekprofile: attribute widgetEditDaysInRow to control visible
             days in one row
  - feature: 49_SSCAM: function "get ... eventlist" added, Reading CamEventNum
             added which containes total number of camera events, change usage
             of reading "LastUpdateTime"
  - added:   79_BDKM: new module for Buderus KM Gateways
  - feature: 57_Calendar: get ... uid ...
  - feature  49_SSCAM: function "runPatrol" added that starts predefined
             patrols of PTZ-cameras, Reading "CamDetMotSc" added
  - feature: LightScene: added nextScene and previousScene commands
  - feature  49_SSCAM: Reading "CamExposureControl" added
  - feature  49_SSCAM: set up of motion detection source now possible
  - feature  55_GDS: disable conditions after 15.03.2016
  - feature  74_HOMBOT: formated Value for Reading lastClean
  - feature  74_HOMBOT: include Detail_Fn link to Luigi Contro Center
  - feature  49_SSCAM: control of exposure mode day, night & auto
  - bugfix:  74_HOMBOT: some set commands not work
  - feature: 32_mailcheck: added set active/inactive commands
  - feature: 02_RSS: new attribute urlOverride
  - feature: 71_YAMAHA_NP: Added auto reading update for tuner and player
  - feature  49_SSCAM: The port in DEF-String is optional
  - bugfix:  98_weekprofile: transfer day settings to other days
  - bugfix:  49_SSCAM: fixed a problem that manual updates using
             "getcaminfoall" are leading to additional pollingloops if polling
             is used, attribute "debugactivetoken" added for debugging-use
  - feature: version: version command shows latest revision since last update
  - feature: 02_RSS: new attribute itemtitle
  - bugfix:  57_Calendar: weekly recurring events on several weekdays, that
             start around midnight
  - bugfix   49_SSCAM: fixed a problem that a usersession won't be destroyed
             if a function couldn't be executed successfully
  - bugfix:  95_Dashboard: fixed javascript error because of changes in fhemweb
  - feature: 49_SSCAM: feature for retrieval snapfilename added
  - bugfix:  57_Calendar: weekly recurring events on several weekdays,
             missing description
  - feature: 57_Calendar: RDATE enabled
  - bugfix:  49:SSCAM: "goAbsPTZ" may be unavailable on Windows-systems
  - feature  49_SSCAM: added function "move" for continuous PTZ action
  - feature: 02_RSS: continue image update sequence after error (HTML)
  - feature: 98_rssFeed: Possibility to modfy feed data via a custom function.
  - change:  49_SSCAM: entries with loglevl "2" reviewed,changed to loglevl "3"
  - feature: 50_TelegramBot  receive media files, send media files directly
             invocation (PNG, JPG, MP3, PDF, etc) etc (see change log in file)
  - feature: 49_SSCAM: added function "goPreset" and "goAbsPTZ" to control the
             move of PTZ lense, refer to commandref or have a look in forum at:
             forum.fhem.de/index.php/topic,45671.msg404275.html#msg404275 ,
             forum.fhem.de/index.php/topic,45671.msg404892.html#msg404892
  - feature: 98_weekprofile: widget: transfer day settings to other days
  - bugfix:  FB_CALLMONITOR: corrected internal_connection mapping.
             especially FON1-FON3. Please check your configuration.
  - change:  98_weekprofile: return sorted lists
  - change:  YAMAHA_AVR: reading/event newFirmware will only be triggered for
             RX-Vx71, RX-Vx73, RX-Ax10 or RX-Ax20 as newer models do not
             support this information anymore
  - change:  57_Calendar: complete rewrite
             see http://forum.fhem.de/index.php/topic,48315.0.html
  - feature: new events for home automation buttons and unassigned buttons
  - feature: 10_KOPP_FC: added blinds and switches
  - updated: 74_AMAD: New Minor Release 1.2.0
             Do not forget to to update the new Automagic Flowset !!!
  - feature: 74_AMAD: shutdown the Device, activate Airplanemode, control
             Notivicationvolume, vibrates the Device, Locked Device by PIN
  - bugfix:  74_AMAD: modified Error handling, best practice for identify
             offline Mode
  - feature: New module 74_HOMBOT to control LG Hombot vacuum cleaner
  - bugfix:  49_SSCAM: credentials won't be deleted if "rereadcfg" is used
  - bugfix:  76_MSGMail: Make use of attribute mailtype again (enabling html)
  - feature: 49_SSCAM: added function "svsinfo" to get informations about
             installed SVS-package
  - bugfix:  49_SSCAM: saved Credentials were deleted if a device will be
             deleted
  - change:  49_SSCAM: if Availability = "disconnected" then "state"-value
             will be "disconnected" too
  - feature: 70_Pushalot: added support for TimeToLive parameter.
  - bugfix:  60_allergy: fixed invalid readings names
  - bugfix:  73_km200: Little Bugfix with the use around Regular Expressions
  - feature: 91_notify: add readLog attribute
  - feature: 98_ping: Add attribute for minimum fails before reporting
             (minFailCount)
  - bugfix:  PRESENCE: fix log warning "use of uninitialized value ..." when
             using power set command without any argument.
  - added:   60_allergy: Allergy forecast data for Germany
  - feature: FB_CALLLIST: new attribute number-cmd to execute a FHEM command
             when clicking on a external number within the calllist. Can be any
             valid FHEM command or Perl code. For details see commandref
  - change:  49_SSCAM: a little bit code optimization
  - bugfix:  31_MilightDevice: Queue length correction for long transitions
  - feature: 31_MilightDevice: Color changes during dim on lower brightness
  - bugfix:  30_MilightBridge/31_MilightDevice: Variable fallbacks, colorcast
  - bugfix:  44_TEK603: fixed wrong values.
  - bugfix:  49_SSCam: fixed the problem a recording may still stay active if
             fhem will be restarted after a recording was triggered and
             the recordtime wasn't be over,
             Enhancement of readings.
  - change:  76_MSGMail: move email delivery from MSGMail_set to MSGMail_send
             to be usable from perl; use Blocking_Call to deliver email
  - change:  55_GDS.pm uses setKeyValue/getKeyValue for user credentials
  - feature: new module 52_I2C_BME280.pm added (klausw)
  - bugfix:  52_I2C_PCA9685: bugfix for interaction with FRM
  - change:  49_SSCAM: changed DEF in order to remove credentials from string,
             added "set credentials" command to save username/password,
             added Attribute "session" to make login-session selectable,
             NOTE: You have to adapt your define-strings after update !!
             look at commandref or forum-post for details:
             forum.fhem.de/index.php/topic,45671.msg397449.html#msg397449
  - bugfix:  73_GasCalculator: Bugfix in Commandref and 2 attributes renamed.
  - feature: 98_weekprofile: including topics\categories
  - change:  98_weekprofile: filter for homatic channel devices
  - feature: YAMAHA_BD: input reading indicates now Netflix, YouTube, and all
             other online apps.
  - feature: 73_GasCalculator: New module for calc. around the gas consumption
  - feature: FB_CALLLIST: new attribute "no-table-header" added, to hide the
             table header for the whole list
  - feature: 49_SSCam: Attribute "httptimeout" added
  - feature: update is executed per default in the background
  - bugfix:  FB_CALLLIST: fix "Use of uninitialized value" warnings on startup
  - change:  49_SSCam: Change of define-string related to rectime.
                       Note: see all changes of rectime usage in commandref
                       or in Forum:
                       .../index.php/topic,45671.msg391664.html#msg391664
  - added:   98_count: count devices specified by devspec or all
  - bugfix:  57_CALVIEW: bugfix for started terms
  - feature: 10_KOPP_FC: Receive Mode for dimmer implemented,
    change:  10_KOPP_FC: removed "toggle" command, use "on" or "off" instead
  - change:  49_SSCam: Vars "USERNAME" and "RECTIME" removed from Internals,
                      Var (Internals) "SERVERNAME" changed to "SERVERADDR",
                      minor change of Log messages,
                      Note: use rereadcfg in order to activate the changes
  - feature: version: version command shows also internal helper modules that
                      are loaded (HttpUtils, Blocking, ...)
  - feature: 70_VIERA: Using non blocking for status update.
                       Added color button for remoteControl and SVG layout
                       Some new SVG icons for remoteControl layout
  - change:  73_km200: New attribute "disabled" and default values changed.
  - feature: HUEbridge: added set deletescene and get scenes detail
  - feature: HUEDevice: added (hue|sat|ct)(Up|Down) commands
  - feature: 51_I2C_TSL2561: support non-blocking I2C-IO, especially when
                             using Firmata over LAN
  - feature: FB_CALLLIST: new attribute answMachine-is-missed-call to treat
                          incoming calls, which were taken by an answering
                          machine, as "missed call". Only relevant for
                          list-type "missed-call".
  - change:  FB_CALLMONITOR: reading "missed_call_line" will not be triggered
                             anymore. Use internal_number instead, which
                             contains the same content
  - feature: FB_CALLMONITOR: new attribute answMachine-is-missed-call to
                             treat incoming calls, which were taken by
                             an answering machine, as "missed call"
  - feature: 98_weekprofile: send profile to other weekprofile intance
                             send profile to multible devices
                             multi-select of devices in widget
  - feature: new module 52_I2C_PCA9685.pm added (klausw)
  - change:  98_weekprofile: create default profile if master device
             has no week profile
  - bugfix:  allowed without a validFor is invalid.
  - feature: 98_weekprofile: detect profile changes in master device
  - feature: 49_SSCam: Function "Get" for retrieval Camera-Readings added,
                       Attributs pollcaminfoall, pollnologging  added,
                       Function for Polling Cam-Infos added.
  - bugfix:  89_HEATRONIC: fixed variable names
  - feature: 89_HEATRONIC: new reading ch_error: error code of boiler
  - change:  SYSMON: end of support for barcharts
  - fix:     SYSMON: html
  - feature: 98_weekprofile: new attribute 'widgetEditOnNewPage' to edit
             weekprofile on new web page
  - change:  89_HEATRONIC: new feature: set heating mode, set temperature
             new reading ch_code
  - bugfix:  FB_CALLMONITOR: empty phonebooks will be recognized correctly,
             phonebook processing continues, when error occurs
  - change:  FB_CALLMONITOR:  attr fritzbox-remote-phonebook-exclude allows
             phonebook names additional to ID's
  - bugfix:  95_Dashboard: fixed issue when using cmdIcon attribute
                           for devices.
  - feature: 71_PHILIPS_AUDIO: select presets and favorites by name.
  - feature: 50_TelegramBot: alias for commands, new readings,
                             support for sending media files; plus fixes
  - feature: 20_ROOMMATE,
             20_GUEST: new attribute r*_geofenceUUIDs for direct GEOFANCY
                       support as an alternative for notify/DOIF/watchdog
                       clutter
  - change:  98_GEOFANCY: attribute devAlias is now mandatory to have all
                          readings created (improves security/stability)
  - feature: configDB: rescue mode added, read forum #46538
  - changed: 49_SSCam: documentation changed
             HINT: use IP-Adresses instead of hostnames in SSCAM-Define!
  - bugfix:  FB_CALLLIST: fix not working longpoll update in FHEMWEB
  - change:  FB_CALLLIST: saved list will be deleted from filesystem
              when delete <name> is executed
  - feature: allowed module added. allowedCommands, basicAuth, password,
             globalpassword attributes moved to this module.
  - bugfix:  YAMAHA_AVR: fixing not working volumeStraight set command
  - change:  FB_CALLLIST: start call processing only when "event:" is triggered
             by corresponding FB_CALLMONITOR device.
  - change:  FB_CALLMONITOR: default value for attr
             fritzbox-remote-phonebook-via has been changed to "tr064"
             (previous: "web") to ensure no problems with new Fritz!OS web
             layout.  Besides TR-064 is official supported by AVM.
  - feature: PHILIPS_AUDIO: Favorite station selection
  - feature: YAMAHA_AVR: new set commands and readings for tuner control
             - new set commands tunerFrequency,tunerPreset for
               controlling tuner frequencies and selecting presets.
             - new readings tunerFrequency,tunerFrequencyBand,
               currentStationFrequency
             - see commandref for details
  - bugfix:  51_I2C_TSL2561: correct lux calculation floatArithmetics case
  - feature: YAMAHA_AVR: add pointer to main zone in Internals for zone defs
  - change:  YAMAHA_AVR: DSP based models use command queue of main zone
             to execute commands for zone definitions
             (many thanks to dev0 for patience and support)
  - bugfix:  YAMAHA_AVR: fix navigateListMenu for RX-Vx71 series models,
             fix bass/treble missbehaviour for DSP based models
  - feature: 98_weekprofile: new module to manage week profiles
  - feature: 49_SSCam: function "enable" and "disable" for SS-Cams added
  - change:  49_SSCam: changed timout of Http-calls to a higher value,
                       commandref enhanced
  - feature: 57_CALVIEW.pm: added new function for running terms
  - change:  57_CALVIEW.pm: improved commandref
  - feature: 98_update.pm: support multiple repositories (Forum #45121)
  - change:  71_YAMAHA_NP: More secure FM frequency input
  - feature: FHEMWEB/Event Monitor: optional FHEM Log monitor.
  - feature: 50_Telegrambot: multiple contacts for send etc/removed depreacted
      messageTo,sendImageTo,sendPhotoTo/allowunknowncontacts
  - bugfix:  70_PushNotifier: remove messages fron FHEM-logfile
  - feature: 49_SSCam: function "snap" for taking snapshots added,
  - bugfix:  49_SSCam: fixed a bug that functions may impact each other
  - feature: 31_MilightDevice: Add restoreAtStart attribute so group devices
      (slot 'A') do not restore state by default at startup
  - bugfix: 30_MilightBridge/31_MilightDevice: Fix startup restore.  Fix crash
      on invalid hostname.
  - feature: YAMAHA_NP: Direct FM frequency setting.
  - feature: 30_pilight_xyz: possibility to change IO-Device (IODEV)
  - bugfix: YAMAHA_AVR: fixing not correctly volume smoothing
  - change: 49_SSCam: turned completly to HttpUtils_NonblockingGet for
                       calling websites nonblocking,
                       LWP is not needed anymore,
                       use of InternalTimer instead of fhem(sleep),
                       improve usage of verbose-modes
  - change:  10_RESIDENTS.pm: Readings residentsTotalOwners* were renamed to
                              residentsTotalRoommates*
  - feature: CUL_MAX: allow multiple instances
             Make sure that you set attr IODev on each MAX device
             (pointing to its CUL_MAX) and set attr IODev on each CUL_MAX
             (pointing to its CUL).
  - feature: YAMAHA_AVR: several new features:
             - new set command navigateMenuList for automatic menu navigation
             - new set command/reading partyMode
             - disabledForInterval attribute added
             see details in commandref
  - change: YAMAHA AVR: optimized HTTP request command queue to allow
            correct processing of concatenated set commands
            (no sleep commands neccesary anymore)
  - bugfix: 95_Dashboard: fixed local link in command ref
  - bugfix: 10_IT: Ignore sending if dummy (Forum ID 44990)
    feature: 10_IT: Add functionality for setting ITClock (Forum ID 44451)
  - bugfix: 14_CUL_TCM97001: Fix creation of plots
  - updated: 74_AMAD: New Mijor Release 1.0.0
                      Add Reading Android Version
                      Add VoiceInput fo VoiceCommands
                      Bug Fixes
                      Call ReadingsVal from Automagic HTTP Request with Respons
  - feature: 89_rssFeed: New module to get data from rss news feeds
  - feature: FB_CALLMONITOR: added attribute disabledForIntervals to specify
             specific time ranges, where FB_CALLMONITOR will be disabled
             (see commandref for the exact syntax)
  - changed: YAMAHA_AVR: added HTTP request queue, send only one request at the
             same time. This increases command reliability and response
             behaviour of the AV receiver.
  - bugfix:  49_SSCam: avoid problems when running this module on
             windows systems
  - feature: 14_CUL_TCM97001: Add redirect for Eurochron to SD_WS07 modul
                              Add support for KW9010 sensor
                              Change autocreate names
  - feature: 14_CUL_REDIRECT: Add redirect for Oregon 3 protocol
  - bugfix:  49_SSCam: avoid possible blocking situation of FHEM when a
             recording is running
  - bugfix:  49_SSCam: avoid messages "insufficient user privilege" even
             though the user was set up properly
  - bugfix:  70_PIONEERAVR: suppressed Smartmatch is experimental warnings
  - feature: 30_pilight_temp add attributes offsetTemp and offsetHumidity to
             correct temperature and humidity
  - changed: PRESENCE/collectord: new collectord-1.5.deb package released
  - changed: YAMAHA_BD: added HTTP request queue, send only one request at the
             same time. This increases command reliability and response
             behaviour of the player.
  - changed: 55_GDS.pm: provide gdsAlertsHeadlines() instead of gdsHeadlines
  - feature: TelegramBot: multiple enhancements and fixes V1.1 keyboards on
             favorites and last command reduced logging:
             pollingVerbose:0_None,1_Digest,2_Log yowsup compatibility commands
             added writeStatefile on contact change cmdReturnEmptyResult - to
             suppress empty results from command execution and more
  - feature: 55_GDS: new command get <name> headlines [separator]
  - bugfix:  YAMAHA_BD: fix power off events when player is turned on
             via set command on
  - bugfix:  95_Dashboard: fixed javascript bug causing tabs not to load
  - feature: 36_DavisVantage.zip (author: "habeIchVergessen")
             Receive Davis Vantage Weather Stations with JeeLink
             and the KeyValueProtocol module
  - feature: new module 36_KeyValueProtocol
  - bugfix:  95_Dashboard: the fhem root url is not hardcoded any more
             but read from the $FW_ME variable. Fixed a problem that causes
             drag&drop being still activated when the dashboard was locked.
             (resize/move)
  - bugfix:  14_SD_WS07 - corrected syntax error and raised loglevels
  - bugfix:  55_GDS.pm - correct wrong cumulation in alerts (1st try)
  - feature: new module 10_DUOFERNSTICK and 30_DUOFERN added
  - feature: 59_Weather: prevent retrieval of older forecasts than the
             one previously retrieved
  - IMPORTANT: featurelevel is now 5.7, rendering @ and % non-functional

- 2015-11-15 (5.7)
  - change: 30_MilightBridge/31_MilightDevice: Allow to disable ping check.
                            Add state "Initialized".
  - feature: 50_HP1000: new module to support HP1000 weather station
  - feature: new module 53_GHoma.pm added (klausw)
  - feature: 14_CUL_REDIRECT: Rename 14_CUL_OTHER to 14_CUL_REDIRECT
  - bugfix:  00_SIGNALduino:
              Firmware Update 3.1.8-HF2 fixes a possible crash
              Fixes missing event when DMSG is updated
  - feature: 02_RSS: new attribute noscroll
  - feature: 98_help: replace anchor links in help output with a working
                      link to local commandref or fhem.de
  - bugfix:  70_XBMC: reworked RPC ID generation
  - feature: 70_XBMC: added openchannelid to switch TV channels
  - bugfix:  74_AMAD: Bessere Variante zur HTTP Headeranalyse, Code cleanup
  - bugfix:  74_AMAD: AMADCommBridge communication problem with automagic 1.29
  - feature: fhem_codemirror: Added DOIF autocomplete-keywords. Added feature
                              to autocomplete on any keypress.
  - change:  ATTENTION: Removed deprecated module 75_MSG.pm. Users will need to
             manually change their device definitions to MSGFile or MSGMail
             respectively.
  - feature: Introduce FHEM message routing by new command 'msg'
  - bugfix:  98_Text2Speech: Google fixed, svox-pico added
  - bugfix:  00_SIGNALduino: Updated Firmware (3.8.1-HF1)
             fixed send raw
  - updated: 74_AMAD: New Mijor Release 0.8.1
  - bugfix:  74_AMAD: fix call statusRequest then screen off is set
                      fix change room then device modify
  - feature: 74_AMAD: insert first code parts of voice input
  - change:  55_GDS.pm new version released, see forum Announcements
  - change:  fhem_codemirror.js: Enabled indentWithTabs by default
                                 Enabled autoCloseBrackets by default
                                 Disabled smartIndent by default
  - bugfix:  74_AMAD: wrong flowset xml file on lib/
  - updated: 74_AMAD: New Major Release 0.8.0
                      !!! IMPORTANT: please forget to update the Flowset !!!
  - feature: 74_AMAD: AMADCommBridge (AMADCommunication Device)
                      toggle between to BT Devices, clear Notificationbar
                      (Automagic,All), play Notify Soundfile (WallClock),
                      check for a activ task on the tablet/phone
  - bugfix:  74_AMAD:  improved error handling
  - bugfix:  70_PIONEERAVR: fixed the decoding for the reading "display".
  - feature: 93_DbLog: Added support for longpoll SVG.
  - feature: contrib/98_openweathermap.pm - add support for stationByZip.
             e.g. 76133,de will find weather data for Karlsruhe,Germany
  - bugfix:  38_CO20: fixed error messages on timeout
  - feature: codemirror modules now loaded by default: search.js, comment.js
                 dialog.js, autorefresh.js, searchcursor.js, dialog.css
             codemirror search & replace is now activated by default.
                 to use this feature now you must only load in fhemweb
                 attribute 'JavaScripts' the codemirror/fhem_codemirror.js file
             new extraKeys for 'TAB', 'Shift+Tab', 'STRG+Q', 'STRG+UP',
                 and 'STRG+DOWN' are added.
             codemirror default parameters are now:
                 indentUnit:4, indentWithTabs:false, autoCloseBrackets:false,
                 matchBrackets:true, autofocus:true, theme:"blackboard",
                 lineNumbers:true, autoRefresh:true
               this can be overwritten with fhemweb attribute 'codemirrorParam'
  - updated: codemirror version to 5.8
             the default codemirror javascript files are now minified
  - feature: 70_XBMC: -added disable attribute
                      -added reading tvshowid
  - feature: new module 00_SIGNALduino.pm and 90_SIGNALduino_un: added
             SIGNALduino module and firmware
  - feature: new module 14_Hideki.pm: added module for sensors with hideki
             protocol
  - feature: new module 14_SD_WS07.pm: added module for sensor devices with
             protocol id7
  - feature: 32_yowsup.pm: allow comma separated receiver list on master send
  - bugfix:  YAMAHA_AVR: fixing not working remoteControl commands for
             several models
  - feature: PRESENCE: support for Solaris ping (mode: lan-ping)
  - feature: HUEbridge: added support for HUE scenes
             (get: scenes; set: savescene, modifyscene, scene)
             new unified syntax for multiple lights
             in group and scene commands
             don't query status after set: use bridge response instead
             added queryAfterSet attribute
  - feature: HUEDevice: added support for HUE scenes (set: savescene, scene)
             new unified syntax for multiple lights in lights command
  - feature: LightScene: support HUE scenes
                         added asyncDelay attribute
  - bugfix:  10_IT: Fix wrong V3 dimm/off code
  - feature: 73_km200: Improving error message in state
  - feature: SYSMON: FormatString for SYSMON_ShowValues.
  - feature: 36_JeeLink: added timeout attribute (by HCS)
  - change: 14_CUL_TCM: implement new sensor types. Fix some wrong
                        interpretations. Add additional readings.
  - feature: on/off-till-overnight (SetExtensions.pm)
  - bugfix:  73_km200: Bugfix for freeze in "Sounding"
  - change:  93_DbLog: changed min/max val 999999 to system specific (~0 >> 1)
  - feature: HUEbridge: added get touchlink
                        added get whitelist, set deletewhitelist
                        new and extendet internals
  - feature: HUEDevice: dimUp&dimDown: use bri_inc if bridge firmware >= 1.7
                        don't send on with dimUp & dimDown if already on
                        new and extendet internals
  - feature: 71_YAMAHA_AVR: new set commands/readings for controlling
             bass and treble (by dev0)
  - feature: 66_ECMD: requestSeparator can be turned off
  - feature: 02_RSS: viewport configurable by attribute
  - change:  93_DbLog: removed use of perl's 'switch' feature.
  - change:  93_DbLog: removed string length limitation for SQLITE.
  - bugfix:  93_DbLog: fixed ploteditor bug when DbLogType=History.
  - feature: 93_DbLog: added new setter 'reduceLog' to clean up database.
  - feature: new Modules 36_EleroStick.pm and 36_EleroDrive.pm for Elero
             shutters
  - change:  55_InfoPanel.pm: support ReadingsVal in ticker #35228
  - bugfix:  31_MilightDevice.pm: improved previousState, fixed log errors
  - bugfix:  30_MilightBridge.pm: fixed ping definition
  - bugfix:  95_FLOORPLAN. fixed device-commands and excess logmessages
  - feature: 02_RSS: viewport in HTML header makes page fit screen on tablets
  - bugfix:  74_AMAD: fixed hash->{PORT} in log output
  - bugfix:  70_PushNotifier: - require Try::Tiny
  - feature: 70_Jabber: - Added OTR (Off the Record) end to end encryption
                        - Added MUC (Multi-User-Channel) joining and handling
  - change:  74_AMAD: improved translation englisch
  - bugfix:  95_Dashboard: fixed access to uninitialized value
  - change:  74_AMAD: change set of STATE has been replaced by Readingsupdate
                      'state'
  - feature: 74_AMAD: commandref english translation, insert default version ID
  - feature: SYSMON: telnet login with no user/pass required
  - bugfix:  95_Dashboard: the sort order in columns is now correctly read
               from the sorting attribute.
  - bugfix:  00_MAXLAN: set time on cube if it has none (by Tom_S)
  - bugfix:  14_CUL_MAX: work together with a-culfw
  - bugfix:  70_PushNotifier: bugfix regex deviceID
  - feature: new Module 74_AMAD to request Information and control Android
             Devices in cooperation with AutomagicApp on the Device (Forum
             #39773) (by M. Oldenburg)
  - bugfix:  70_PushNotifier.pm: regex error handling
  - bugfix:  31_MilightDevice.pm: fixed bug that lead to crash on lost bridge
             connection, added module name prefix to round function
  - bugfix:  38_CO20.pm: removed unneccesary error messages due to USB timeout
  - feature: 70_PushNotifier: use regexe for deviceID
  - bugfix:  30_pilight_temp: pressure, windavg, winddir, windgust from weather
             stations without temperature
  - feature: 74_Unifi: - new readings for controller, accesspoints and clients
                       - new Setter: archiveAlerts, disconnectClient, restartAP
                         setLocateAP, unsetLocateAP
                       - new Getter: events, unarchivedAlerts
                       - new Attributes: eventPeriod, httpLoglevel
  - feature: 30_pilight_temp: - Added support for pressure, windavg, winddir,
              windgust from weather stations
  - feature: 98_Text2Speech.pm:
              - Quality and Speed as new Parameter
              - Bugfixing with Google Download
              - added VoiceRSS as new Ressouce
              - TTS_FileTemplateDir: Beginning with absolute directory now
                possible
              - TTS_Timeout (optional) added
  - feature: 74_Unifi: - ReadingNames now by default (in this order):
                         Attr 'devAlias' > controllerAlias > hostname > user_id
                       - Attr 'devAlias' now can rename:
                         controllerAlias, hostname, user_id
                       - Command 'get clientData' can now called with these
                         parameters: devAlias,controllerAlias,hostname,user_id
  - bugfix:  70_Jabber: Fixed broken callback registration in Net::XMPP >= 1.04
  - bugfix:  95_Dashboard: support for alias attribute, which if set, is shown
               instead of the device name in the left navigation
  - feature: 70_Pushover: Rewrite for Non-Blocking HttpUtils
               - much more readings
               - Support for emergency callback via push
               - Support for supplementary URLs incl. push callback (e.g. for
                 priority < 2)
               - Added readingFnAttributes to AttrList
               - Added support for HTML formatted text
               - Added user/group token validation
  - feature: 74_Unifi: - Added Attribute 'devAlias' to rename device names (ID)
                       - bugfix: Module not started without restart after def
  - feature: 74_Unifi: - Added support for Controller v3 (v4 already supported)
  - change:  74_Unifi: - changed get-Name from 'clientDetails' to 'clientData'
                       - changed start from defFn to NotifyFn
                       - added 'get clientData' selection by client-ID
                       - added disable Attribute
                       - updated commandref
  - added:   74_Unifi.pm for the Ubiquiti Networks (UBNT) - Unifi Controller.
  - change:  70_VolumeLink: - Changed vol/mute-RegexPattern modifier to /si
                - Changed default timeout to 0.5
                - Fixed bug while storing RegEx from Attr to hash
                - Added Attribute for separate muteRegexPattern
                - Added Attribute httpNoShutdown
                - Added possibility to disable ampInput check
  - feature: YAMAHA_AVR: new reading "newFirmware" for indicating firmware
             update. new argument "direct" for volume commands to avoid
             volume smoothing (if activated)
  - added:   70_VolumeLink.pm: New module to link the volume-level and
             mute-state from a physical-device (e.g. a TV) with a fhem-device
             (e.g.  a SONOS-Playbar or an AVR).
  - feature: 30_MilightBridge: Add tcpPing mode (MarkusM)
  - change:  98_pilight: all protocols, rewrite
  - feature: 70_PHTV: added support for WoWifi/WoLAN to wake device up
  - change:  98_GEOFANCY: improved/tightened input validation. 3rd party mobile
               apps need to ensure using correct API data format.
  - bugfix:  95_Dashboard: fixed issue with disappearing menu and command input
             in room "Everything"
  - bugfix:  95_Dashboard: fixed problem with smallscreen styles that caused
             devices to be shown in wrong tabs
  - bugfix:  34_NUT: versucht bei disabled=1 nicht mehr, eine Verbindung
             aufzubauen
  - change:  57_CALVIEW: - replace unwanted backslash before a comma sign
  - bugfix:  95_Dashboard: fixed sorting for grouped devices
  - bugfix:  95_Dashboard: fixed style issue with colorpicker in ios6touchpad
             style fixed issue with editing groups in the dashboard
             configuration dialog
  - feature: 30_pilight_dimmer.pm: SetExtensions (on-for-timer, etc.)
  - feature: 30_pilight_switch.pm: SetExtensions (on-for-timer, etc.)
  - feature: 30_pilight_raw.pm: send raw codes to pilight
  - feature: 95_Dashboard: added new attribute dashboard_tabXdevices which
               supports devspec definitions for shown dashboard groups.
               Storage of current opened tab and restore when opening dashboard
               Fixed some CSS issues (text alignment, colors ...)
  - change:  SYSMON: warning (userdefined readings), reading for perl version
  - feature: 38_CO20.pm: added advanced features, retries and timeout (by
             Markus M.)
  - feature: 32_yowsup.pm: added support for groups
  - feature: FB_CALLLIST: new attribute icon-mapping for customizing the icons
             for all call states. For details see commandref
  - bugfix:  73_km200: Removal of Static polling and new sounding after
             attribute change
  - bugfix:  Dashboard: text alignment issue for ios7 style.
  - bugfix:  Dashboard: fixed some perl warnings.
                        smallscreen styles are not destroying view any more..
  - bugfix:  Dashboard: text alignment issue for ios6touchpadstyle.
  - change:  57_CALVIEW: -update fpr modi-management
                        -the modes now can be set with attribute modes
                        -thx to Risiko for patch
  - bugfix:  Dashboard: group names now also can contain regex special
             characters restoring of saved group state works now as expected
             fixed issue that some readingGroups are not updated correcly
  - change:  02_RSS: replaced refresh method by javascript DOM gymnastics
  - change:  59_Weather: removed empty header row from WeatherAsHtmlV
  - feature: 02_HTTPSRV: support tabletui (Forum #37232)
  - bugfix:  SOMFY: Only send stop if position changed
             improved timing for position update fix typos (go-my instead of
             go_my)
  - feature: ios6touchpadstyle: style adjustments for the Dashboard
             module version 3.0
  - bugfix:  10_IT: Correct command parsing (forum id 38467)
  - bugfix:  Dashboard: corrected version number
  - feature: SYSSTAT: added mibs attribute for snmp monitoring
  - bugfix:  Dashboard: fixed CSS height issue for rows (top, center, bottom)
  - feature: FB_CALLLIST: new attribute "external-mapping", new column for
             external_connection reading (see commandref for details, by
             Michael)
  - feature: Dashboard: release version 3.0
  - bugfix: SYSMON: 'disable' not working at FHEM-start
  - bugfix: Text2Speech: ogg/wav as direkt mp3files are now possible
  - bugfix: SOMFY: Added attr "additionalPosReading" to store current position
                   Bugfixing, made position calculation more stable
  - bugfix: 10_IT: Fix readings State for IT V3 switch (Forum #38406)
  - change: SOMFY: New state and action handling (added virtual receiver
            capability)
  - change: FRITZBOX: for most features no telnet access needed anymore
             Execution of own TR-064 commands now possible
  - bugfix: FB_CALLMONITOR: fixing not working company numbers
  - bugfix: 34_NUT: Handling bei Verlust der Verbindung verbessert
  - bugfix: 31_MilightDevice: Small changes from MarkusM
                            (Remove dependency on Math::Round)
  - bugfix: 30_MilightBridge: Minor change to ping code to try and resolve
                            crash when hostname not in dns
  - bugfix: pilight_ctrl: reset - clear send queue
  - feature: pilight_ctrl: add attribute SendTimeout for aborting sending
             commands
  - feature: FB_CALLMONITOR: add TR-064 support for remote phonebook reading
             via official AVM API (by JoWiemann)
  - feature: 10_pilight_ctrl.pm: added disconnect
  - feature: 32_yowsup.pm: added home attribute
  - feature: readingsGroup: allow commands for attributes
                           allow calculation with values in the rows and column
                            allow default mappings with { '' => <default> }
                            added setList and setFn attributes
  - added: 32_yowsup.pm: New module to send and receive WhatsApp messages
  - feature: new module FB_CALLLIST for creating a call list based on
             events generated by FB_CALLMONITOR (original idea by Elektolurch)
  - feature: 01_FHEMWEB: add cmdIcon
  - bugfix:  10_pilight_ctrl: set reset - lost connection to submodules
  - bugfix:  70_Pushalot: corrected parameter order for image
  - change:  70_Pushalot: changed http call to non-blocking
  - feature: 70_Pushalot: module to send push notification to Windows Phone
  - feature: 59_Weather: polish translations (Lukasz)
  - changed: 57_CALVIEW.pm: code cleanup
  - bugfix:  30_pilight_*: restore (StateFn), trigger changes twice
  - feature: 30_pilight_dimmer: new attributes dimlevel_on, dimlevel_off
             dimmers without direct dimlevel support (switch combined with
             screen)
  - bugfix:  73_km200: Bugfix for sorting and comparison method
  - bugfix: SYSMON: CPU frequency
  - feature: OWServer/OWDevice: new device EDS00XX (forum #37453)
  - feature: 59_Weather: french translations and pressure shown in
             state (phervier)
  - feature: 36_LaCrosse: Implemented WS 1600
  - feature: 10_IT: Add HE800 support see
            http://forum.fhem.de/index.php/topic,36399.msg296739.html#msg296739
  - bugfix:  73_km200 - Bugfix for faulty comparison method
  - bugfix:  70_PIONEERAVR: set statusRequest updates now input names
  - feature: 30_pilight_dimmer: up|down commands to change the dimlevel
  - bugfix:  76_MSGMail: Add MSGMail_Attr()
  - feature: 70_PIONEERAVR: new set <dev> hdmiOut <1/2>to switch hdmi outputs
             - new set <name> networkStandby (on|off) Needed to turn on/off...
             - new readings hdmiOut, screenLineNumber[First,Last,Total]
             - commandref reworked
  - bugfix:  73_km200; Floating point calculation error fixed
  - feature: 73_km200; Writing of complete week-list in one single set command
  - feature: 98_Text2Speech.pm; language now selectable
  - feature: 93_DBLog.pm
             - SuppressUndef
               http://forum.fhem.de/index.php/topic,36615.msg289041.html
             - Hinzufuegen von Anfang und Ende-Werten beim Ploten in engen
               Grenzen
               (http://forum.fhem.de/index.php?topic=34006)
             - add new Attribute: DbLogInclude: 93_DbLog_DbLogInclude.diff
             - recognizing of DbLogTyp using DbReadings:
               93_DbLog_dbReadings_using_DbLogType.diff
  - bugfix:  14_CUL_TCM97001: Fix some uninitialized vars, update docu
  - feature: 30_pilight_temp: attribut corrHumidity to correct humidity
  - feature: 76_MSGMail: Add attribute mailtype as suggested by Roger
                         (forum #37206)
  - feature: 30_pilight_temp: reading battery state, attribut corrTemp to
             correct temperature
  - change:  73_km200: Wrong SwitchProgram time format fixed
  - feature: 73_km200: SwitchPrograms can be written/changed
  - change:  MSGMail: Improve error logging to assist problem solving
  - feature: 10_pilight_ctrl possibility to ignore all incomming messages,
             added protocol quigg_gt*
  - change:  MSG: Replace file and mail related code with delegates
  - change:  MSGFile: Assimilate file related code from 75_MSG
                      to make it standalone, without requiring MSG device
  - change:  MSGMail: Assimilate mail related code from 75_MSG
                      to make it standalone, without requiring MSG device
  - bugfix:  MSG: Determine which SSL implementation to use for sending mail
             (required for libnet-3.06)
  - change: MilightDevice/MilightBridge: Fixes, features, changes (by MarkusM)
  - bugfix: SYSMON: network speed
  - improved: I2C_TSL2561: asynchronous measurements, new readings (by jensb),
              new set update command, removed get command
  - feature: SYSMON: method to create html bar chart (thanks to snx)
  - added: SYSMON: new statistic readings for RAM and SWAP
  - change: pilight_ctrl: rename attribut ignore to ignoreProtocol
  - added: SYSMON: some new readings: starttime_text, starttime,
            fhemstarttime_text, fhemstarttime
  - fixed: SYSMON: cpu_freq_stat
  - fixed:  SYSMON: some warnings
  - added:  SYSMON: new readings <network>_speed, cpuX_freq_stat,
            cpuX_idle_stat, cpu_temp_stat
  - improved:  SYSMON: documentation
  - change:  WMBus: support for Easymeter
  - added:   New modules 10_pilight_ctrl, 30_pilight_dimmer, 30_pilight_switch
             and 30_pilight_temp to support pilight (sending and receiving)
  - bugfix:  98_EDIPLUG: change kW/h to kWh and fix missing Id
  - feature: FB_CALLMONITOR: new reverse search method "textfile" for custom
                             definitions
  - bugfix:  FB_CALLMONITOR: correct reverse search of Call-By-Call outgoing
             calls
  - feature: FB_CALLMONITOR: reverse search order can now be configured
  - bugfix:  57_CALVIEW: fixed tomorrow dates when new month
  - bugfix:  73_km200 - Fix for handling back "0" floatvalues with get-command
  - bugfix:  73_km200 - Fix for wrong service as reading for errorLists
  - bugfix:  73_km200 - Fix DoNotPoll of root services
  - feature: 73_km200 - Handback of complete errorList on notification-service
  - change:  CUL_IT: Update documentation
  - Bugfix:  CUL_TCM97001: Add temperature trend, update documentation
  - feature: new fhemweb widgets. see widgetOverride in commandref
  - Bugfix:  73_km200 - Fix for get-command responding with false error message
  - Feature: 73_km200 - Get and Set command blocked during initialisation
             process
  - Feature: 73_km200 - Optional Argument for get command introduced
  - Bugfix:  55_GDS - use onset for a_X_valid calculation
  - Bugfix:  Update of set-command introducing ReadBackDelay - attribute
  - feature: SYSMON: new reading 'cpu_model_name'
  - feature: FB_CALLMONITOR: new set command rereadCache
  - feature: SYSMON: new reading: cpu_core_count
  - feature: SYSMON: Allows to suppress reading certain information.
  - change:  14_CUL_TCM97001: Add support for ABS700, NC_WS, GT-WT-02 and
             AURIOL sensors
  - added:   New modue 38_JawboneUp: Fitness and sleep statistics in FHEM
  - change:  FB_CALLMONITOR: use cache first for reverse search
  - feature: 14_CUL_TCM97001: Add receiving for GT-WT-.. and Rubicson sensors
  - feature: 73_km200: Sounding changed from static list to automatic
  - feature: FHEMWEB: filter dialog for eventMonitor allows filtering for
             specific events
  - feature: 10_IT.pm: add support for intertechno protocol 3 dimmer
  - feature: 51_I2C_TSL2561.pm: add support for using IODev, allows use without
             HiPi being installed. By jensb, forum id 277192
  - feature: SYSMON: Freq. for 8 CPU Cores
  - feature: 98_Modbus.pm: added base module for modbus devices
  - feature: 98_ModbusAttr.pm: added module for generic modbus devices
             Readings can be defined by attributes comparable to HTTPMOD
  - feature: 98_ModbusSET.pm: added module for SET Silent Heat pumps
  - change:  10_RESIDENTS: renamed reading residentsGuests to
             residentsTotalGuests
  - change:  SYSMON: warnings, docu
  - bugfix:  73_km200: Bugfix for fullResponse
  - feature: 73_km200: New services found
  - change:  57_CALVIEW: commandref improved and improved def check (for
             mode-parameter)
  - feature: 73_km200: Read of switchPrograms added
  - bugfix:  57_CALVIEW: fixed commandref
  - feature: GUEST: added support for RESIDENTS toolkit
  - feature: ROOMMATE: added support for RESIDENTS toolkit
  - feature: RESIDENTS: added support for RESIDENTS toolkit
  - added:   RESIDENTStk: new RESIDENTS toolkit and first function wakeuptimer
  - bugfix:  37_SHC: go back to last release version v0.9.0 (rr2000)
  - change:  SYSMON: prevent some warnings
  - bugfix:  SYSMON: ethernet readings on bbb (thx to nesges)
  - changed: 37_SHC: now add all files for the previous commit (rr2000)
  - feature: 37_SHC: add new support for SoilMoistureMeter and add
             support for DigPort and DigPin in Powerswitch (rr2000)
  - feature: 02_HTTPSRV: query string sets readings (Stefan Strobel)
  - bugfix:  57_CALVIEW: - bugfix in set function
  - change:  57_CALVIEW: - fixed function 'set intervall'
             - see comandref for detail (now use the define
               for change intervall)
  - change:  73_km200 - More Services added
  - bugfix:  73_km200 - Re-Read bug in set function corrected
  - change:  SYSMON: improved network readings
  - change:  FB_CALLMONITOR: new attribute "country-code" to import
             phonebook entries with your local country code preceded as
             a national phonenumber in a correct way.
             Per default "0049" is used as country code. (by prodigy7)
  - feature: FB_CALLMONITOR: new get commands showPhonebookEntries
             and showCacheEntries to get all related entries
  - changed: enabled authentication with the logitech myharmony server
             for hub firmware version 4.x, version 3.x still works without.
  - feature: YAMAHA_BD: support 95_remotecontrol.pm module features
  - changed: Reverted to previous version. Module not working on RPi
  - feature: 71_PHILIPS_AUDIO: Implemented UPNP/DLNA player discovery.
  - feature: 57_CALVIEW: added multiple CALENDAR support, reading source
             and location for terms
  - update : 73_km200 Update: New services found
  - feature: 89_HEATRONIC.pm: added power of heating pump
  - feature: 31_MilightDevice.pm: Support LightScene
  - changed: 89_HEATRONIC.pm: calculation of sol_Tcollector changed
  - feature: # comments in fhem.cfg are only removed at the line-start
  - feature: set command modifyTimeSpec for at, to be used in webCmd
  - added:   New module 71_PHILIPS_AUDIO.pm for Philips MCi, Streamium and
             Fidelio devices.
  - bugfix:  FB_CALLMONITOR: fixed reverse-search for search.ch
  - feature: help is now a separate module
  - feature: pahColor() added to Color.pm to convert temperatures
             into rgb values. See forum thread #30128
  - feature: FB_CALLMONITOR: read all available phonebooks directly wia
             web interface (also online phonebooks from Google, etc.).
             new attributes fritzbox-remote-phonebook-via and
             fritzbox-remote-phonebook-exclude.
             new get command showPhonebookIds. Details can be read in
             commandref (by JoWiemann)
  - feature: 02_RSS.pm: new attribut autoreread; new NotifyFn and UndefFN;
             new layout commands textboxf, embed, push, pop;
             FWext is automatically deleted after deletion of last
             RSS device; RSS Overview and elements opened in new tab;
             refresh 0 to disable autorefresh; new function plotFromUrl
  - bugfix:  SOMFY: use correct attributename when calculating updatetime
  - feature: 95_FLOORPLAN.pm: arrange by drag&drop,
             copy, rename, delete processes userattr fp_<name>
  - added:   30_LIGHTIFY.pm: New module for OSRAM LIGHTIFY gateways
  - changed: 98_pilight.pm: New protocols
  - feature: 55_InfoPanel - added direct link to rect,circle,ellipse,
                            img, trash
                          - added new layout item "counter"
  - changed: SYSMON: telnet support improved
  - feature: SYSMON: (partially) QNAP-support
  - feature: SYSMON: user defined functions
  - feature: SYSMON: list_lan_devices (FritzBox only)
  - changed: SYSMON: improved support for FritzBox OS 6.23
  - bugfix:  SYSMON: some warnings
  - added:   move 55_InfoPanel.pm from ./contrib to ./FHEM
  - feature: YAMAHA_AVR: new commands play, pause, stop, skip, shuffle, repeat
  - feature: 71_YAMAHA_NP: New command set and readings for menu navigation
  - feature: 71_YAMAHA_NP: New command 'dimmer [1..3]'
  - bugfix:  31_MilightDevice: if already off don't turn on to set dim level!
  - added:   new dustbin icon
  - bugfix:  SYSMON: some warnings
  - changed: SYSMON: documentation
  - feature: SYSMON: query parameters from remote system (telnet)
  - feature: 71_YAMAHA_NP.pm Improved timer setting
  - feature: 55_GDS uses own FWEXT instead HTTPSRV
  - feature: 98_logProxy.pm added postFn and scale2reading options
  - feature: 70_Pushbullet.pm: new module 70_Pushbullet.pm
  - changed: 31_MilightDevice (Thanks to MarkusM):
                     Saturation set/transition, set with command saturation
                     Bugfix for long transition on hue=0 and hue = 360
                     Set hardware brightness to minimum before off
  - bugfix:  FB_CALLMONITOR: allow spaces in phone numbers stored in phonebooks
  - bugfix:  SYSMON: Symbol '#' in Readings prevents update
  - feature: new helper module TimeSeries.pm (Boris)
  - feature: 71_YAMAHA_NP.pm: Make timer setting more convenient.
  - changed: FB_CALLMONITOR: allow chars in phone numbers for reverse search
  - changed: SYSMON: non-blocking
  - changed: 71_YAMAHA_NP.pm: Provide entire http link to Player AlbumArt.
  - changed: 71_YAMAHA_NP.pm: Minor code improvements.
  - changed: 71_YAMAHA_NP.pm: Perl code clean-up after 'perlcritic' check.
  - feature: 71_YAMAHA_NP.pm: New readings: tunerModeDAB, tunerBitrateDAB,
                                 tunerAudioModeDAB, tunerFrequencyDAB.
                              New internals: NP_ICON_x, UDN, Friendly_Name
  - changed: 73_km200.pm: More services found.
  - bugfix:  FB_CALLMONITOR: read phonebooks after all attributes are set
             from fhem.cfg.
  - feature: 70_XBMC.pm: clear readings when stopping media
  - feature: 70_XBMC.pm: new reading is3DFile for 3D files
  - bugfix:  70_XBMC.pm: improved JSON separator
  - added:   73_km200: More services added.
  - changed: 73_km200: Fhem get-command is able to return raw.
  - bugfix:  73_km200: Handling of unknown attributes corrected.
  - feature: 31_MilightDevice.pm: Add hue/ct colorpickers.
                                  Add "presets" set command.
  - feature: 70_XBMC.pm: new commands poweron,poweroff.
                         configurable by attribute powerCmd
  - added: 71_YAMAHA_NP.pm: New module for controlling Yamaha
                            network players such as CRX-N560(D)
  - bugfix: FB_CALLMONITOR: fix not working telnet login, when user based
            authentication is configured in FritzBox
  - feature: 02_RSS.pm: improved frontpage for RSS
  - bugfix: FB_CALLMONITOR  regognize "user:" as login prompt for
            remote telnet connection (phonebook)
  - changed: 73_km200.pm: DoNotPoll includes top-down hierarchy
  - bugfix : 73_km200.pm: Correction of commandref - entry
  - changed: 98_Text2Speech (thanks to TeeVau):
                             added calculate the MP3 Duration into Reading
                             adjust Volume now in indirect mode possible
  - changed: 57_CALVIEW.pm: code cleanup
  - changed: 73_km200.pm: Reading will be deleted after set by DoNotPoll
  - bugfix:  73_km200.pm: German commandref still contained English text
  - bugfix: 02_FRAMEBUFFER: enable align and textwrap properties of RSS
  - changed: 73_km200.pm: New attribute DoNotPoll and German commandref.
  - added:   57_CALVIEW.pm (chris1284)
  - changed: configDB.pm use fhem function createUniqueId()
             configDB.pm do not show 99_Utils.pm in „Edit files“
  - fix: CUL_MAX: fix usage of advanced culfw features on non-CUL devices
  - changed: 09_CUL_FHTTK: small update to the documentation in order to
             simulate the same
  - fix: 66_ECMD: use STATE not state for connection checking (forum #31307)
  - feature: 57_Calendar: enable gzipped ical files (forum #31845)
  - bugfix: 70_Jabber.pm: XMPP DNS SVR record query added
  - bugfix: 70_PIONEERAVR: fixed "missed to call readingsBeginUpdate first"
  - feature: fhemweb.js rewrite based on jQuery, single-widget-implementation
  - feature: SVG: multiple sources allowed, Plot-Editor
  - feature: textfield-long and knob widgets
  - added:   some new icons by Rampler
  - feature: PRESENCE: new reading "presence" which contains the current (or
    last known) presence state (can be "absent" or "present")
  - bugfix: 70_Jabber.pm: hardening XML::Stream Process() call and fix of
    ssl_verify
  - feature: readingsGroup: allow devspec :FILTER= expressions in device
    selection
  - added:   73_km200.pm for the Buderus KM200 heating controller (Sailor)
  - feature: 70_XBMC: added command 'connect' to connect instantly
  - change: FB_CALLMONITOR: use standard file read/write function to support
    use of configDb
  - bugfix: FB_CALLMONITOR: fix phonebook file read when using configDb (Forum
    #30244)
  - feature: 70_XBMC: added commands: openmovieid, openepisodeid, addon,
    jsonraw (thanks to siggi85)
  - fix: 70_XBMC: made fork attribute to close file handles correctly
  - feature: 70_XBMC: added mechanism to detect disconnects (TCP)
  - fix: 66_ECMD: avoid reading from a closed connection in ECMD_READ
  - feature: 70_PIONEERAVR: readings for currentAlbum etc., more internals
    (network settings, moved some from readings to internals), new attributes
    volumeLimit & volumeLimitStraight
  - added: some new icons (hourglass, frost, sani_heating_level_XX)
  - fix:   sani_heating_boost (possibility to colorize)
  - feature: FB_CALLMONITOR: add remote phonebook lookup via telnet connection
                             to FritzBox (JoWiemann).
  - bugfix: 70_PIONEERAVR & 71_PIONEERAVRZONE: fixed not working set-extensions
    (on-for-timer,...)
  - feature: fheminfo: report third-party modules
  - feature: 99_Utils.pm: add getUniqueID, getKeyValue, setKeyValue
  - feature: SMARTMON: additional parameters for smartctl
  - added: 00_HXB / 10_HXBDevice for Hexabus devices
  - feature: HUEbridge: added group handling
                        added pollDevices attribute
                        added httpUtils for nonblocking mode
  - feature: HUEDevice: added group handling
                        added renaming of devices and groups in the bridge
  - added: 30_MilightBridge / 31_MilightDevice: Support Milight
           (Applamp/LimitlessLED/EasyBulb) LED lights/strips/controllers.
  - feature: HUEDevice: allow ct presets in webCmd
                        new subTypes extcolordimer and ctdimer
                        start support for Lightify bulbs
  - added: SONOS and SONOSPLAYER to support Sonos Multiroom Audiosystems
    (Reinerlein)
  - change: 64_ESA2000.pm: add batterystate
  - added:   42_SMARTMON: Frontend to smartctl (maintainer: hexenmeister)
  - feature: 70_PushNotifier added line break in Messages (xusader)
  - feature: readingsGroup: added valuePrefix and valueSuffix attributes
                            added collapsed/collapsible to visibility attribute
                            added visibility command
  - bugfix: FB_CALLMONITOR: fixing not working company numbers
            reverse search for search.ch
  - bugfix: 70_PushNotifier repair set function (xusader)
  - bugfix: PRESENCE: fixing not working timer, when using set [...]
    statusRequest
  - bugfix: FB_CALLMONITOR: fixing reverse search for klicktel.de
  - feature: new module 52_I2C_MCP342x.pm added (klausw)
  - feature: SYSMON: read cpu temp on FritzBox
  - feature: ios7smallscreenstyle.css: table width based on screen width, new
                                       header, links colored in detail view
  - feature: new module FRITZBOX: controls Fritz!Box router and Fritz!Fon
  - feature: new module 52_I2C_EEPROM.pm added (klausw)
  - feature: readingsGroup: added ! flag,
                            added visibility and cellStyle attributes
  - feature: new module 52_I2C_MCP23008.pm added (klausw)
  - feature: new module 98_logProxy.pm added (justme1968)
  - change: 66_ECMD: ReadyFn added (fixes issue under Windows)
  - change: 02_RSS: use a GUID in RSS; urlq source for img command
  - feature: 70_PushNotifier improve usebility, configuration without cURL
    (xusader)
  - bugfix: SYSMON: prevent empty line im log by userReadings
  - feature: 10_IT empfang (by bjoernh)
  - bugfix: PRESENCE: fix race condition, when delete disabled attribute and
                      PRESENCE does not start to scan.
  - feature: OPENWEATHER: captures weather forecast from API of www.wetter.com
  - fhem 5.6 released

- 2014-11-09 (5.6)
  - bugfix: FB_CALLMONITOR: fixing race condition of missing events while
                            performing multiple calls
  - feature: PROPLANTA: captures weather forecast from web pagewww.proplanta.de
  - feature: 15_CUL_EM added attribute maxPeak (arnoaugustin)
  - bugfix: 10_IT changed "setstate" to avoid eventMap errors (arnoaugustin)
  - feature: new module 37_harmony.pm added (justme1968)
  - change: WMBUS: use _ instead of : as readings separator, better support for
            EnergyCam
  - feature: new module 23_KOSTALPIKO added (john)
  - feature: new module 98_HourCounter added, 99_UtilsHourCounter.pm added to
             contrib (john)
  - added: MYSENSORS: connect to serial or Ethernet MySensors Gateway
  - added: MYSENSORS_DEVICE: represent a MySensors sensor- or actor node
  - feature: global ATTR/DELETEATTR/MODIFIED events
  - feature: 55_GDS.pm - attr disable added
  - bugfix: SYSMON: prevent endless loop at startup with 'disable' attribute
  - feature: SYSMON: added FritzBox informations: DSL rate, DSLAM sync time,
             count of CRC an FEC
  - bugfix: SYSMON: unwanted characters in dsl info lines
  - change: 57_Calendar: process continuation lines, get/set syntax checks
  - bugfix: SYSMON: fix availability of cpu/kernel_max
  - bugfix: SYSMON: numeric check
  - change: 59_Weather: change icons for conditions 31, 34, 36
  - added: MQTT: connect fhem with mqtt
  - added: MQTT_BRIDGE: bidirectional mapping of existing fhem-device to
           mqtt-topic
  - added: MQTT_DEVICE: fhem-device that can be controlled by and publishes to
           mqtt
  - added: I2C_LCD: module to drive PCF8574T based LCD connected via I2C
  - added: I2C_DS1307: module to read time and date from DS1307 connected by i2
  - added: OWX_ASYNC: asynchronous, non-blocking version of OWX for DS2480,
           DS9097 and FRM
  - feature FRM: work as physical IODev for I2C_XXX modules
    added: FRM_ROTENC: read rotary-encoders with FRM
    added: FRM_RGB: control rgb-leds with FRM
    added: FRM_STEPPER: control stepper-motors with FRM
    added: FRM_AD: analog input for FRM
    added: FRM_PWM: analog (pwm) output for FRM
    added: FRM_SERVO: control servo-motors with FRM
  - added: FRM_IN: digital input for FRM
  - added: FRM_OUT: digital output for FRM
  - added: FRM: connect Arduino with firmata to fhem
  - change: 57_Calendar: line parsing rewritten, care for missing
                         modification timestamps
  - change: SYSMON: support userReadings in SYSMON_ShowValues
  - change: 59_Weather: change icon for condition clear to sunny.png
  - bugfix: 57_Calendar: calendar event anymore in modeAlarmed if started
  - feature: 57_Calendar: deal with non-existent end times
  - bugfix: SOMFY: fix non-working on/off-for-timer methods
                   made positioning attributes optional
  - feature: SOMFY: support for exact positioning (one-time setup of run times
             required) support for parse()-function, requires newest CULFW.
  - feature: userattr is now also device attribute
  - feature: ZWave: Fibaro_FGRM222 MANUFACTURER_PROPRIETARY class
  - feature: sequence: reportEvents attribtue added
  - feature: SYSMON: RAM and SWAP Readings on OSX
  - change:  34_NUT: removed calculation of values. Use userReadings instead.
                     removed autogeneration of attr model and serNo.
  - feature: SYSMON: improvement: support network information (IP, IPv6) on
             german linux
  - feature: Synology DiskStation NAS basic spk file creation
  - change:  34_NUT: readingFnAttributes added; creation of units deleted;
                changed attr asReadings to use comma instead of space
  - bugfix:  SYSMON: crash on FritzBox
  - bugfix:  34_NUT: fixed possible buffer overflow, rewrote reception of data
  - bugfix:  SYSMON: idletime on multicore, warnings
  - change:  09_CUL_FHTTK.pm: modified set option for sync, open and closed
  - feature: SYSMON: HTML/Text output for SYSMON-CloneDummies
  - feature: SYSMON: Method for titled HTML/Text output
  - added:   34_NUT.pm (maintainer: creideiki)
  - feature: SYSMON: added new reading: perl_version
  - feature: add toggle to SetExtensions (introduced for ZWave)
  - bugfix:  plotEmbed FHEMWEB attribute (fix for an iOS8 bug)
  - feature: SHC: support for analog inputs (EnvSensor) and new device
                  RGB_Dimmer added (rr2000)
  - feature: PRESENCE: MAC address support for mode fritzbox (by Markus M.)
  - bugfix:  PRESENCE: fixing presence detection in mode fritzbox with new
             Fritz!OS 6.20 (by Markus M.)
  - feature: FB_CALLMONITOR: reverse-search attribute is now providing all
             possible values, which are selectable (via fhemweb_multiple.js).
             see commandref for all possible values
  - feature: speed up through caching of postproc and regex in ECMDDevice
  - bugfix:  fixed handling of autocreation for 10_OWServer.pm
  - feature: option to cope with partial messages in ECMD/ECMDDevice
  - bugfix:  SOMFY: add module to CUL client list, to set IODev automatically
  - feature: sequence: triggerPartial Attribute added
  - feature: 36_JeeLink: changed flash command to use fhem firmware
                         directory (by HCS)
  - feature: 70_ENIGMA2: new attribute lightMode for old/slow devices
                         limited restricted functionality
  - added:   98_CustomReadings.pm (maintainer: HCS)
  - change:  98_Text2Speech.pm: fix a problem with microseconds in time()
             by using mp3-templates or playing mp3 directly
  - feature: state definition and split attribute added to 66_ECMD,
             67_ECMDDevice
  - FHEMWEB: JavaScripts and CssFiles attributes added
  - change:  avoid updating weather information on get (59_Weather.pm)
  - change:  removed noshutdown=0 for HTTP connections made in 57_Calendar.pm
            and 59_Weather.pm to address issues when FHEM is behind a web proxy
  - feature: update rewritten, restore added
  - feature: enabled JavaScript in 02_RSS to support WebViewControl
  - added:   new module 36_WMBUS.pm (kaihs) Wireless M-Bus
  - feature: SYSMON: aded new plots (power infos for cubietruck)
  - feature: SYSMON: aded new readings for each network interface: ip and ip6
  - feature: SYSMON: aded power supply informations to the text output method
  - feature: SYSMON: power supply informations (ac, usb, battery)
  - feature: added 70_PushNotifier.pm
  - feature: 70_VIERA: Add parameter "HDMI1" -"HDMI4" for command remoteControl
             to select HDMI input directly. Add command "input" to select a
             HDMI port, TV or SD-Card as source
  - bugfix:  LevelSender: Version 1.0.5: Could not get compiled by the Arduino
             IDE
  - feature: PRESENCE: new event "error" and "timeout" for state reading to
             indicate a non successful check
  - bugfix:  70_Jabber: fixed UTF8 encoding/decoding of messages
  - feature: 10_OWServer autocreate coexists with OWXXX modules (Boris &
             ntruchsess)
  - feature: added 36_Level.pm
  - feature: netatmo: added plz support for public stations
  - change:  70_ENIGMA2: keep reading for recordings up-to-date during standby
  - bugfix:  98_Text2Speech: - playing mp3files directly, eg: :ring.mp3:
                             - playing any mp3file only text
  - feature: FB_CALLMONITOR: new reading "direction" to differentiate
             between incoming and outgoing call.
  - feature: FB_CALLMONITOR: all informational readings about a call will be
             triggered for each call event
             (call, ring, connect and disconnect)
  - feature: mailcheck: allow user and pssword as perl expression
  - feature: netatmo: support for public stations
  - feature: PRESENCE: new set command "power" to execute a FHEM command
             which can power on or off the checked device (given via attribute)
  - feature: readingsGroup: added valueColumn attribute
  - feature: readingsGroup: added ...,<reading>@<device>,... argument format
  - feature: 52_I2C_PCF8574.pm: added attribute OnStartup
             52_I2C_PCA9532.pm: added attribute OnStartup,
                added attribute OutputPorts as substitute for InputPorts
             51_RPI_GPIO.pm: changed access to gpio via userspace by default
                (for BBB and Cubie), access via gpio utility as fallback
  - feature: PIONEERAVR: new attribute: checkConnection
  - change:  do no parse empty lines in 57_Calendar.pm
  - bugfix:  10_SOMFY.pm: save enc-key and rolling-code as reading instead of
             attribute to prevent loss of control after FHEM restart.
  - feature: new module 10_SOMFY.pm to support Somfy RTS blinds
  - bugfix:  70_PIONEERAVR.pm: fix for STATE if connection is lost
  - bugfix:  37_SHC.pm: Move xml file under subdir lib, otherwise it won't be
             deployed during update
  - bugfix:  70_PIONEERAVR.pm: player commands are now available for more input
             "play" was not in the drop down list of available set commands
             check every 120s if the data connection to the Pioneer AV
             receiver is still up check if we get a reply from the Pioneer AV
             receiver not later than 3s after a command was sent fix for alias
             names of inputs more input presets (spotify, mhl, hdmi7, hdmi8),
             inputs are now queried from 1 - 59
             71_PIONEERAVRZONE.pm: bugfix:logging, set input
  - change:  00_RPII2C.pm: hardware access changed to ioctl and syswrite/read
             SMBus module not needed anymore but still usable, see attribute
             useHWLib possibility to swap I2C-0 to P5 for Rev. B raspberries
             via attribute swap_i2c0 (not tested yet)
  - feature: 70_ENIGMA2: add attribute
             remotecontrol=[standard,advanced,keyboard]
  - bugfix:  70_PIONEERAVR.pm and PIONEERAVRZONE.pm: added "use SetExtensions",
             commandref updates fixed RC_layout
  - feature: new modules 70_PIONEERAVR.pm and PIONEERAVRZONE.pm
  - feature: FLOORPLAN has new style 7 to display commands only.
  - added:   89_HEATRONIC.pm (heikoranft)
  - bugfix:  duration parsing of calendar events in 57_Calendar.pm fixed
  - feature: LightScene: added followDevices attribute
  - feature: non-blocking retrieval of data in 59_Weather.pm (Boris & herrmannj
  - feature: new modules 37_SHC.pm and 37_SHCdev.pm added (rr2000)
  - feature: 36_EMT7110: added this new module
  - feature: 36_JeeLink: added initCommands attribute and flash command (by HCS
  - feature: SYSMON: DECT Temperatur
  - bugfix:  SYSMON: prevent some warnings
  - change:  SYSMONremoved support for old format of filesystem reading
  - change:  moved 98_openweathermap.pm to contrib
             moved 98_geodata.pm to contrib
             moved 55_BBB_BMP180.pm to contrib
  - change:  honor DURATION in 57_Calendar.pm
  - bugfix:  YAMAHA_AVR: don't let FHEM hang anymore, when the receiver
             is not reachable
  - change:  55_GDS.pm: use Blocking.pm for retrieval of large files
  - change:  YAMAHA_BD: make YAMAHA_BD more performant by using non-blocking
             HTTP request (from HttpUtils.pm)
  - added:   YAMAHA_BD: new set command trickPlay and more remoteControl
             commands. new reading trickPlay
  - added:   new module 98_statistics.pm: hourly, daily, monthly, yearly
             statistics for min/avg/max/delta/duration of selected readings
  - added:   new module 52_I2C_MCP23017.pm (klausw)
  - feature: Dashboard Configuration-Dialog for Tabs
  - feature: new module 33_readingsHistory.pm added (justme1968)
  - feature: new command copy (justme1968)
  - feature: enabled GIF, PNG and JPG as background image formats, enabled
             relative font size changed and perl specials for font size
             in 02_RSS.pm
  - feature: YAMAHA_AVR: new set commands and readings for controlling
             the sound output behavior (Enhancer, DSP and straight
             output) and sleep timer. For details, see commandref.
  - bugfix:  configdb filemove not working after previous changes
  - change:  IMPORTANT CHANGES TO configDB!
             changed: all files will be imported as binary
             changed: all existing textfiles will be moved to binary
             removed: command binfileimport
             added: sorted write and read of configuration data
  - bugfix:  SYSMON: css class name (sysmon)
  - feature: option to determine the number of icons from WeatherAsHtml
  - feature: DbLog: (thanks to betateilchen)
             * added new global modules function $hash->{DbLog_splitFn}
               to let split the generated events by the own module
               into readingsname, value and unit
             * added SVG_sampleDataFn
             * added FW_detailFn
  - added:   new module contrib/97_SprinkleControl.pm (tobiasfaust)
  - added:   new module contrib/98_Sprinkle.pm (tobiasfaust)
             both modules helps to control the sprinkles in your garden
             --> take a look to the Wiki-Article
             http://www.fhemwiki.de/wiki/Bew%C3%A4sserungssteuerung
  - feature: FB_CALLMONITOR: new reading "missed_call_line" indicating
             the line number which received the missed call
  - feature: YAMAHA_AVR current* readings will be erased in case they
             not applicable
  - feature: YAMAHA_AVR currentTitle available for TUNER
  - feature: new Method: SYSMON_getValues([desired keys])
  - feature: JSONMETER: hourly statistics
  - feature: configdb: new command search
  - feature: LUXTRONIK2: estimation of electrical power consumption,
             considers time depending tariffs (activeTariff)
  - added:   configDB functions for handling binary files
  - feature: 02_RSS.pm: alpha channel for colors
  - feature: JSONMETER: time depending tariffs added (activeTariff)
  - updated: codemirror version 3.24
  - feature: new module 35_SWAP_0000002200000008 for panstamp
             indoor multi sensor board with tft
  - added:   new module 36_EC3000.pm (justme1968)
  - feature: IT: added support for set-extensions (justme1968)
  - added:   new modules 10_Itach_IR and 88_Itach_IRDevice to
             use Itach WF2IR or IP2IR to be used as universal
             infrared remotecontrol
  - added:   new module 51_I2C_TSL2561.pm (kaihs)
  - added:   new module 02_FRAMEBUFFER.pm (kaihs)
  - feature: SYSMON: many FritzBox specific readings:
             wlan_state, wlan_guest_state, internet_ip, internet_state,
             night_time_ctrl, num_new_messages, fw_version_info
  - feature: configDB: added command fileshow
  - feature: configDB: added commands filelist and filedelete
  - feature: configDB: added commands fileimport and fileexport
  - feature: 36_JeeLink: added LaCrosse, ETH200comfort, CUL_IR,
             HX2272 and FS20 modes from ulli
             added AliRF
             added Clients and MatchList attribute
  - feature: 02_RSS.pm: HTTPS enabled, png as image type added, autofreshing
             HTML page with image map added
  - feature: ECMD and ECMDDevice completely reworked, see
             http://forum.fhem.de/index.php/topic,21515.0.html
  - feature: new layout command rect and new attribute bgcolor for RSS
  - added:   new module 55_weco.pm (betateilchen)
  - added:   new module 70_Jabber.pm (BioS)
  - bugfix:  Dashboard: use "loadScript" for load JavaScripts
  - feature: new module 00_NetzerI2C.pm, 51_Netzer.pm added (klausw)
  - feature: new command reload for 57_Calendar.pm forces cleanup
  - changed: small update to the documentation of recurring events in
             57_Calendar.pm
  - bugfix:  PRESENCE: fixing wrong presence state for mode lan-ping
             when device is unreachable
  - feature: 10_EnOcean: new EEP profiles: D2-01-00 - D2-01-11 (VLD)
  - changed: 00_TCM/10_EnOcean: learning mode (teach-in / teach-out) changed
             and extended
  - added:   new module 10_UNIRoll.pm (c-herrmann)
  - feature: cloneDummy: new attribut cloneIgnore
  - feature: cloneDummy: new optional parameter [reading]
  - bugfix:  Dashboard: dashboard_showfullsize not applied in room "all"
  - feature: new module 98_PID20.pm added (John / betateilchen)
  - feature: new module 00_RPII2C.pm, 52_I2C_PCA9532.pm, 52_I2C_PCF8574.pm,
             52_I2C_SHT21.pm added (klausw)
  - change:  module 71_LISTENLIVE.pm moved to contrib
             module 23_WEBTHERM.pm   moved to contrib
  - change:  module 98_PID.pm        moved to contrib as preparation for
             next major replace. Replaced by 98_PID20.pm (John/betateilchen)
  - change:  openweathermap: added set command "clear"
  - change:  MAX: interpret SetTemperature command from WT to HT
  - feature: MAX: retry packets 3 times if missing an ack
  - feature: new module 98_cloneDummy.pm added (Joachim)
  - feature: STACKABLE_CC (busware.de device for the RPi) added
  - feature: configdb export/import added for data security (betateilchen)
  - feature: new module 38_netatmo.pm added (justme1968)
  - change:  09_CUL_FHTTK.pm: clean up code to avoid "Use of uninitialized
             value in concatenation.."
  - change:  09_CUL_FHTTK.pm: extend module list to FHT80TF and FHT80TF-2
             and update of documentation (matscher)
  - feature: disabledForIntervals attribute added for at/notify/watchdog
  - feature: jsonlist2 added, jsonlist is deprecated.
  - feature: DbLog: Added new function : ReadingsVal/ReadingsTimestamp
  - feature: Text2Speech: added new attribute TTS_VolumeAdjust
  - feature: new module 70_PHTV.pm (loredo)
  - feature: JSONMETER: added statistic functions
  - feature: LightScene: added scene editor from UliM
  - feature: SYSMON: New method: SYSMON_ShowValuesText
  - feature: configDB.pm use sql database instead of fhem.cfg (betateilchen)
  - feature: new module 98_geodata collect location based data (betateilchen)
  - feature: 98_pilight: Added support for Elso protocol
  - feature: readingsGroup: added sortDevices attribute
  - feature: ENIGMA2: new reading 'recordings', new command record
  - change:  ENIGMA2: rewrite for NonBlocking
  - feature: SYSMOM: new Plot + Doc
  - feature: Dashboard: Custom CSS Attribute. Max. 7 Tabs.
  - bugfix:  Dashboard: Change Groupcontent sorting. Fix Bug that affect
             new Groups.
  - feature: 10_EnOcean: UTE protocol implemented
  - feature: 00_TCM: new command teach
  - bugfix:  SYSMOM: uninitialized value warning on FritzBox
  - added:   09_CUL_FHTTK.pm: german module documentation (matscher)
  - feature: readingsGroup: allow FHEMWEB slider and dropdown menus as commands
  - feature  FB_CALLMONITOR: new attribute "disable" to
             disable FB_CALLMONITOR
  - feature: YAMAHA_BD: new attribute "disable" to disable cyclic status
             updates of player
  - change:  09_CUL_FHTTK.pm: added event-on...readings and event-min-interval
             updated to reading update mechanism (matscher)
  - feature: Dashboard: Groupstitel now can show icons,
             Backbutton in Fullsize-Mode
  - deleted: 51_BBB_WATCHDOG.pm - not really needed
  - bugfix:  DbLog: adding ShutdownFunction
  - feature: YAMAHA_AVR: new attribute "disable" to disable cyclic status
             updates of receiver
  - feature: LightScene: added attribute switchingOrder
  - added:   new module 00_THZ.pm (immiimmi)
  - added:   new module 98_HTTPMOD.pm (stefanstrobel)
  - added:   new module 51_BBB_WATCHDOG.pm (betateilchen)
  - bugfix:  SYSMON: Fix: uninitialized variable
  - feature: new modul 73_MPD added (Wzut)
  - bugfix:  SYSMON: Fix: root fs with /dev/mapper
  - feature: Dashboard: The display of the dashboard can be limited to a
             defined FHEMWEB. Change view of readingroups
  - feature: new module 70_JSONMETER to read obis compatible data in json
             format from so called smart meters for electricity, gas or heat
  - feature: new modules 10_RESIDENTS, 20_ROOMMATE and 20_GUEST added (loredo)
  - feature: LUXTRONIK2: attribute 'doStatistics' calculates boiler gradients
  - feature: GEOFANCY: support both apps, Geofency.app and Geofancy.app
  - feature: LightScene: added attribute lightSceneRestoreOnlyIfChanged
  - bugfix:  SYSMON: Fix: CPUTemp & BogoMIPS for utilite-Box.
  - bugfix:  PRESENCE: fix present-check-interval to be equal with normal
             check-interval if not set in define statement and not 30 sec.
  - feature: DASHBOARD: Tabs can show an icon.
  - bugfix:  DASHBOARD: dashboard_showfullsize only in DashboardRoom.
             Fix showhelper Bug on lock/unlock. The error that after a trigger
                         action the curren tab is changed to the "old"
                         activetab tab has been fixed.
  - bugfix:  SYSMON: Filesystems (absent medium)
  - feature: FLOORPLAN-menu-items can get icons attached by new
             attribute fp_roomIcons
  - feature: FLOORPLAN-specific icons can now be assigned by just
             creating a folder under fhem/images with the flooplan-name
  - feature: DASHBOARD:  Tabs can set on top, bottom or hidden.
  - bugfix:  SYSMON: another format for ifconfig output
  - feature: DASHBOARD: Use longpoll to update content. rowcentercolwidth can
             now be defined per column.  Dashboard can hide FHEMWEB Roomliste
             and Header => Fullsizemode.
  - bugfix:  SYSMON: null reading for absent mount points
  - feature: DbLog: jokers "%" in device/reading definition are now possible
  - feature: SYSMON: new CPU Statistics and Plots
  - feature: changed 10_OWServer.pm and 11_OWDevice.pm to use
             NOTIFYDEV (justme1968)
  - feature: LightScene: added setcmd command
  - feature: DASHBOARD: Dashboard get Tabs. Redesign saving of Group positionin
  - bugfix:  SYSMON: Log Warnings, unnoetige Readings erkenen und entfernen
  - feature: LUXTRONIK2: Setting of controller parameter and internal clock
  - feature: new module 71_YAMAHA_BD.pm to control Yamaha Blu-Ray
             players over network.
  - bugfix:  DbLog: fix for plotfork
  - bugfix:  SYSMON: filesystems may be wrong on some systems
  - feature: new module 98_pilight.pm added (andreas-fey)
  - change:  LUXTRONIK2 - made compatible with current developer guidelines
             (Blocking.pm, reading update mechanism)
  - feature: readingsGroup: added icons and links/commands
  - feature: new module 98_Text2Speech.pm added (Tobias Faust)
             Google Translator Engine or ESpeak can be used
  - feature: YAMAHA_AVR: define separate on and off status intervals for
             cyclic status updates
  - feature: Visualizations (Plots) for SYSMON added
  - feature: new module 42_SYSMON.pm added (hexenmeister)
  - feature: YAMAHA_AVR: new readings for radio stations, current title
             and more. see commandref for more details.
  - feature: new module 32_withings.pm added (justme1968)
  - bugfix:  PRESENCE: fixing user detection on FritzBox!
  - feature: new module 38_CO20.pm added (justme1968)
  - feature: new module 98_GEOFANCY.pm added (loredo)
  - feature: new module 70_XBMC.pm added (dbokermann)
  - feature: new module 51_RPI_GPIO.pm added (klausw)
  - bugfix:  Dashboard: fixed bug identification an existing Weblink.
             fixed bug dashboard_sorting check. Buttonbar can now placed on
             top or bottom of the Dashboard. Dashboard is always edited out
             the Room Dashboard.
  - bugfix:  VIERA: fixed bug related to set command remoteControl
  - bugfix:  ENIGMA2: improved compatibility for Fritzbox and old Webif version
  - feature: readingsGroup: process events only if visible in browser,
             allow <br> for line breaks in multi-reading lines
  - feature: FLOORPLAN: Style4 (S300TH specific) now keeps its formatting
             even with longpoll; Text "desiredTemperature" will now
             be eliminated - for MAX devices.
  - feature: HCS has now MAX Thermostat support
  - change:  integrated OWServer/OWDevice nonblocking and random start
             time patches (justme1968 & Boris)
  - feature: Add new module Dashboard
  - change:  ONKYO_AVR: transfer command database into separate packet
             ONKYOdb.pm
  - feature: ENIGMA2: bouquet support e.g. for named channels
  - feature: Add new module ONKYO_AVR
  - feature: SYSSTAT: allow (remote) monitoring via snmp, support
             for monitoring windows systems and synology system temperature
  - feature: New module LINDY_HDMI_SWITCH.pm added
  - change:  ENIGMA2: improved logging, default attributes for webCmd and
             devStateIcon
  - feature: ENIGMA2: support for option channels
  - feature: mailcheck: decode non ascii subjet to utf-8, verify gpg signatures
  - feature: PRESENCE: "statusRequest" command for lan-bluetooth mode
             (collectord >= 1.4, presenced >= 1.1 required)
  - feature: PRESENCE: new collectord package
  - feature: devspec: removed range, added :FILTER and more general search
  - feature: HUEBridge,HUEDevice: support for groups added
  - feature: YAMAHA_AVR: new argument "toggle" for mute command
  - feature: FB_CALLMONITOR: replace &amp; to & at reverse search
  - feature: new module 33_readingsProxy to make (a subset of) a reading
             from one device available as a new device. can be used to
             separate channels from 1-wire, EnOcean or SWAP multichannel
             devices (by justme1968)
  - change:  improvements for OWDevice and OWServer (justme1968)
  - feature: new attribute resolution for 1-wire temperature readings
             (justme1968 & Boris)
  - feature: new layout commands moveto, moveby and relative positioning
             in 02_RSS.pm (Betateilchen & Boris)
  - feature: FHEMWEB column attribute
  - feature: new layout commands halign, valign, condition in 02_RSS.pm
             (Betateilchen & Boris)
  - bugfix:  PRESENCE: Fix nonworking initialization in mode "lan-bluetooth"
  - bugfix:  fhem.pl: write-select to avoid blocking in inform/Event Monitor
  - bugfix:  fix issue with DST changes in 57_Calendar.pm
  - feature: new module 36_LaCrosse.pm for LaCrosse IT+ temperature and
             humidity sensors with a JeeLabs JeeLink as RF modem.
             The matching JeeNode sketch can be found in
             .../36_LaCrosse-LaCrosseITPlusReader.zip (by ohweh&justme1968)
  - feature: YAMAHA_AVR: new attribute request-timeout.
  - bugfix:  YAMAHA_AVR: fix missing greater-than sign. Use different
             Control-Tag name for RX-Vx75 series
  - bugfix:  PRESENCE: fixing not working re-initialization when
             disabled attribute is set to 0 in lan-bluetooth mode
  - feature: LightScene: added attribute lightSceneParamsToSave for
             device specific configuration of </command pairs
             used to save/restore device state
  - feature: cmdalias added
  - feature: rain Module by baumrasen
  - feature: endPlotNow attribute for SVG-Plots (ChrisD)
  - feature: new module 51_BBB_BMP180.pm added (betateilchen)
  - feature: readingsGroup: allow devStateIcon to be displayed
  - feature: readingsGroup: allow multiple device readings in one line
  - feature: YAMAHA_AVR - new remoteControl commands for Tuner Preset
             selection
  - feature: RSS amended (read image from pipe, scaling options, line width)
  - feature: WWO Module by baumrasen
  - feature: plotAsPng() in 98_SVG.pm (Boris & betateilchen)

- 2013-09-29 (5.5)
  - feature: new module 55_PIFACE.pm added (betateilchen)
  - feature: Calendar can read from file and limit number of calendar events
             retrieved in get command
  - feature: new module 70_ENIGMA2.pm added (by loredo)
  - change:  CustomGetFileFromURL() in HttpUtils.pm now reacts to
             "301 Moved Permanently" return code
  - change:  changed exit to POSIX::_exit in 10_OWServer.pm
  - feature: new module 32_mailcheck.pm (by justme1968)
  - feature: TCM: new commands added
  - bugfix:  TCM: TCM_ReadAnswer(): response error corrected
  - feature: readingsGroup: new attribute nolinks
  - feature: readingsGroup: new attribute nameIcon
  - feature: readingsGroup: allow device selecton by TYPE=xxx
  - feature: new module Revolt for Revolt NC-5462 power metering devices.
             (by mehf)
  - feature: HUEDevice: added alert command
  - change:  The DBLOG propagated Attribute DbLogExclude will work as
             regexp to exclude defined readings to log.
             If a MinInterval is set, the logentry is dropped if the
             defined interval is not reached and value vs. lastvalue is eqal
  - change:  readingsGroup added valueFormat
  - feature: new modules JeeLink and PCA301 and for the ELV PCA 301 power
             meter with a JeeLabs JeeLink as RF modem. The matching JeeNode
             sketch can be found in .../contrib/36_PCA301-pcaSerial.zip
             (by ohweh&justme1968)
  - change:  PRESENCE: using ping command line utility to check presence
             on Windows based machines.
  - feature: install FHEM as Windows service by T.E., see docs/HOWTO_Windows.tx
  - feature: new module 33_readingsGroup to display a collection of readings
             from one or more devices. this will replace weblink readings.
             (by justme1968)
  - feature: setreading command added
  - feature: DbLog: by using DbLog a new Attribute DbLogExclude will be
             propagated to all Devices. DbLogExclue will work as regexp to
             exclude defined readings to log
  - change:  loglevel attribute deprecated/replaced by the verbose attribute
  - change:  VIERA: changed several readings/commands according to
             DevelopmentGuidelinesAV. See FHEM Wiki and commandref for more
             details.
  - change:  YAMAHA_AVR: changed several readings/commands and introduced new
             volume handling. please see the commandref for more details
  - change:  weblink fileplot/dbplot converted to SVG device (+FHEMWEB cleanup)
  - change:  VIERA: Added support for get dropdown
  - change:  EnOcean: Manufacturer Specific Applications (EEP A5-3F-7F),
             Shutter: readings position and anglePos are updated automatically,
             if command position is sent and the reading state was changed
             manually to open or closed
  - bugfix:  EnOcean: profile MD15 now sends current temperature values
  - feature: EnOcean: subtype roomSensorControl.05 (Room Sensor and Control
             Unit): actor commands added
  - feature: EnOcean: new sensor device Heating/Cooling Relay
  - feature: EnOcean: new attr sensorMode, temperatureRefDev, humidityRefDev
  - feature: EnOcean: EEP: MSC basic functions implemented (no teach-in)
  - feature: EnOcean: 4BS teach-in with EEP number and Manufacturer ID
  - bugfix:  EnOcean: subtypes tempSensor.??: calculations corrected
  - feature: new module 55_GDS.pm added (betateilchen)
  - feature: HUEDevice: special svg icon for unreachable (hard switched off)
             devices
  - feature: FHEMWEB detail screen with get dropdown
  - feature: displayattr command added
  - feature: SYSSTAT: allow (remote) monitoring system uptime
  - feature: new module 98_openweathermap.pm added (betateilchen)
  - feature: WeatherAsHtmlH(), WeatherAsHtmlD() added to 59_Weather.pm (Boris)
  - feature: new module I2C_BMP180 for reading I2C digital pressure sensor
             BMP180 or BMP085 connected to Raspberry Pi (Dirk)
  - feature: new module 35_SWAP_0000002200000003 for panstamp rgb led driver
             board with ir and dmx support
  - feature: 95_remotecontrol does not require a weblink anymore (UliM)
  - feature: optional sleep parameter quiet
  - feature: additional buttons for use with 95_remotecontrol
  - feature: new module 71_LISTENLIVE.pm for use with media players
             (betateilchen)
  - feature: use xhr for colorupdates by colorpicker and rgb presets
  - feature: new module 34_SWAP for generic SWAP protocoll support using
             a panStick and 34_panStamp as IODevice (by justme1968)
  - feature: new module 34_panStamp to use a panStick as a RF modem
             for panStamps using the SWAP protocoll (by justme1968)
  - feature: EGPM2LAN module added for Gembird (R) Energenie LAN Support
  - feature: FHEMWEB use widget module to update colorpicker in longpoll
  - feature: FHEMWEB widget (slider/etc) javascript handler modularized
  - feature: FHEMWEB longpoll in multiple browserwindows
  - feature: fhem.pl: version command added
  - feature: LightScene: add html overview of all configured scenes in
             detail view. allow usage of overview in a weblink.
  - feature: FLOORPLAN: enhanced detail-screen for floorplans in fhemweb,
             arrange-mode has delete-button, new command "get <floorplan-name>
             config"
  - feature: readings type added to weblink (justme1968)
  - feature: offset and monotonic added to userReadings modifier (justme1968)
  - feature: HUEDevice: support SVG icons for LWB001 living whites bulb
  - feature: HUEDevice: support more than one bridge
  - feature: updateInBackground global attribute
  - feature: SYSSTAT: allow stateFormat
  - feature: Module 70_VIERA supports now module 95_remotecontrol with own
             layout for VIERA TV
  - feature: InternalVal function added (like ReadingsVal)
  - feature: new module speedtest to monitor internet connection speed with
             speedtest-cli
  - feature: new module "remotecontrol" to display a graphical remotecontrol
             for any device
  - feature: HUEDevice: new attribute color-icons to colored svg icons
  - feature: FHEMWEB: longpoll is default now, longpollSVG (default off) added
  - feature: HUEDevice: allow usage of openautomation svg icons
  - feature: FHEMWEB: svg icons / iconPath / www/images/openautomation added
  - feature: FHEMWEB: SVGcache attribute & clearSvgCache set command added
  - feature: SYSSTAT: allow (remote) monitoring raspberry pi on cpu frequency
  - feature: MANTAINER.txt added
  - feature: PRESENCE: new mode "shellscript" to use own
             scripts or binaries for presence recognition
  - feature: YAMAHA_AVR: new set command to select scenes
  - feature: PRESENCE: new attribute ping_count
  - feature: userReadings may have a filter
  - feature: HUEBridge: allow starting of bridge firmware update
  - change:  EnOcean: profile PM101 changed, old profiles FAH, FBH, FTF, SR04
             removed
  - feature: TCM: new attr blockSenderID:
             Block receiving telegrams with a TCM SenderID sent by repeaters
  - feature: TCM: For TCM120 Transceiver now the transmission of RPS and 4BS
             commands supported
  - feature: EnOcean: Now all RPS / 1BS profiles, more than 90 4BS profiles and
             some manufacturer specific profiles are supported
  - feature: EnOcean: profiles (subType) are updated from EEP 2.1 to EEP 2.5
  - feature: FHEMWEB attribute roomIcons added
  - feature: SYSSTAT: optionaly calculate geometric average of last 4
             temperature values
  - feature: weblink details screen can be used to edit .gplot files
  - feature: eventTypes module added, to help with FileLog details screen
  - feature: FB_CALLMONITOR: new reverse search provider dasschnelle.at for
             reverse search of austrian telephone numbers
  - bugfix:  event-on-change-reading in combination with event-change-interval
  - change:  HUEDevice: allow color preset buttons in webCmd
  - feature: SYSSTAT: allow (remote) monitoring raspberry pi on chip temperatur
  - feature: HUEDevice: use webCmdFn for colorpicker
             added jscolor for colorpicker
  - feature: FHEMWEB: module specific summaryFn/detailFn + defineable webCmdFn
  - change:  ESA2000: adapted device detection , rename readings
  - change:  stucture triggers on each change, see event-on-change-reading
  - feature: PRESENCE: new mode "function" to use own perl functions for
             presence checks
  - bugfix:  fixing not-working FHEM restart, when a PRESENCE check is running
  - bugfix:  fixing memory overflow when "list" a PRESENCE definition
  - bugfix:  fixing dead PRESENCE definitions in case of timeouts
  - bugfix:  update: error while updating single files fixed. (M. Fischer)

- 2013-04-08 (5.4)
  - feature: updatefhem will be silently converted to update
  - feature: FHEMWEB: save button replaced with the menu entry "Save config"
  - feature: notify supports $NAME/$EVENT/$EVTPART0/etc. @/% is deprecated.
  - feature: 93_DbLog extended to give more functions for the charting frontend
             This includes new queries for raw table data and also statistics,
             which get sum/max/min/avg values from the database.
             Documentation has been updated.
  - feature: new module 31_LightScene to save and restore the state of a
             group of lights and other actors
  - feature: VIERA module added (by teevau)
  - change:  FHEMWEB: the first webCmd argument is no longer used by the
             state-icon, this can be implemented by the new devStateIcon
  - change:  30_HUEDevice: allow autodetection of bridge with hue portal
             services
  - feature: THRESHOLD Module by Damian
  - change:  30_HUEDevice: use new devStateIcon feature to show device color
             in room overview
  - feature: added example Setup SQL and configuration for SQLite
  - change:  modified MySQL Setup SQL to use 512 characters in EVENT column
  - feature: added new Javascript Frontend based on ExtJS (by Johannes)
  - feature: new modules 30_HUEBridge and 31_HUEDevice for phillips hue and
             smartlink devices (by justme1968)
  - change:  SYSSTAT: allow remote monitoring by ssh
  - change:  SYSSTAT: allow less frequent updates for diskusage
  - feature: new module 32_SYSSTAT to monitor system load and disk usage
             on linux FHEM hosts (by justme1968)
  - feature: new Module 73_PRESENCE to make automatic presence detection of
             mobile phones or other mobile devices (like tablets) via ping or
             bluetooth checks (by M. Bloch)
  - feature: new Module 98_Heating_Control to switch heatsinks automaticly
             with a weekly profile (by D. Ortmann / T. Faust)
  - feature: new Module 93_DbLog.pm for logging events into Databases.
             Generating Plots with weblinks are supportet.
             (by B. Neubert / T. Faust)
  - feature: new Module 59_HCS.pm for monitoring heating valves (FHT, HM-CC-VD)
             to contral a central heating unit. I thank Benjamin for his
             support! (M.  Fischer)
  - feature: new Module 72_FB_CALLMONITOR for receiving telephone call events
             (Markus)
  - feature: new Module 71_YAMAHA_AVR.pm for controlling Yamaha AV receivers
             over network (by Markus)
  - feature: optional second parameter to fhem() to make it silent
  - feature: autoloading commands, XmlList/etc renamed from 99 to 98.
  - feature: FHEMWEB returns external files in chunks to save memory
  - feature: commandref.html splitted: documentation is now appended to the
             modules.
  - change:  introduced readingsBulkUpdate, readingsSingleUpdate
  - change:  added GPLv2 licensing information
  - feature: FLOORPLAN added fp_setbutton attribute
  - bugfix:  FHEMWEB slider with min > 0
  - change:  FHEMWEB CORS moved to options
  - change:  FHEMWEB closing old TCP connections
  - change:  FHEMWEB added "Associated with" to detail-screen (Uli)
  - change:  FHEMWEB added ETag headers (Matthias)
  - change:  FHEMWEB devStateIcon added
  - change:  HOWTO auf deutsch (ilmtuelp0815)
  - change:  98_update.pm due a (probable) bug in perl, modules are no longer
             loading automatically. A restart is required now! (M. Fischer)
  - feature: 98_update.pm saves the statefile before an update (M. Fischer)
  - feature: FHEMWEB longpoll reconnect (Matthias)
  - bugfix:  rename may overwrite other devices
  - feature: FLOORPLAN longpoll (Matthias)
  - feature: support for recurring events added in 57_Calendar.pm (Boris)
  - feature: added support for OWL CM119,CM160 and CM180, energy sensors in
             TRX_WEATHER using RFXtrx433 (Willi Herzig)
  - feature: added support for KD101 smoke sensor (also set alert and pair) in
             TRX_SECURITY using RFXtrx433 (Willi Herzig)
  - change:  changed dewpoint to work with event-on-change-reading and
             technoline TX3TH (Willi Herzig)
  - feature: new command fheminfo. Shows system informations. (M. Fischer)
  - feature: added support for UV sensors in TRX_LIGHT using RFXtrx433 (Willi
             Herzig)
  - feature: added on-till and on-timer for set in TRX_LIGHT using RFXtrx433
             (Willi Herzig)
  - feature: generate devices with hexcodes as state for unknown types in
             TRX_ELSE using RFXtrx433 (Willi Herzig)
  - feature: new modules 10_OWServer.pm and 11_OWDevice.pm to interface with
             OWFS
  - feature: stateFormat (readingsFn modules) and showInternalValues attributes
  - feature: new readingsFn modules: FS20 CUL_WS HMS CUL_EM CUL_TX EnOcean ZWav
  - change:  BS, USF1000, ECMDDevice, Weather, dummy migrated to readingsFN
             (Boris)
  - feature: telnet client mode
  - bugfix:  FHEMWEB longpoll misses initial state change (HM: set_on vs. on)
  - change:  20_OWFS.pm, 21_OWTEMP modules flagged as "deprecated". These
             modules will be removed in a future release. Use OWServer /
             OWDevice instead. (M. Fischer)
  - feature: a lot of new features and known 1-wire slaves to OWServer /
             OWDevice added (M. Fischer)
  - feature: set-extensions (additional set commands) for FS20, EnOcean, ZWave
  - feature: added new command 'notice'. (M. Fischer)
  - change:  update supports the display and confirmation of system messages
             via the new notice command (M. Fischer)
  - feature: added new set commands and basicauth to 49_IPCAM.pm (M. Fischer)
  - feature: userReadings
  - feature: average supports more than one value in combined readings (T:x H:y
  - feature: FHEMWEB serves arbitrary files from the www directory
  - feature: FB_checkPw now works with a distinct fritzbox user
  - bugfix:  floorplan-correction for readings with longpoll. Requires local
             change in css!
  - feature: floorplan added js-extension from Dirk
  - feature: hour resolution in SVG
  - feature: ZWave support for MULTI_CHANNEL class
  - feature: FHEMWEB: old-dir-support removed, image-indexing rebuilt,
              smallscreen/touchpad moved to stylesheetPrefix, menuEntries
              added, Extend devStateIcon, js setting of attr values in detail
              screen, live slider update in detail and room view
  - feature: added support for third-party packages to 98_update.pm (M. Fischer
  - feature: FBAHA/FBDECT for FRITZ!DECT devices
  - feature: event-min-interval Attribute

- 2012-10-28 (5.3)
  - feature: added functions trim, ltrim, rtrim, UntoggleDirect,
    UntoggleIndirect
  - feature: added functions FB_mail, FB_WLANswitch
  - rework:  CUL_HM reworks with respect to protocol.  additions for several
    devices and commands
  - feature: rfmode supports to listen to MAX if fw>1.46, 00_CUL.pm (Jens)
  - feature: Status and length on cmdStack in webinterface for 10_CUL_HM
  - feature: devicepair in 10_CUL_HM.pm supports unset
  - feature: devicepair for single Button in 10_CUL_HM.pm (by MartinP)
  - feature: new Modules 75_MSG.pm, 76_MSGFile.pm and 76_MSGMail.pm (by
    Ruediger)
  - feature: new Module 59_Twilight.pm to calculate current daylight
  - feature: internal NotifyOrderPrefix: 98_average.pm is more straightforward
  - feature: the usb command tries to flash unflashed CULs on linux
  - feature: FHEMWEB: jsonp support, .holiday and .cfg added to Edit Files
  - feature: SVG: filled area support, some ls/lw fixes
  - feature: WOL (wake on lan) module added (by Matthias)
  - feature: additional groups from /etc/groups are applied (Christopher)
  - feature: updatefhem backup is using tar+gzip now
  - feature: EIB: introduce Get, interpret received values upon defined model
    (by datapoint types) (Maz)
  - feature: NetIO230B module by Andy
  - feature: Retaining configfile comments (not within a define statement)
  - feature: EnOcean PM101 by Ignaz
  - feature: FHEMWEB redirectCmds attribute added
  - feature: CUL_TX minsecs attribute (by Arno)
  - feature: webCmd in smallScreen added
  - feature: TRX modules by Willi
  - feature: FHEMWEB icons (by Joerg)
  - feature: FHEMWEB console (same as inform timer)
  - feature: remove dependency on Google::Weather, major rewrite (Boris)
  - feature: started experimental interface implementation (fhem API v2)
    (Boris)
  - feature: sleep issued in at/notify/etc is not blocking fhem anymore
  - feature: dummy got a setList attribute
  - feature: new module 02_RSS.pm
  - feature: at attribute alignTime added
  - feature: FHEMWEB attribute values via dropdown, slider for dimmer
  - feature: new attribute group for FHEMWEB (Boris)
  - change:  11_FHT.pm, 50_WS300.pm, 59_Weather.pm migrated to readingsUpdate
    mechanism (Boris)
  - change:  59_Weather.pm migrated from Google to Yahoo Weather API (Boris)
  - change:  updatefhem modifications to support a clean install of fhem and
    pgm2 installation, see commandref.html (M. Fischer)
  - change:  FHEMWEB support for the new www/pgm2 directroy added (M. Fischer)
  - change:  Makefile support for for the new www/pgm2 directroy and new
    targets backup and uninstall added. More verbose output. (M. Fischer)
  - change:  backup separated from updatefhem to a new command (M. Fischer)
  - feature: new command backup added (M. Fischer) new global attribute
    <backupsymlink> added new global attribute <backupcmd> added new global
    attribute <backup_before_update> added
  - feature: new module 57_Calendar.pm (Boris)
  - feature: new parameter <changed> for updatefhem added (M. Fischer) new
    global attribute <exclude_from_update> added (M. Fischer)
  - feature: optional telnet password added / telnet port is optional
  - feature: holiday returns all matches, not only the first.
  - change:  CULflash separated from updatefhem to a new module (M. Fischer)
  - feature: time and internet helper routines added to fhem.pl (Boris)
  - change:  separating common functions used by the FHEM modules into
    *Utils.pm files from fhem.pl
  - feature: portpassword and basicAuth may use evaluated functions
  - feature: motd with SecurityCheck added
  - feature: telnet module added, attr global port moved. allowfrom changed.
  - feature: FhemUtils/release.pm for the new update process added. (M.
    Fischer)
  - bugfix:  correct one-time relative at commands after reboot
  - feature: ZWave added
  - feature: module IPCAM added. (M. Fischer)
  - feature: module HTTPSRV added (Boris)
  - feature: module FLOORPLAN added (Uli Maass)
  - bugfix:  FHEMWEB: weblink with group attribute is shown together with other
    elements
  - feature: FHEMWEB: timepicker added
  - feature: FHEMWEB: support for modul specific icons added (M. Fischer)


- 2011-12-31 (5.2)
  - bugfix:  applying smallscreen attributes to firefox/opera
  - feature: CUL_TX added (thanks to Peterp)
  - feature: TCM120/TCM310 + EnOcean parser added
  - feature: eventMap enhanced
  - bugfix:  enabled logging for 59_Weather.pm (Boris)
  - feature: language selection for 59_Weather.pm (Erwin)
  - feature: .gplot files renamed from type to content
  - bugfix:  FS20 on-for-timer error reporting only in the logfile
  - bugfix:  FHEM2FHEM should work with CUL again, after syntax change
  - feature: CUL directio mode (No Device::SerialPort needed)
  - feature: FritzBox 7270 ZIP file
  - bugfix:  prevent fhem from stalling if telnet times out in 66_ECMD.pm
  - feature: added postproc ability to classdef in 66_ECMD.pm (Boris, Heinz)
  - feature: FHEMWEB longpoll mode, small fixes, tuned smallscreen mode
  - feature: average module added
  - change:  moved the berliOS CVS repository to a sourceforge SVN repository
  - feature: all FHEM modules have now a subversion id.
  - bugfix:  new perl compiled for the FritzBox 7270
  - feature: regexp1WontReactivate Attribute added
  - bugfix:  XmlList special handling
  - bugfix:  CUL_WS rain sensor corr1 fix
  - feature: FHEMWEB stylesheet attribute repaced with stylesheetPrefix
  - feature: notify attribute forwardReturnValue
  - change:  move JsonList from contrib to main-modules
  - change:  JsonList output optimized and more structured
  - feature: FHEMWEB save button, smallscreen first screen fix
  - feature: FHEMWEB encoding is now UTF-8, alias attribute is respected
  - change:  HTTPS certs directory moved from cwd into modpath
  - feature: shutdown parameter restart added
  - feature: usb scan/create command added (part of autocreate).
  - feature: SaveAs added to FHEMWEB Edit-Files
  - feature: EnOcean ElTako dimmer by Marc.
  - feature: fhem is started as user fhem on the FB7390


- 2011-07-08 (5.1)
  - feature: smallscreen optimizations for iPhone
  - feature: FHT8V rewrite (and moved from contrib into the FHEM directory).
  - feature: PID rewrite (and moved from contrib into the FHEM directory).
  - feature: FHEM2FHEM module
  - bugfix:  CUL get should not digest foreign events (fhtsoftbuffer)
  - bugfix:  S300TH sanity check won't allow negative temperatures.
  - feature: decode CUL uptime
  - feature: USB doc changes, FHZ initFS20_02/stopHMS parameters by Andreas.
  - feature: CUL_HM for some HomeMatic devices.
  - bugfix:  HTML-Syntax check of the pgm2 output and documents (*.html)
  - feature: added date alias for FHT80b (Boris)
  - feature: attr may be a regexp (for CUL_IR)
  - feature: Homepage moved from koeniglich.de/fhem to fhem.de
  - feature: eventMap attribute
  - feature: 64_ESA2000 added (by STefan/Gerd)
  - feature: new modules 66_ECMD.pm and 67_ECMDDevice.pm for ethersex-enabled
             devices and alike.
  - bugfix:  serial port setting on Linux broken if running in the background
  - feature: IPV6 support, FHEMWEB basicAuth and HTTPS support
  - feature: createlog added to the autocreate module
  - feature: contrib/tcptee.pl added
  - feature: HMLAN support
  - feature: Fritzbox7390 image
  - feature: pgm2 tablet support, included into the default configuration
  - feature: TUL/EIB Support (by Maz)
  - feature: updatefhem/CULflash
  - feature: $value{} => Value(), $oldvalue => OldValue()/OldTimestamp()


- 2010-08-15 (5.0)
  - **NOTE*: The default installation path is changed to satisfy lintian
  - feature: KM271
  - bugfix:  99_SUNRISE_EL endless loop bug
  - feature: CUL: optional baudrate spec in definition
  - feature: CUL: sendpool attribute
  - feature: CUL_HOERMANN module added
  - bugfix:  DST change: absolute at and relative sunrise fix
  - feature: FHEMWEB javascript additions for SVG plots (click on lines/labels)
  - feature: FHEMWEB smallscreen attribute (for smartphones)
  - bugfix:  the internal fhem() used in perl oneliners does not return a value
  - feature: Dimmer function of X10 module changed to match FS20
  - feature: allow only meaningful readings (fill level > -5%) in USF1000
  - feature: device attr links in commandref.html
  - bugfix:  make BS known to CUL to avoid lost messagesif both FHZ1300 and CUL
             are connected, adjust matching rule
  - feature: Copy&Paste in SVG
  - feature: Debian/Ubuntu Package. Install-path changes to satisfy lintian
  - feature: Allnet 3076/4027/4000T
  - feature: RFXCOMM Module for Oregon Weatherstations
  - feature: Davis VantagePro2
  - feature: ELV USB-WDE1
  - feature: addvaltriggers CUL attribute for adding RSSI as a trigger
  - feature: CUL_WS sanity check for large temp differences.

- 2010-03-13 (4.9)
  - bugfix:  changed the fhem prompt from FHZ> to fhem>
  - bugfix:  CUL_RFR fixes (chaining RFR's should work)
  - bugfix:  Path in the examples fixed (got corrupted)
  - bugfix:  PachLog fixes from Axel
  - bugfix:  HOWTO/Examples revisited for correctness
  - bugfix:  INITIALIZED, DEFINED, RENAMED, DELETED triggers
  - feature: image weblinks from Stefan
  - feature: OWFS support for passive Devices e.g. DS9097 (see commandref.html)
  - bugfix:  OWFS crash fhem with PGM2/3, xmllist (M.Fischer)
  - bugfix:  OWTEMP Defining a device without OWFS now fails (M.Fischer)
  - bugfix:  21_OWTEMP.pm missing trigger fo notify/filelog (M.Fischer)
  - feature: 99_getstate.pm get state from S555TH now (M.Fischer)
  - feature: pgm3: automatic support for CUL_WS (S300TH) added (MartinH)
  - bugfix:  21_OWTEMP.pm missing space within state logging (M.Fischer)
  - bugfix:  21_OWTEMP.pm interval fixed (M.Fischer)
  - bugfix:  21_OWTEMP.pm rewrite with errorcontrol and demo mode (M.Fischer)
  - feature: ignore attribute
  - bugfix:  [pgm3] table-format on Android-Browser optimized
  - feature: [pgm3] Skinable - change the colors.
  - feature: [pgm3] Rooms possible for Webcam and Google-Weather
  - bugfix:  dummy/structure was listed twice in list and xmllist
  - feature: 11_FHT.pm added new readings for warnings on battery, lowtemp,
             window and windowsensor (M.Fischer)
  - feature: autocreate.pm (create undefined RF devices, logs and plots)
  - feature: on-for-timer added for X10 modules (Boris)
  - bugfix:  pgm3: Better check of availability of google-weather (MartinH)
  - feature: pgm3: DBLog added for everything except UserDefs (Gerhard Pfeffer
             / MartinH)
  - feature: pgm2 style changes, SVG in background, optional compression

- 2009-11-28 (4.8)
  - bugfix:  loosing data when sending FS20 messages in a group
  - bugfix:  better handling of disconnected CUN
  - feature: softfhtbuffer added to CUL
  - bugfix:  pgm3: Pulldown-Menu FHTDEV with error-check (MartinH)
  - feature: duplicate buffer added for multi-cul/-fhz setups
  - feature: 20_OWFS.pm for 1-Wire via OWFS added (Martin Fischer)
  - feature: 21_OWTEMP.pm for 1-Wire Digital Thermometer added (Martin Fischer)
  - feature: CUL_FHTTK from Kai
  - feature: pgm3: Google-Weather, Battery-Check, Log-View added (MartinH)
  - feature: CUL_RFR (RF_ROUTING) added
  - feature: Command save retains now the order of the old config file
  - feature: List parameter added (list .* RFR_MSGCNT)

- 2009-10-23 (4.7)
  - bugfix:  Reattached corrupted CUL device caused uninitialized message
  - bugfix:  CUL/HMS changes, HMS cleanup
  - bugfix:  EM/EMWZ/EMGZ set changed to work in FHEMWEB
  - bugfix:  Avoid unitialized in xmllist for corrupt readings, reporter Boris
  - bugfix:  Add binmode to 01_fhemweb.pm for windows
  - bugfix:  Uniform check for windows, enable CUL for windows.
  - bugfix:  CUL/HMS parsing patches from Peter
  - bugfix:  Fixes for Windows by Klaus
  - bugfix:  Another "rereadcfg" bugfix
  - feature: Update to the current (1.27) CUL FHT interface
  - feature: suppress inplausible readings from USF1000
  - feature: get time, fwrev, set reopen for CM11 (Boris 2009-09-12)
  - bugfix:  FHZ_ReadAnswer bugfix for Windows (Klaus, 20.8.2009)
  - feature: CUL: device access code reorganized, TCP/IP support added (CUN)
  - feature: Pachube module from Axel
  - feature: dumpdef module from Axel in contrib
  - feature: javascripting support in FHEMWEB (Klaus/Axel)
  - feature: Module 09_BS.pm for brightness sensor added (Boris 2009-09-20)

- 2009-07-03 (4.6)
  - bugfix:  fht actuator message clarification by Klaus
  - feature: getstate command from Martin (25.12)
  - bugfix:  at drifts for relative timespecs
  - bugfix:  Add IODev to CUL/EM/CUL_WS/HMS/KS300
  - bugfix:  FileLog get (pgm2 plots) wont find the first row in the file
  - feature: 00_CUL: Answer CUR requests (status/time/fht)
  - bugfix:  support for second correction factor for EMWZ in 15_CUL_EM added
  - feature: CUL further sets/gets added
  - feature: Removed msghist for multiple FHZ handling, IODev attribute added
  - bugfix:  cut off string "(counter)" from fallback value in 13_KS300.pm
  - feature: daily/monthly cumulated values for EMWZ/EMGZ/EMWM with 15_CUL_EM
  - feature: 01_FHEMWEB.pm: multiple room assignments
  - feature: 01_FHEMWEB.pm: fixedrange with optional [day|week|month|year]
  - feature: 01_FHEMWEB.pm: attr title and label for flexible .gplot files
  - feature: fhem.pl: attr global logdir used by wildcard %ld
  - feature: do not block on disconnected devices (FHZ/CM11/CUL)
  - bugfix:  deleting at definition in the at command
  - bugfix:  deleting a notify/at/watchdog definition in a notify/at/watchdog
  - feature: devspec <attr>=<value>. E.g. set room=kitchen off; list disabled=
  - feature: Common Module calling for CUL/FHZ/CM11
  - feature: Store CUL sensitivity info
  - feature: avoid the "unknown/help me" message for unloaded devices
  - feature: structure module for large installations
  - feature: Cost Control in 15_CUL_EM (CostPerUnit, BasisFeePerMonth)
  - feature: add counter differential per time in 81_M232Counter.pm
  - feature: added USB compendium to documentation
  - feature: pgm3: Documentation for pgm3 updated, HMS100CO added (and bugfix)
  - bugfix:  Defining a repeated at job in a sunrise/sunset at job fails
  - bugfix:  FHT "summer" fix (avoiding a lot of syncnow)
  - feature: FHEMWEB modules added
  - feature: holiday module + doc + example + holiday2we attribute
  - bugfix:  sunrise stuff fixed, doc missing
  - feature: CUL FHT sending added
  - bugfix:  workaround to make M232 counter wraparound
  - feature: sequence module added
  - feature: Google Weather API support for FHEM (Boris 2009-06-01)
  - feature: lazy attribute for FHT devices (Boris 2009-06-09)
  - feature: tmpcorr attribute for FHT devices
  - feature: CUL_EM generates an event for each of the READINGS
  - feature: USF1000S support for FHEM added (Boris 2009-06-20)
  - feature: CUL supports HMS (culfw >= 1.22 needed)
  - feature: CUL shutdown procedure added
  - feature: 14_CUL_WS: better error checking
  - bugfix:  webpgm2 multi line editing is working again

- 2008-12-23 (4.5)
  - bugfix:  further 01_FHEMWEB cleanup
  - feature: CUL support for FS20(r/w), FHT(readonly), KS300 and EM
  - feature: command list outputs the device attributes too
  - bugfix:  rename bugs fixed
  - bugfix:  better integration of ReadyFn (Windows), slight overall speedup
  - bugfix:  Ignore/correct casing when autoloading modules
  - bugfix:  at is executed twice after a modify (rufus99, 2008-09-10)
  - feature: FHT internal modifications (better protocol understanding)
  - feature: add timestamp to inform
  - feature: The strange stty settings in 00_FHEM.pm are optional
  - bugfix:  webpgm2 iPhone fix
  - feature: fullinit and reopen commands for FHZ added (Boris 2008-11-01)
  - bugfix:  undefined NotifyFn in fhem.pl (Boris 2008-11-01)
  - feature: new modules 00_CM11.pm and 20_X10.pm for integration of X10
             devices in fhem (Boris 2008-11-02)
  - feature: X10 support for pgm3 (Boris 2008-11-02)
  - bugfix:  FHT short message warning
  - bugfix:  rereadconfig crashes with active webpgm2 connections (2008-11-13)
  - bugfix:  watchdog crash (2008-11-15)
  - bugfix:  Strange call for nonexistent MyCUL: ReadFn
  - feature: webpgm2: gplot output goes to /tmp/gnuplot.err
  - feature: devspec TYPE,DEF,STATE. e.g. list TYPE:FS20, set DEF:123 on
  - bugfix:  at schedules 2 events after the DST change (fix not verified)
  - feature: commandref.html reorg. There are now device sections.
  - feature: CUL / CUL_EM / CUL_WS documentation
  - feature: do not block fhem when the CUR is disconnected
  - bugfix:  correct correction factors for EMEM in 15_CUL_EM.pm
  - bugfix:  more stable CUL initialization
  - feature: reworked 15_CUL_EM.pm to account for timer wraparounds, more
             readings added
  - feature: speed gain through disabled refreshvalues query to all FHTs at
             definition; if you want it back at a "set myFHT report1 255
             report2 255" command to the config file.
  - feature: fhem commands may be added in modules. XmlList is external now.
  - bugfix:  rereadcfg from webpgm2 does not crash fhem.pl
  - feature: jsonlist command from Martin (contrib/JsonList)
  - feature: contrib/rotateShiftWork from Martin
  - feature: contrib/fhem2speech from Martin
  - bugfix:  attributes of at devices disappear
  - feature: attribute rainadjustment for KS300 (Boris 2008-12-17)
  - bugfix:  deleting at / watchdog while active creates an empty device
  - feature: ExactId trigger added for wildcard HMS devices

- 2008-08-04 (4.4)
  - feature: RM100-2 battery empty warning (mare 23.07.08)
  - feature: optimising the pgm2/SVG memory usage
  - feature: autoloading FHEM modules
  - bugfix:  STATE/$value is carrying again the correct value
  - feature: enhancing the Makefile and the documentation
  - feature: 90_at is using now InternalTimer, subsecond precision added
  - feature: HMS100-FIT added (01.01.08 by Peter and 22.01.08 by Juergen)
  - feature: 91_watchdog added to handle the HMS100-FIT
  - feature: cum_kWh/cum_m3 added to EMWZ/EMGZ (11.01.08 by Peter)

- 2008-07-12 (4.3)
  - bugfix:  KS300 state was wrong after the STATE bugfix
  - feature: HMS100CO (by Peter)
  - feature: EMGZ (by Peter)
  - feature: Generate warning if too many commands were sent in the last hour
  - doc:     linux.html: Introduction (Peter S.)
  - feature: contrib/82_M232Voltage.pm (by Boris, 24.12)
  - feature: delattr renamed to deleteattr (Rudi, 29.12)
  - feature: defattr renamed to setdefaultattr (Rudi, 29.12)
  - feature: device spec (list/range/regexp) for most commands implemented
  - feature: %NAME, %EVENT, %TYPE parameters in notify definition
  - feature: added 93_DbLog.pm, database logging facility (Boris, 30.12.)
  - feature: webfrontend/pgm2 converted to a FHEM module
  - bugfix:  99_SUNRISE_EL.pm: may schedule double events
  - bugfix:  62_EMEM.pl, contrib/em1010.pl: correct readings for energy_kWh
             and energy_kWh_w (Boris, 06.01.08)
  - feature: global attr allowfrom, as wished by Holger (8.1.2008)
  - feature: FHT: multiple commands, softbuffer changes, cmd rename, doc
  - feature: EM1010PC: automatic reset
  - feature: contrib/00_LIRC.pm (25.3, by Bernhard)
  - bugfix : 00_FHZ: additional stty settings for strange Linux versions
  - bugfix : pgm2 wrong temp summary for FHT's (reported by O.D., 16.4.2008)
  - feature: FHEM modules may live on a filesystem with "ignorant" casing (FAT)
  - feature: FileLog "set reopen" for manual tweaking of logfiles.
  - feature: multiline commands are supported through the command line
  - feature: pgm2 installation changes, multiple instances, external css
  - feature: 87_ws2000.pm (thomas 10.05.08)
  - contrib: ws2000_reader.pl Standalone decoder and server (thomas 10.05.08)
  - doc:     update fhem.html and commandline.html reflecting ws2000 and
             windows installation(thomas 10.05.08)
  - feature: add ReadyFn to fhem.pl in main loop to have an alternative for
             select, which is not working on windows (thomas 11.05)
  - feature: set timeout to 0.2s, if HandleTimeout returns undef=forever
  - bugfix : WS2000:fixed serial port access on windows by replacing FD with
             ReadyFn
  - bugfix : FileLog: dont use FH->sync on windows (not implemented there)
  - feature: EM, WS300, FHZ:Add Switch for Device::SerialPort and
             Win32::SerialPort to get it running in Windows (sorry, untested)
  - bugfix:  FileLog undefined $data in FileLog_Get
  - feature: fhem.pl check modules for compiletime errors and do not initialize
             them
  - feature: M232 add windows support (thomas 12.05.08)
  - feature: add simple ELV IPWE1 support (thomas 12.05.08)
  - feature: FileLog get to read logfiles. Used heavily by webpgm2
  - feature: webpgm2: gnuplot-scroll mode to navigate/zoom in logfiles
  - bugfix:  deleting FS20 device won't result in unknown device (Daniel, 11.7)
  - feature: webpgm2 generates SVG's from logs: no need for gnuplot
  - bugfix:  examples corrected to work with current syntax

- 2007-12-02 (4.2)
  - feature: added archivedir/archivecmd to the the main logfile
  - feature: 99_Sunrise_EL.pm (does not need any Date modules)
  - bugfix:  seldom xmllist error resulting in corrupt xml (Martin/Peter, 4.9)
  - bugfix:  FHT mode holiday_short added (9.9, Dirk)
  - bugfix:  Modifying a device from its own trigger crashes (Klaus, 10.9)
  - feature: webpgm2 output reformatted
  - feature: webpgm2 displaying multiple plots
  - feature: FHT lime-protection code discovered by Dirk (7.10)
  - feature: softwarebuffer for FHT devices (Dirk 17.10)
  - feature: FHT low temperatur warning and offset (Dirk 17.10)
  - change:  change FHT state into warnings (Dirk 17.10)
         NOTE: you'll get an undefined type state &
         undefined type unknown_85 after upgrade.
  - feature: Softwarebuffer code simplified (Rudi 22.11)
  - bugfix:  bug #12327 doppeltes my
  - bugfix:  set STATE from trigger
  - bugfix:  readings state vs STATE problem (xmllist/trigger)
  - change:  SUNRISE doc changed (99_SUNRISE.pm -> 99_SUNRISE_EL.pm)
  - feature: support for the M232 ELV device (Boris, 25.11)
  - feature: alternativ Quad-based numbers for the FS20 (Matthias, 24.11)
  - feature: dummy type added (contrib/99_dummy.pm)

- 2007-08-05 (4.1)
  - doc:     linux.html (private udev-rules, not 50-..., ATTRS)
  - bugfix:  setting devices with "-" in their name did not work
  - doc:     fhem.pl and commandref.html (notifyon -> notify, correction
             of examples)
  - feature: modify command added
  - feature: The "-" in the name is not allowed any more
  - bugfix:  disabled notify causes "uninitialized value" (STefan, 1.5)
  - bugfix:  deleted FS20 items are still logging (zombie) (Gerhard, 16.5)
  - bugfix:  added FS20S8, removed stty_parmrk (Martin, 24.5)
  - feature: added archivedir/archivecmd to the FileLog
  - feature: added EM1010PC/EM1000WZ/EM1000EM support
  - bugfix:  undefined messages for unknown HMS devs (Peter, 8.6)
  - bugfix:  em1010 and %oldvalue bugs (Peter, 9.6)
  - bugfix:  SCIVT solar controller (peterp, 1.7)
  - bugfix:  WS300 loglevel change (from 2 to 5 or device specific loglevel)
  - feature: First steps for a Fritz!Box port. See the fritzbox.html

- 2007-04-14 (4.0)
  - bugfix:  deny at +{3}... (only +*{3} allowed), reported by Bernd, 25.01
  - bugfix:  allow numbers greater then 9 in at +{<number>}
  - feature: new 50_WS300.pm from Martin (bugfix + rain statistics, 26.01)
  - feature: renamed fhz1000 to fhem
  - feature: added HISTORY and README.DEV
  - doc:     Added description of attribute "model".
  - bugfix:  delete the pidfile when terminating. (reported by Martin and Peter
  - feature: attribute showtime in web-pgm2 (show time instead of state)
  - feature: defattr (default attribute for following defines)
  - feature: added em1010.pl to the contrib directory
  - doc:     added linux.html (multiple devices, udev-links)
  - REORGANIZATION:
    - at/notify "renamed" to "define <name> at/notify"
    - logfile/modpath/pidfile/port/verbose "renamed" to "attr global xxx"
    - savefile renamed to "attr global statefile"
    - save command added, it writes the configfile and the statefile
    - delattr added
    - list/xmllist format changed
    - disable attribute for at/notify/filelog
    See HISTORY for details and reasoning
  - added rename command
  - webpgm2 adapted to the new syntax, added device specific attribute
    and "set" support, gnuplot files are configurable, links to the
    documentation added.
  - bugfix: more thorough serial line initialization

- 2007-01-25 (3.3)
  - bugfix:  50_WS300.pm fix from Martin
  - bugfix:  pidfile does not work as expected (reported by Martin)
  - bugfix:  %U in the log-filename is wrong (bugreport by Juergen)
  - feature: %V added to the log-filename
  - feature: KS300 wind calibration possibility added
  - feature: (software) filtering repeater messages (suggested by Martin)
  - feature: the "client" fhz1000.pl can address another host
  - bugfix:  empty FHT battery is not reported (by Holger)
  - feature: new FHT codes, e.g. month/day/hour/minute setting (by Holger)

- 2007-01-14 (3.2)
  - bugfix:  example $state changed to $value (remco)
  - bugfix:  sun*_rel does not work correctly with offset (Sebastian)
  - feature: new HMS100TF codes (Sebastian)
  - feature: logging unknown HMS with both unique and class ID (Sebastian)
  - feature: WS300: "Wetter-Willi-Status", rain_raw/rain_cum added, historic
             data (changes by Martin & Markus)
  - bugfix:  broken rereadcfg / CommandChain after init
             (reported by Sebastian and Peter)
  - bugfix:  sunrise_coord returned "3", which is irritating

- 2007-01-08 (3.1)
  - bugfix:  delete checks the arg first "exactly", then as a regexp
  - bugfix:  sun*_rel does not work correctly with offset (Martin)
  - feature: FAQ entry on how to install the sunrise stuff.
  - feature: the inner core is modified to be able to handle more than one "IO"
             device, i.e multiple FHZ at the same time, or FHZ + FS10 + WS300.
             Consequences:
    - "fhzdev <usbdevice>" replaced with "define <FHZNAME> FHZ <usbdevice>"
    - "sendraw <fn> <code>" replaced with "set <FHZNAME> raw <fn> <code>"
    - module function parameters changed (for module developers)
    - set FHZ activefor dev
    - select instead sleep after sending FHZ commands
    - the at timer is more exact (around 1msec instead of 1 sec)
    - ignoring FS20 device 0001/00/00
  - feature: contrib/serial.pm to debug serial devices.
  - feature: WS300 integrated: no external program needed (Martin)
  - feature: updated to pgm3-0.7.0, see the CHANGELOG at Martins site

- 2006-12-28 (3.0)
  - bugfix:  KS300: Make the temperature negative, not the humidity
  - bugfix:  generate correct xmllist even with fhzdev none (Martin, 12.12)
  - feature: one set command can handle multiple devices (range and enumeration
  - feature: new FS20 command on-till
  - feature: perl: the current state is stored in the %value hash
  - feature: perl: sunset renamed to sunset_rel, sunset_abs added (for on-till)
  - feature: perl: isday function added
  - feature: follow-on-for-timer attribute added to set the state to off
  - bugfix:  the ws300pc negative-temp bugfix included (from Martin Klerx)
  - feature: version 0.6.2 of the webpgm3 included (from Martin Haas)

- 2006-11-27 (2.9a)
  - bugfix:  FileLog+Unknown device generates undefined messages
  - bugfix:  trigger with unknown device generates undefined messages

- 2006-11-19 (2.9)
  - bugfix:  fhz1000.pl dies at startup if the savefile does not exist
  - bugfix:  oldvalue hash is not initialized at startup (peter, Nov 09)
  - feature: Notify reorganization (requested by juergen and matthias) :
    - inform will be notified on both real events and set or trigger commands
    - filelogs will additionally be notified on set or trigger commands
    - the extra_notify flag is gone: it is default now, there is a
      do_not_notify flag for the opposite behaviour.
  - feature: at timespec as a function. Example: at +*{sunset()}
    commandref.html and examples revisited.
  - feature: 99_SUNRISE.pm added to use with the new at functionality
    (replaces the old 99_SUNSET.pm)
  - feature: webpgm2 "everything" room, at/notify section, arbitrary command
  - bugfix:  resetting the KS300
  - feature: updated ws300pc (from martin klerx, Nov 08)
  - bugfix:  parsing timed commands implemented => thermo-off,thermo-on and
             activate replaced with timed off-for-timer,on-for-timer and
             on-old-for-timer (reported by martin klerx, Nov 08)
  - feature: pidfile (requested by peter, Nov 10)
  - bugfix:  function 81 is not allowed

- 2006-11-08 (2.8)
  - feature: store oldvalue for triggers. perl only. requested by peter.
  - feature: inform cmd. Patch by Martin. There are many Martins around here
  - bugfix:  XML: fix & and < and co
  - bugfix:  Accept KS300 negative temperature values
  - change:  the FS20 msg "rain-msg" is called now "activate"
  - feature: start/stop rc script from Stefan (in the contrib directory)
  - feature: attribute extra_notify: setting the device will trigger a notify
  - feature: optional repeat count for the at command
  - feature: skip_next attribute for the at command
  - feature: WS300 support by Martin. Check the contrib/ws300 directory.
  - bugfix:  91_DbLog.pm: retry if the connection is broken by Peter
  - feature: Martin's pgm3-0.5.2 (see the CHANGELOG on his webpage)
  - feature: RRD logging example by Peter (in the contrib/rrd directory)

- 2006-10-03 (2.7)
  - bugfix:  Another try on the > 25.5 problem. (Peters suggestion)
  - feature: 99_ALARM.pm from Martin (in the contrib directory)
  - feature: HMS100TFK von Peter P.
  - feature: attribute loglevel
  - feature: attribute dummy
  - feature: attr command documented
  - feature: the current version (0.5a) of the pgm3 from Martin.

- 2006-09-13 (2.6a)
  - bugfix:  the FHT > 25.5 problem again. A never ending story.

- 2006-09-08 (2.6)
  - bugfix:  updated the examples (hint from Juergen)
  - bugfix:  leading and trailing whitespaces in commands are ignored now
  - feature: making life easier for perl oneliners: see commandref.html
             (motivated by STefans suggestions)
  - feature: include command and multiline commands in the configfiles (\)
  - bugfix:  web/pgm2 KS300 rain plot knows about the avg data
  - bugfix:  the FHT > 25.5 problem. Needs to be tested.
  - feature: log unknown devices (peters idea, see notifyon description)
  - feature: HMS wildcard device id for all HMS devices. See the define/HMS
             section in the commandref.html for details.  NOTE: the wildcard
             for RM100-2 changed from 1001 to 1003.  (peters idea)
  - feature: rolwzo_no_off.sh contrib file (for those who were already closed
             out by automatically closing rollades, by Martin)
  - feature: the current version (0.4.5) of the pgm3 from Martin.

- 2006-08-13 (2.5)
  Special thanks to STefan Mayer for a lot of suggestions and bug reports
  - If a command is enclosed in {}, then it will be evaluated as a perl
    expression, if it is enclosed in "" then it is a shell command, else it is
    a "normal" fhz1000 command.
    "at" and "notifyon" follow this convention too.
    Note: a shell command will always be issued in the background.
  - won't die anymore if the at spec contains an unknown command
  - rereadcfg added. Sending a HUP should work better now
  - escaping % and @ in the notify argument is now possible with %% or @@
  - new command trigger to test notify commands
  - where you could specify an fhz command, now you can specify a list of
    them, separated by ";". Escape is ;;
  - KS300 sometimes reports "negative" rain when it begins to rain.  Filter
    such values. israining is set when the raincounter changed or the ks300
    israining bit is set.
  - sleep command, with millisecond accuracy
  - HMS 100MG support by Peter Stark.
  - Making FHT and FS20 messages more uniform
  - contrib/fs20_holidays.sh by STefan Mayer
    (simulate presence while on holiday)
  - webfrontends/pgm4 by STefan Mayer: fs20.php
  - KS300 avg. monthly values fixed (hopefully)
  - deleted undocumented "exec" function (you can write it now as {...})

- 2006-07-23 (2.4)
  - contrib/four2hex (to convert between ELV and our codes) by Peter Stark
  - make dist added to set version (it won't work in a released version)
  - reload function to reload (private) perl modules
  - 20_FHT.pm fix: undef occures once without old data
  - "setstate comment" is replaced with the attr command (i.e. attribute).
    The corresponding xmllist COMMENT tag is replaced with the ATTR tag.
    Devices or logs can have attr definitions.
  - webfrontend/pgm2 (fhzweb.pl) updated to handle "room" attributes(showing
    only devices in this room).
  - version 0.4.2 of webfrontend/pgm3 integrated.
  - contrib/ks300avg.pl to compute daily and monthly avarage values.
  - the 40_KS300.pm module is computing daily and monthly avarages for the
    temp/hum and wind values and sum of the rain. The cum_day and cum_month
    state variables are used as helper values.  To log the avarage use the
    .*avg.* regexp. The regexp for the intraday log will trigger it also.
  - Added the contrib file garden.pl as a more complex example: garden
    irrigation. The program computes the time for irrigation from the avarage
    temperature reported by the ks300-2.
  - Enable uppercase hex codes (Bug reported by STefan Mayer)
  - Renamed the unknown_XX FHT80b codes to code_XXXXXX, this will produce
    "Undefined type" messages when reading the old save file
  - RM100-2 added (thanks for the codes from andikt).

- 2006-6-22 (2.3)
  - CRC checking (i.e. ignoring messages with bad CRC, message on verbose 4)
  - contrib/checkmesg.pl added to check message consistency (debugging)
  - FHT: unknown_aa, unknown_ba codes added. What they are for?
  - Empty modpath / no modpath error messages added (some user think modpath is
    superfluous)
  - Unparsed messages (verbose 5) now printed as hex
  - Try to reattach to the usb device if it disappears: no need to
    restart the server if the device is pulled out from the USB socket and
    plugged in again (old versions go into a busy loop here).
  - Supressing the seldom (ca 1 out of 700) short KS300 messages.
    (not sure how to interpret them)
  - Added KS300 "israining" status flag. Note: this not always triggers when it
    is raining, but there seems to be a correlation. To be evaluated in more
    detail.
  - notifyon can now execute "private" perl code as well (updated
    commandref.html, added the file example/99_PRIV.pm)
  - another "perl code" example is logging the data into the database
    (with DBI), see the file contrib/91_DbLog.pm. Tested with an Oracle DB.
  - logs added to the xmllist
  - FHT80b: Fix measured-temp over 25.5 (handling the tempadd messages better)

- 2006-05-20 (2.2)
  - FHZ1300 support verified (+ doc changes)
  - KS300 support added (with Temperature, Humidity, Wind speed, Rain).
    Not verified/undecoded: subzero temp, weak battery, Is-raining flag,
    wind speed > 100km/h
  - webpgm2 log fix for "offed" FHT devices (with no actuator data)
  - webpgm3 upgrade (by Martin Haas, see webpgm/pgm3/docs/CHANGES for details)
  - HMS logging/state format changed to make it similar to KS300
  - added HMS100WD (thanks to Sascha Pollok)
  - ntfy/logging changed to be able to notify for multiple attributes
    arriving in one message
  - central FHTcode settable (see commandref.html)
  - optionally listen for non-local requests (port <num> global)
  - unknown logging
  - FAQ

- 2006-04-15 (2.1)
  - webfrontend/pgm2 changes:
    - make it work on Asus dsl-routers (no "use warnings")
    - css/readonly configurable
    - Formatting for HMS data
  - comments can be added to each device (setstate <dev> comment:xxx)
  - testbed to dry-test functionality (test directory)
  - added an empty hull for the KS300 weather module
  - added undocumented "exec" function to call arbitrary program parts
    for debugging. Example: exec FhzDecode("81xx04xx0101a0011234030011");
  - webfrontend/pgm3, contributed by Martin Haas
  - fixed pgm1: changing values should work now

- 2006-04-02 (2.0)
  - XmlList and webfrontend/pgm1 programs from Raoul Matthiessen
  - list tries to display the state and not the last command
  - Both log facilities (FileLog and Log) take wildcards
    (week, year, month, etc) to make logfile rotating easier
  - webfrontend/pgm2

- 2006-02-12 (1.9b)
  - Bugfix: Fixing the same bug again (thanks to Martin)

- 2006-02-12 (1.9a)
  - Bugfix: wrong rights for HMS and wrong place for readonly
    (thanks to Juergen)

- 2006-02-10 (1.9)
  (aka as the Juergen release)
  - The FHZ1300 is reported to work
  - Bugfix: spaces before comment in the config file should be ignored
  - added FS20STR codes to 10_FS20.pm
  - names restricted to A-Za-z0-9.:- (especially _ is not allowed)
  - delete calles now an UndefFn in the module
  - implementation of FS20 function group/local master/global master
  - the list command tells you the definition of the device too

- 2006-01-05 (1.8)
  - Bugfix: detailed FS20 status was not set from external event
  - Bugfix: setstate for FS20 returned the last state set
  - Bugfix: undefined FS20 devices (can) crash the server
  - HMS module added by Martin Mueller
    (currently supporting the HMS100T & HMS100TF)
  - Log modules added, the first one being a simple FileLog
    (inspired by Martin Mueller)
  - A little  gnuplot script to display temperature and actuator changes

- 2006-01-04 (1.7)
  - the at command can be used to execute something repeatedly with *
  - ntfy can filter on device or on device+event with a regexp
  - checking the delete and notify regexps if they make sense
  - the FHT init string is now a set command (refreshvalues)
  - shutdown saves the detailed device information too

- 2006-01-03 (1.6)
  - signal handling (to save the state on shutdown)
  - module FHZ addded (for the FHZ1000PC device itself)
  - added the get function (to make the initialization prettier)
  - the module ST was renamed to FS20
  - FS20 timer commands added
  - modules command removed (we are loading everything from the modpath
    directory)
  - FHT80b module added (yes, it is already useful, you can set
    and view a lot of values)
  - documentation adapted
  - Added a TODO file

- 2005-12-26 (1.5)
  - "modularized" in preparation for the FHT80B -> each device has a type
  - added relative "at" commands (with +HH:MM:SS)
  - multiple commands on one line separated with ;
  - sleeping 0.22 seconds after an ST command
  - some commands/syntax changed:
    - switch => set
    - device => fhzdevice
    - define <name> ... => define <name> <type> ...
  - the state of the devices and the at commands are saved
  - at start always sending a "set 0001 00 01" to enable the FHZ receiever.
    This is a workaround.
  - doc rewrite, examples directory

- 2005-11-10 (1.4)
  - Reformatting the package and the documentation
  - New links

- 2005-10-27 (1.3)
  - Bugfix: multiple at commands at the same time.
