#!/bin/bash
# -*- bash -*-
# vim: ft=bash
#
# $Id$
#

: << =cut

=head1 NAME

fhem_fht80b_ - plugin to graph temperature and other values of ELV FHT80B devices
 (other devices may also work (untested))

=head1 APPLICABLE SYSTEMS

FHEM must be installed and configured and reacheable via telnet (network or localhost)

Additionally the module 99_getstate.pm has to be enabled. Copy it from the contrib 
directory to the FHEM directory and do a shutdown restart, ie:
cp /usr/share/fhem/contrib/getstate/99_getstate.pm /usr/share/fhem/FHEM/

You can test if your devices are able to be queried by submitting this line to FHEM (via telnet or web):
  getstate <device>
  i.e: getstate wz_thermostat
    output should be something like this: day-temp:20.0 desired-temp:17.0 measured-temp:21.2 windowopen-temp:12.0 temperature:21.2 

=head1 CONFIGURATION

fhem_fht80b_ has to be linked to the device name, ie. fhem_fht80b_wz_thermostat

The following environment variables are available

  host - hostname of the fhem server (default: localhost)
  port - telnet port (default: 7072)

This is a typical configuration:

 [fht_80b_*]
   env.host fritz.box
   env.port 7072

=head1 INTERPRETATION

Shows a graph with temperature

=head1 MAGIC MARKERS

 #%# family=auto
 #%# capabilities=autoconf

=head1 BUGS

None known.

=head1 AUTHOR

2012 Oliver Voelker <code@magenbrot.net>

=head1 LICENSE

This program is free software: you can redistribute it and/or modify
it under the terms of the GNU General Public License as published by
the Free Software Foundation, either version 3 of the License, or
(at your option) any later version.

This program is distributed in the hope that it will be useful,
but WITHOUT ANY WARRANTY; without even the implied warranty of
MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
GNU General Public License for more details.

You should have received a copy of the GNU General Public License
along with this program.  If not, see <http://www.gnu.org/licenses/>.

=cut

NC=`which nc 2>/dev/null`
DEVICE=`echo $0 | sed -e 's/.*fhem_fht80b_\(.*\)/\1/'`

HOST="localhost"
PORT="7072"

if [ "$host" ]; then HOST=$host; fi
if [ "$port" ]; then PORT=$port; fi

if [ "$1" = "autoconf" ]; then
  if [ -z "$NC" -o ! -x "$NC" ] ; then 
      echo "no (no nc executable)"
      exit 0
  fi
fi

if [ "$1" = "config" ]; then
  echo "graph_title FHEM sensor (${DEVICE})"
  echo "graph_vlabel temp"
  echo "graph_category fhem"
  echo "temp.label temperature"
  echo "temp.colour 00FF00"
  echo "actuator.label actuator"
  echo "actuator.colour fe2e64"
  echo "daytemp.label day temperature"
  echo "daytemp.colour fa5858"
  echo "desiredtemp.label desired temperature"
  echo "desiredtemp.colour df0101"
  echo "nighttemp.label night temperature"
  echo "nighttemp.colour 610b0b"
  echo "windowopentemp.label open window temperature"
  echo "windowopentemp.colour 3b0b0b"
  exit 0
fi

fhem=`echo -e "getstate ${DEVICE}\nquit" | ${NC} $HOST $PORT`
temp=`echo $fhem | awk '{split($0,a,"temperature:"); split(a[2],b," "); print b[1]}'`
actuator=`echo $fhem | awk '{split($0,a,"actuator:"); split(a[2],b," "); print b[1]}' | tr -d "%"`
daytemp=`echo $fhem | awk '{split($0,a,"day-temp:"); split(a[2],b," "); print b[1]}'`
desiredtemp=`echo $fhem | awk '{split($0,a,"desired-temp:"); split(a[2],b," "); print b[1]}'`
nighttemp=`echo $fhem | awk '{split($0,a,"night-temp:"); split(a[2],b," "); print b[1]}'`
windowopentemp=`echo $fhem | awk '{split($0,a,"windowopen-temp:"); split(a[2],b," "); print b[1]}'`

echo temp.value $temp
echo actuator.value $actuator
echo daytemp.value $daytemp
echo desiredtemp.value $desiredtemp
echo nighttemp.value $nighttemp
echo windowopentemp.value $windowopentemp
